--- a/arch/arm/boot/dts/armada-xp.dtsi
+++ b/arch/arm/boot/dts/armada-xp.dtsi
@@ -237,12 +237,10 @@
 };
 
 &i2c0 {
-	compatible = "marvell,mv78230-i2c", "marvell,mv64xxx-i2c";
 	reg = <0x11000 0x100>;
 };
 
 &i2c1 {
-	compatible = "marvell,mv78230-i2c", "marvell,mv64xxx-i2c";
 	reg = <0x11100 0x100>;
 };
 
