// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include "mt7621_edimax_rx21s.dtsi"

/ {
	compatible = "edimax,ra21s", "mediatek,mt7621-soc";
	model = "Edimax RA21S";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	leds {
		compatible = "gpio-leds";

		led_power: led_1 {
			label = "ra21s:red:led1";
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
		};

		led_2 {
			label = "ra21s:red:led2";
			gpios = <&gpio 12 GPIO_ACTIVE_HIGH>;
		};

		led_3 {
			label = "ra21s:red:led3";
			gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
		};

		led_4 {
			label = "ra21s:red:led4";
			gpios = <&gpio 15 GPIO_ACTIVE_HIGH>;
		};
	};
};
