// SPDX-License-Identifier: GPL-2.0
/*
 * Copyright (c) 2019 MediaTek Inc.
 *
 * Author: Ryder Lee <ryder.lee@mediatek.com>
 */

#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/clock/mt7629-clk.h>
#include <dt-bindings/power/mt7622-power.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/phy/phy.h>
#include <dt-bindings/reset/mt7629-resets.h>

/ {
	compatible = "mediatek,mt7629";
	interrupt-parent = <&sysirq>;
	#address-cells = <2>;
	#size-cells = <2>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		enable-method = "mediatek,mt6589-smp";

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x0>;
			clock-frequency = <1250000000>;
			cci-control-port = <&cci_control2>;
		};

		cpu1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x1>;
			clock-frequency = <1250000000>;
			cci-control-port = <&cci_control2>;
		};
	};

	pmu {
		compatible = "arm,cortex-a7-pmu";
		interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 9 IRQ_TYPE_LEVEL_LOW>;
		interrupt-affinity = <&cpu0>, <&cpu1>;
	};

	clk20m: oscillator-0 {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <20000000>;
		clock-output-names = "clk20m";
	};

	clk40m: oscillator-1 {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <40000000>;
		clock-output-names = "clkxtal";
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupt-parent = <&gic>;
		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
		clock-frequency = <20000000>;
		arm,cpu-registers-not-fw-configured;
	};

	soc {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		infracfg: syscon@10000000 {
			compatible = "mediatek,mt7629-infracfg", "syscon";
			reg = <0x10000000 0x1000>;
			#clock-cells = <1>;
		};

		pericfg: syscon@10002000 {
			compatible = "mediatek,mt7629-pericfg", "syscon";
			reg = <0x10002000 0x1000>;
			#clock-cells = <1>;
		};

		scpsys: scpsys@10006000 {
			compatible = "mediatek,mt7629-scpsys",
				     "mediatek,mt7622-scpsys";
			#power-domain-cells = <1>;
			reg = <0x10006000 0x1000>;
			clocks = <&topckgen CLK_TOP_HIF_SEL>;
			clock-names = "hif_sel";
			assigned-clocks = <&topckgen CLK_TOP_HIF_SEL>;
			assigned-clock-parents = <&topckgen CLK_TOP_UNIVPLL1_D2>;
			infracfg = <&infracfg>;
		};

		timer: timer@10009000 {
			compatible = "mediatek,mt7629-timer",
				     "mediatek,mt6765-timer";
			reg = <0x10009000 0x60>;
			interrupts = <GIC_SPI 169 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 170 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clk20m>;
			clock-names = "clk20m";
		};

		sysirq: interrupt-controller@10200a80 {
			compatible = "mediatek,mt7629-sysirq",
				     "mediatek,mt6577-sysirq";
			reg = <0x10200a80 0x20>;
			interrupt-controller;
			#interrupt-cells = <3>;
			interrupt-parent = <&gic>;
		};

		apmixedsys: syscon@10209000 {
			compatible = "mediatek,mt7629-apmixedsys", "syscon";
			reg = <0x10209000 0x1000>;
			#clock-cells = <1>;
		};

		rng: rng@1020f000 {
			compatible = "mediatek,mt7629-rng",
				     "mediatek,mt7623-rng";
			reg = <0x1020f000 0x100>;
			clocks = <&infracfg CLK_INFRA_TRNG_PD>;
			clock-names = "rng";
		};

		topckgen: syscon@10210000 {
			compatible = "mediatek,mt7629-topckgen", "syscon";
			reg = <0x10210000 0x1000>;
			#clock-cells = <1>;
		};

		watchdog: watchdog@10212000 {
			compatible = "mediatek,mt7629-wdt",
				     "mediatek,mt6589-wdt";
			reg = <0x10212000 0x100>;
		};

		pio: pinctrl@10217000 {
			compatible = "mediatek,mt7629-pinctrl";
			reg = <0x10217000 0x8000>,
			      <0x10005000 0x1000>;
			reg-names = "base", "eint";
			gpio-controller;
			gpio-ranges = <&pio 0 0 79>;
			#gpio-cells = <2>;
			#interrupt-cells = <2>;
			interrupt-controller;
			interrupts = <GIC_SPI 153 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-parent = <&gic>;
		};

		gic: interrupt-controller@10300000 {
			compatible = "arm,gic-400";
			interrupt-controller;
			#interrupt-cells = <3>;
			interrupt-parent = <&gic>;
			reg = <0x10310000 0x1000>,
			      <0x10320000 0x1000>,
			      <0x10340000 0x2000>,
			      <0x10360000 0x2000>;
		};

		cci: cci@10390000 {
			compatible = "arm,cci-400";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x10390000 0x1000>;
			ranges = <0 0x10390000 0x10000>;

			cci_control0: slave-if@1000 {
				compatible = "arm,cci-400-ctrl-if";
				interface-type = "ace-lite";
				reg = <0x1000 0x1000>;
			};

			cci_control1: slave-if@4000 {
				compatible = "arm,cci-400-ctrl-if";
				interface-type = "ace";
				reg = <0x4000 0x1000>;
			};

			cci_control2: slave-if@5000 {
				compatible = "arm,cci-400-ctrl-if";
				interface-type = "ace";
				reg = <0x5000 0x1000>;
			};

			pmu@9000 {
				compatible = "arm,cci-400-pmu,r1";
				reg = <0x9000 0x5000>;
				interrupts = <GIC_SPI 58 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 59 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 60 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		uart0: serial@11002000 {
			compatible = "mediatek,mt7629-uart",
				     "mediatek,mt6577-uart";
			reg = <0x11002000 0x400>;
			interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_LOW>;
			clocks = <&topckgen CLK_TOP_UART_SEL>,
				 <&pericfg CLK_PERI_UART0_PD>;
			clock-names = "baud", "bus";
			status = "disabled";
		};

		uart1: serial@11003000 {
			compatible = "mediatek,mt7629-uart",
				     "mediatek,mt6577-uart";
			reg = <0x11003000 0x400>;
			interrupts = <GIC_SPI 92 IRQ_TYPE_LEVEL_LOW>;
			clocks = <&topckgen CLK_TOP_UART_SEL>,
				 <&pericfg CLK_PERI_UART1_PD>;
			clock-names = "baud", "bus";
			status = "disabled";
		};

		uart2: serial@11004000 {
			compatible = "mediatek,mt7629-uart",
				     "mediatek,mt6577-uart";
			reg = <0x11004000 0x400>;
			interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_LOW>;
			clocks = <&topckgen CLK_TOP_UART_SEL>,
				 <&pericfg CLK_PERI_UART2_PD>;
			clock-names = "baud", "bus";
			status = "disabled";
		};

		i2c: i2c@11007000 {
			compatible = "mediatek,mt7629-i2c",
				     "mediatek,mt2712-i2c";
			reg = <0x11007000 0x90>,
			      <0x11000100 0x80>;
			interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_LOW>;
			clock-div = <4>;
			clocks = <&pericfg CLK_PERI_I2C0_PD>,
				 <&pericfg CLK_PERI_AP_DMA_PD>;
			clock-names = "main", "dma";
			assigned-clocks = <&topckgen CLK_TOP_AXI_SEL>;
			assigned-clock-parents = <&topckgen CLK_TOP_SYSPLL1_D2>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		spi: spi@1100a000 {
			compatible = "mediatek,mt7629-spi",
				     "mediatek,mt7622-spi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x1100a000 0x100>;
			interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_LOW>;
			clocks = <&topckgen CLK_TOP_SYSPLL3_D2>,
				 <&topckgen CLK_TOP_SPI0_SEL>,
				 <&pericfg CLK_PERI_SPI0_PD>;
			clock-names = "parent-clk", "sel-clk", "spi-clk";
			status = "disabled";
		};

		qspi: spi@11014000 {
			compatible = "mediatek,mt7629-nor",
				     "mediatek,mt8173-nor";
			reg = <0x11014000 0xe0>;
			clocks = <&pericfg CLK_PERI_FLASH_PD>,
				 <&topckgen CLK_TOP_FLASH_SEL>;
			clock-names = "spi", "sf";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		wmac: wmac@18000000 {
			compatible = "mediatek,mt7629-wmac";
			reg = <0x18000000 0x100000>;
			interrupts = <GIC_SPI 211 IRQ_TYPE_LEVEL_LOW>,
				     <GIC_SPI 129 IRQ_TYPE_LEVEL_LOW>;
			mediatek,mtd-eeprom = <&factory 0x0000>;
			status = "disabled";
		};

		ssusbsys: syscon@1a000000 {
			compatible = "mediatek,mt7629-ssusbsys", "syscon";
			reg = <0x1a000000 0x1000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
		};

		ssusb: usb@1a0c0000 {
			compatible = "mediatek,mt7629-xhci",
				     "mediatek,mtk-xhci";
			reg = <0x1a0c0000 0x01000>,
			      <0x1a0c3e00 0x0100>;
			reg-names = "mac", "ippc";
			interrupts = <GIC_SPI 232 IRQ_TYPE_LEVEL_LOW>;
			clocks = <&ssusbsys CLK_SSUSB_SYS_EN>,
				 <&ssusbsys CLK_SSUSB_REF_EN>,
				 <&ssusbsys CLK_SSUSB_MCU_EN>,
				 <&ssusbsys CLK_SSUSB_DMA_EN>;
			clock-names = "sys_ck", "ref_ck", "mcu_ck", "dma_ck";
			assigned-clocks = <&topckgen CLK_TOP_AXI_SEL>,
					  <&topckgen CLK_TOP_SATA_SEL>,
					  <&topckgen CLK_TOP_HIF_SEL>;
			assigned-clock-parents = <&topckgen CLK_TOP_SYSPLL1_D2>,
						 <&topckgen CLK_TOP_UNIVPLL2_D4>,
						 <&topckgen CLK_TOP_UNIVPLL1_D2>;
			power-domains = <&scpsys MT7622_POWER_DOMAIN_HIF1>;
			phys = <&u2port0 PHY_TYPE_USB2>,
			       <&u3port0 PHY_TYPE_USB3>;
			status = "disabled";
		};

		u3phy1: usb-phy@1a0c4000 {
			compatible = "mediatek,generic-tphy-v2";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			status = "disabled";

			u2port0: usb-phy@1a0c4000 {
				reg = <0x1a0c4000 0x700>;
				clocks = <&ssusbsys CLK_SSUSB_U2_PHY_EN>;
				clock-names = "ref";
				#phy-cells = <1>;
				status = "okay";
			};

			u3port0: usb-phy@1a1c4700 {
				reg = <0x1a1c4700 0x700>;
				clocks = <&clk20m>;
				clock-names = "ref";
				#phy-cells = <1>;
				status = "okay";
			};
		};

		pciesys: syscon@1a100800 {
			compatible = "mediatek,mt7629-pciesys", "syscon";
			reg = <0x1a100800 0x1000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
		};

		ethsys: syscon@1b000000 {
			compatible = "mediatek,mt7629-ethsys", "syscon";
			reg = <0x1b000000 0x1000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
		};

	        eth: ethernet@1b100000 {
                compatible = "mediatek,mt7629-eth",
                                "syscon";
                reg = <0x1b100000 0x20000>;
                interrupts = <GIC_SPI 223 IRQ_TYPE_LEVEL_LOW>,
                             <GIC_SPI 224 IRQ_TYPE_LEVEL_LOW>,
                             <GIC_SPI 225 IRQ_TYPE_LEVEL_LOW>;
                clocks = <&topckgen CLK_TOP_ETH_SEL>,
                         <&topckgen CLK_TOP_F10M_REF_SEL>,
                         <&ethsys CLK_ETH_ESW_EN>,
                         <&ethsys CLK_ETH_GP0_EN>,
                         <&ethsys CLK_ETH_GP1_EN>,
                         <&ethsys CLK_ETH_GP2_EN>,
                         <&ethsys CLK_ETH_FE_EN>,
                         <&sgmiisys0 CLK_SGMII_TX_EN>,
                         <&sgmiisys0 CLK_SGMII_RX_EN>,
                         <&sgmiisys0 CLK_SGMII_CDR_REF>,
                         <&sgmiisys0 CLK_SGMII_CDR_FB>,
                         <&sgmiisys1 CLK_SGMII_TX_EN>,
                         <&sgmiisys1 CLK_SGMII_RX_EN>,
                         <&sgmiisys1 CLK_SGMII_CDR_REF>,
                         <&sgmiisys1 CLK_SGMII_CDR_FB>,
                         <&apmixedsys CLK_APMIXED_SGMIPLL>,
                         <&apmixedsys CLK_APMIXED_ETH2PLL>;
                clock-names = "ethif", "sgmiitop", "esw", "gp0", "gp1", "gp2",
                              "fe", "sgmii_tx250m", "sgmii_rx250m",
                              "sgmii_cdr_ref", "sgmii_cdr_fb",
                              "sgmii2_tx250m", "sgmii2_rx250m",
                              "sgmii2_cdr_ref", "sgmii2_cdr_fb",
                              "sgmii_ck", "eth2pll";
                assigned-clocks = <&topckgen CLK_TOP_ETH_SEL>,
                                  <&topckgen CLK_TOP_F10M_REF_SEL>;
                assigned-clock-parents = <&topckgen CLK_TOP_UNIVPLL1_D2>,
                                         <&topckgen CLK_TOP_SGMIIPLL_D2>;
                power-domains = <&scpsys MT7622_POWER_DOMAIN_ETHSYS>;
                mediatek,ethsys = <&ethsys>;
                mediatek,sgmiisys = <&sgmiisys0>,<&sgmiisys1>;
                mediatek,infracfg = <&infracfg>;
                #address-cells = <1>;
                #size-cells = <0>;
                status = "disabled";
		};

		sgmiisys0: syscon@1b128000 {
			compatible = "mediatek,mt7629-sgmiisys", "syscon";
			reg = <0x1b128000 0x3000>;
			#clock-cells = <1>;
			mediatek,physpeed = "2500";
		};

		sgmiisys1: syscon@1b130000 {
			compatible = "mediatek,mt7629-sgmiisys", "syscon";
			reg = <0x1b130000 0x3000>;
			#clock-cells = <1>;
			mediatek,physpeed = "2500";
		};
	};
};
