// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca953x.dtsi"

/ {
	aliases {
		led-boot = &led_link4;
		led-failsafe = &led_link4;
		led-running = &led_link4;
		led-upgrade = &led_link4;
		label-mac-device = &wmac;
	};

	leds: leds {
		compatible = "gpio-leds";

		link1 {
			label = "tp-link:green:link1";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		link2 {
			label = "tp-link:green:link2";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		link3 {
			label = "tp-link:green:link3";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		led_link4: link4 {
			label = "tp-link:green:link4";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};
};

&uart {
	status = "okay";
};

&spi {
	status = "okay";

	num-cs = <1>;

	flash@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				label = "partition-table";
				reg = <0x020000 0x010000>;
				read-only;
			};

			info: partition@30000 {
				label = "info";
				reg = <0x030000 0x010000>;
				read-only;
			};

			partition@40000 {
				label = "firmware";
				reg = <0x040000 0x780000>;
				compatible = "tplink,firmware";
			};

			config: partition@7c0000 {
				label = "config";
				reg = <0x7c0000 0x030000>;
				read-only;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	mtd-mac-address = <&info 0x8>;
};

&eth0 {
	status = "okay";

	phy-handle = <&swphy4>;

	mtd-mac-address = <&info 0x8>;
};
