From 7f2f9b54862f7df5cdef95b85234fad83b6b3480 Mon Sep 17 00:00:00 2001
From: Naushir Patuck <naush@raspberrypi.com>
Date: Wed, 22 Apr 2020 08:32:32 +0100
Subject: [PATCH] staging: vchiq: Load bcm2835_isp driver from vchiq

bcmn2835_isp is a platform driver dependent on vchiq,
therefore add the load/unload functions for it to vchiq.

Signed-off-by: Naushir Patuck <naush@raspberrypi.com>
---
 drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c | 3 +++
 1 file changed, 3 insertions(+)

--- a/drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c
+++ b/drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c
@@ -142,6 +142,7 @@ static struct platform_device *bcm2835_c
 static struct platform_device *bcm2835_audio;
 static struct platform_device *bcm2835_codec;
 static struct platform_device *vcsm_cma;
+static struct platform_device *bcm2835_isp;
 
 static struct vchiq_drvdata bcm2835_drvdata = {
 	.cache_line_size = 32,
@@ -3281,6 +3282,7 @@ static int vchiq_probe(struct platform_d
 	bcm2835_codec = vchiq_register_child(pdev, "bcm2835-codec");
 	bcm2835_camera = vchiq_register_child(pdev, "bcm2835-camera");
 	bcm2835_audio = vchiq_register_child(pdev, "bcm2835_audio");
+	bcm2835_isp = vchiq_register_child(pdev, "bcm2835-isp");
 
 	return 0;
 
@@ -3293,6 +3295,7 @@ failed_platform_init:
 
 static int vchiq_remove(struct platform_device *pdev)
 {
+	platform_device_unregister(bcm2835_isp);
 	platform_device_unregister(bcm2835_audio);
 	platform_device_unregister(bcm2835_camera);
 	platform_device_unregister(bcm2835_codec);
