#!/bin/sh
#
# Copyright (C) 2018 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
adtran,bsap1800-v2|\
adtran,bsap1840)
	ucidef_add_gpio_switch "wifi1_ext_a" "5GHz External Antenna A" "489" "1"
	ucidef_add_gpio_switch "wifi1_int_a" "5GHz Internal Antenna A" "493"
	ucidef_add_gpio_switch "wifi1_ext_b" "5GHz External Antenna B" "494" "1"
	ucidef_add_gpio_switch "wifi1_int_b" "5GHz Internal Antenna B" "495"
	ucidef_add_gpio_switch "wifi1_ext_c" "5GHz External Antenna C" "496" "1"
	ucidef_add_gpio_switch "wifi1_int_c" "5GHz Internal Antenna C" "497"
	ucidef_add_gpio_switch "wifi0_ext_a" "2.4GHz External Antenna A" "505" "1"
	ucidef_add_gpio_switch "wifi0_int_a" "2.4GHz Internal Antenna A" "506"
	ucidef_add_gpio_switch "wifi0_ext_b" "2.4GHz External Antenna B" "507" "1"
	ucidef_add_gpio_switch "wifi0_int_b" "2.4GHz Internal Antenna B" "508"
	ucidef_add_gpio_switch "wifi0_ext_c" "2.4GHz External Antenna C" "509" "1"
	ucidef_add_gpio_switch "wifi0_int_c" "2.4GHz Internal Antenna C" "510"
	;;
comfast,cf-e5)
	ucidef_add_gpio_switch "lte_power" "LTE Power" "14" "1"
	ucidef_add_gpio_switch "lte_wakeup" "LTE Wakeup" "11" "1"
	ucidef_add_gpio_switch "lte_poweroff" "LTE Poweroff" "1" "1"
	ucidef_add_gpio_switch "lte_reset" "LTE Reset" "12" "1"
	;;
devolo,magic-2-wifi)
	ucidef_add_gpio_switch "plc_pairing" "PLC pairing" "11" "1"
	ucidef_add_gpio_switch "plc_enable" "PLC enable" "13" "1"
	;;
dlink,dir-825-c1|\
dlink,dir-835-a1)
	ucidef_add_gpio_switch "wan_led_auto" "WAN LED Auto" "20" "0"
	;;
librerouter,librerouter-v1)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "1" "0"
	;;
teltonika,rut955)
	ucidef_add_gpio_switch "sim_sel" "SIM select" "503" "1"
	ucidef_add_gpio_switch "DOUT1" "DOUT1 (OC)" "504" "0"
	ucidef_add_gpio_switch "DOUT2" "DOUT2 (Relay)" "505" "0"
	ucidef_add_gpio_switch "modem_vbus" "Modem enable" "506" "1"
	ucidef_add_gpio_switch "modem_rst" "Modem reset" "507" "0"
	ucidef_add_gpio_switch "DOUT3" "DOUT3" "508" "0"
	;;
teltonika,rut955-h7v3c0)
	ucidef_add_gpio_switch "sim_sel" "SIM select" "503" "1"
	ucidef_add_gpio_switch "DOUT1" "DOUT1 (OC)" "504" "0"
	ucidef_add_gpio_switch "DOUT2" "DOUT2 (Relay)" "505" "0"
	ucidef_add_gpio_switch "modem_vbus" "Modem enable" "508" "1"
	ucidef_add_gpio_switch "modem_rst" "Modem reset" "509" "0"
	;;

tplink,archer-c25-v1)
	ucidef_add_gpio_switch "led_control" "LED control" "21" "0"
	ucidef_add_gpio_switch "led_reset" "LED reset" "19" "1"
	;;
tplink,cpe210-v1|\
tplink,cpe220-v2|\
tplink,cpe220-v3|\
tplink,cpe510-v1|\
tplink,wbs210-v1|\
tplink,wbs210-v2|\
tplink,wbs510-v1|\
tplink,wbs510-v2)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "20"
	;;
ubnt,nanostation-ac)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "3"
	;;
ubnt,nanostation-m)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "8"
	;;
ubnt,nanostation-m-xw)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "2"
	;;
ubnt,acb-isp)
	ucidef_add_gpio_switch "poe_passthrough" "PoE Passthrough" "11"
	;;
zbtlink,zbt-wd323)
	ucidef_add_gpio_switch "io0" "IO#0" "0"
	ucidef_add_gpio_switch "io1" "IO#1" "1"
	ucidef_add_gpio_switch "io2" "IO#2" "2"
	ucidef_add_gpio_switch "io14" "IO#14" "14"
	;;
esac

board_config_flush

exit 0
