From b763f24aed409296eb76d085c279b2c40462f8a1 Mon Sep 17 00:00:00 2001
From: Christoph Hellwig <hch@lst.de>
Date: Tue, 19 Nov 2019 17:38:58 +0100
Subject: [PATCH] dma-direct: exclude dma_direct_map_resource from the
 min_low_pfn check

commit 68a33b1794665ba8a1d1ef1d3bfcc7c587d380a6 upstream.

The valid memory address check in dma_capable only makes sense when mapping
normal memory, not when using dma_map_resource to map a device resource.
Add a new boolean argument to dma_capable to exclude that check for the
dma_map_resource case.

Fixes: b12d66278dd6 ("dma-direct: check for overflows on 32 bit DMA addresses")
Reported-by: Marek Szyprowski <m.szyprowski@samsung.com>
Signed-off-by: Christoph Hellwig <hch@lst.de>
Acked-by: Marek Szyprowski <m.szyprowski@samsung.com>
Tested-by: Marek Szyprowski <m.szyprowski@samsung.com>
---
 arch/x86/kernel/amd_gart_64.c | 4 ++--
 drivers/xen/swiotlb-xen.c     | 4 ++--
 include/linux/dma-direct.h    | 5 +++--
 kernel/dma/direct.c           | 4 ++--
 kernel/dma/swiotlb.c          | 2 +-
 5 files changed, 10 insertions(+), 9 deletions(-)

--- a/arch/x86/kernel/amd_gart_64.c
+++ b/arch/x86/kernel/amd_gart_64.c
@@ -185,13 +185,13 @@ static void iommu_full(struct device *de
 static inline int
 need_iommu(struct device *dev, unsigned long addr, size_t size)
 {
-	return force_iommu || !dma_capable(dev, addr, size);
+	return force_iommu || !dma_capable(dev, addr, size, true);
 }
 
 static inline int
 nonforced_iommu(struct device *dev, unsigned long addr, size_t size)
 {
-	return !dma_capable(dev, addr, size);
+	return !dma_capable(dev, addr, size, true);
 }
 
 /* Map a single continuous physical area into the IOMMU.
--- a/drivers/xen/swiotlb-xen.c
+++ b/drivers/xen/swiotlb-xen.c
@@ -375,7 +375,7 @@ static dma_addr_t xen_swiotlb_map_page(s
 	 * we can safely return the device addr and not worry about bounce
 	 * buffering it.
 	 */
-	if (dma_capable(dev, dev_addr, size) &&
+	if (dma_capable(dev, dev_addr, size, true) &&
 	    !range_straddles_page_boundary(phys, size) &&
 		!xen_arch_need_swiotlb(dev, phys, dev_addr) &&
 		swiotlb_force != SWIOTLB_FORCE)
@@ -397,7 +397,7 @@ static dma_addr_t xen_swiotlb_map_page(s
 	/*
 	 * Ensure that the address returned is DMA'ble
 	 */
-	if (unlikely(!dma_capable(dev, dev_addr, size))) {
+	if (unlikely(!dma_capable(dev, dev_addr, size, true))) {
 		swiotlb_tbl_unmap_single(dev, map, size, size, dir,
 				attrs | DMA_ATTR_SKIP_CPU_SYNC);
 		return DMA_MAPPING_ERROR;
--- a/include/linux/dma-direct.h
+++ b/include/linux/dma-direct.h
@@ -51,14 +51,15 @@ static inline phys_addr_t dma_to_phys(st
 	return __sme_clr(__dma_to_phys(dev, daddr));
 }
 
-static inline bool dma_capable(struct device *dev, dma_addr_t addr, size_t size)
+static inline bool dma_capable(struct device *dev, dma_addr_t addr, size_t size,
+		bool is_ram)
 {
 	dma_addr_t end = addr + size - 1;
 
 	if (!dev->dma_mask)
 		return false;
 
-	if (!IS_ENABLED(CONFIG_ARCH_DMA_ADDR_T_64BIT) &&
+	if (is_ram && !IS_ENABLED(CONFIG_ARCH_DMA_ADDR_T_64BIT) &&
 	    min(addr, end) < phys_to_dma(dev, PFN_PHYS(min_low_pfn)))
 		return false;
 
--- a/kernel/dma/direct.c
+++ b/kernel/dma/direct.c
@@ -326,7 +326,7 @@ static inline bool dma_direct_possible(s
 		size_t size)
 {
 	return swiotlb_force != SWIOTLB_FORCE &&
-		dma_capable(dev, dma_addr, size);
+		dma_capable(dev, dma_addr, size, true);
 }
 
 dma_addr_t dma_direct_map_page(struct device *dev, struct page *page,
@@ -375,7 +375,7 @@ dma_addr_t dma_direct_map_resource(struc
 {
 	dma_addr_t dma_addr = paddr;
 
-	if (unlikely(!dma_capable(dev, dma_addr, size))) {
+	if (unlikely(!dma_capable(dev, dma_addr, size, false))) {
 		report_addr(dev, dma_addr, size);
 		return DMA_MAPPING_ERROR;
 	}
--- a/kernel/dma/swiotlb.c
+++ b/kernel/dma/swiotlb.c
@@ -678,7 +678,7 @@ bool swiotlb_map(struct device *dev, phy
 
 	/* Ensure that the address returned is DMA'ble */
 	*dma_addr = __phys_to_dma(dev, *phys);
-	if (unlikely(!dma_capable(dev, *dma_addr, size))) {
+	if (unlikely(!dma_capable(dev, *dma_addr, size, true))) {
 		swiotlb_tbl_unmap_single(dev, *phys, size, size, dir,
 			attrs | DMA_ATTR_SKIP_CPU_SYNC);
 		return false;
