/dts-v1/;

#include "vr9.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/mips/lantiq_rcu_gphy.h>

/ {
	compatible = "netgear,dm200", "lantiq,xway", "lantiq,vr9";
	model = "Netgear DM200";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_amber;
		led-running = &power_green;
		led-upgrade = &power_green;

		led-dsl = &dsl_green;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;
		reset {
			label = "reset";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		annexa {
			gpio-export,name = "annexa";
			gpio-export,output = <0>;
			gpios = <&gpio 12 GPIO_ACTIVE_HIGH>;
		};
		annexb {
			gpio-export,name = "annexb";
			gpio-export,output = <0>;
			gpios = <&gpio 15 GPIO_ACTIVE_HIGH>;
		};
	};

	leds {
		compatible = "gpio-leds";

		power_amber: power_amber {
			label = "dm200:amber:power";
			gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
		};
		power_green: power_green {
			label = "dm200:green:power";
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
		};

		lan_amber {
			label = "dm200:amber:lan";
			gpios = <&gpio 33 GPIO_ACTIVE_HIGH>;
		};
		lan_green {
			label = "dm200:green:lan";
			gpios = <&gpio 11 GPIO_ACTIVE_HIGH>;
		};

		dsl_amber {
			label = "dm200:amber:dsl";
			gpios = <&gpio 8 GPIO_ACTIVE_HIGH>;
		};
		dsl_green: dsl_green {
			label = "dm200:green:dsl";
			gpios = <&gpio 36 GPIO_ACTIVE_HIGH>;
		};
	};
};

&eth0 {
	lantiq,phys = <&gphy1>;

	lan: interface@0 {
		compatible = "lantiq,xrx200-pdi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0>;

		ethernet@4 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <4>;
			phy-mode = "mii";
			phy-handle = <&phy13>;
		};
	};

	mdio {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "lantiq,xrx200-mdio";

		phy13: ethernet-phy@13 {
			reg = <0x13>;
			compatible = "lantiq,phy22f", "ethernet-phy-ieee802.3-c22";
		};
	};
};

&gphy1 {
	lantiq,gphy-mode = <GPHY_MODE_FE>;
};

&pcie0 {
	status = "disabled";
};

&spi {
	status = "okay";

	flash@4 {
		compatible = "jedec,spi-nor";
		reg = <4>;
		spi-max-frequency = <10000000>;

		partitions {
			#address-cells = <1>;
			#size-cells = <1>;
			compatible = "fixed-partitions";

			partition@0 {
				reg = <0x0 0x20000>;
				label = "uboot";
				read-only;
			};

			partition@20000 {
				reg = <0x20000 0x10000>;
				label = "gphyfirmware";
				read-only;
			};

			partition@30000 {
				reg = <0x30000 0x7b0000>;
				label = "firmware";
			};

			partition@7e0000 {
				reg = <0x7e0000 0x10000>;
				label = "sysconfig";
				read-only;
			};

			partition@7f0000 {
				reg = <0x7f0000 0x2000>;
				label = "ubootconfig";
				read-only;
			};

			partition@7f2000 {
				reg = <0x7f2000 0x1000>;
				label = "ART";
				read-only;
			};

			partition@7f3000 {
				reg = <0x7f3000 0x1000>;
				label = "pot";
				read-only;
			};

			partition@7f4000 {
				reg = <0x7f4000 0xc000>;
				label = "ret";
				read-only;
			};
		};
	};
};
