From d870db86f12a69361472fc86bc516b89d9bf468c Mon Sep 17 00:00:00 2001
From: Kuldeep Singh <kuldeep.singh@nxp.com>
Date: Wed, 8 Jan 2020 15:50:44 +0530
Subject: [PATCH] arm64: dts: ls1012ardb: Update qspi node property

Use generic node name and specific label name.
Add m25p,fast-read.

Use dt-bindings constants in interrupts instead of using numbers.

Signed-off-by: Kuldeep Singh <kuldeep.singh@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1012a-rdb.dts | 3 ++-
 arch/arm64/boot/dts/freescale/fsl-ls1012a.dtsi    | 2 +-
 2 files changed, 3 insertions(+), 2 deletions(-)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1012a-rdb.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1012a-rdb.dts
@@ -89,11 +89,12 @@
 &qspi {
 	status = "okay";
 
-	qflash0: s25fs512s@0 {
+	s25fs512s0: flash@0 {
 		compatible = "jedec,spi-nor";
 		#address-cells = <1>;
 		#size-cells = <1>;
 		spi-max-frequency = <20000000>;
+		m25p,fast-read;
 		reg = <0>;
 		spi-rx-bus-width = <1>;
 		spi-tx-bus-width = <1>;
--- a/arch/arm64/boot/dts/freescale/fsl-ls1012a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1012a.dtsi
@@ -391,7 +391,7 @@
 			reg = <0x0 0x1550000 0x0 0x10000>,
 				<0x0 0x40000000 0x0 0x10000000>;
 			reg-names = "QuadSPI", "QuadSPI-memory";
-			interrupts = <0 99 IRQ_TYPE_LEVEL_HIGH>;
+			interrupts = <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH>;
 			clock-names = "qspi_en", "qspi";
 			clocks = <&clockgen 4 0>, <&clockgen 4 0>;
 			status = "disabled";
