From e53b64cab45ea4d01226840efd963a6bec8ad2f9 Mon Sep 17 00:00:00 2001
From: Vladimir Oltean <vladimir.oltean@nxp.com>
Date: Mon, 6 Jan 2020 14:31:58 +0200
Subject: [PATCH] Revert "net: phylink: make QSGMII a valid PHY mode for
 in-band AN"

This reverts commit fe7fd9f6afce50c0fc09fd3d56cd59eda44d8dd0.

Signed-off-by: Vladimir Oltean <vladimir.oltean@nxp.com>
---
 drivers/net/phy/phylink.c | 1 -
 1 file changed, 1 deletion(-)

--- a/drivers/net/phy/phylink.c
+++ b/drivers/net/phy/phylink.c
@@ -283,7 +283,6 @@ static int phylink_parse_mode(struct phy
 
 		switch (pl->link_config.interface) {
 		case PHY_INTERFACE_MODE_SGMII:
-		case PHY_INTERFACE_MODE_QSGMII:
 			phylink_set(pl->supported, 10baseT_Half);
 			phylink_set(pl->supported, 10baseT_Full);
 			phylink_set(pl->supported, 100baseT_Half);
