/dts-v1/;

#include "mt7620a_asus_rt-ac5x.dtsi"

/ {
	compatible = "asus,rt-ac51u", "ralink,mt7620a-soc";
	model = "Asus RT-AC51U";

	aliases {
		label-mac-device = &ethernet;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "rt-ac51u:blue:power";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
		};

		usb {
			label = "rt-ac51u:blue:usb";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
			trigger-sources = <&ohci_port1>, <&ehci_port1>;
			linux,default-trigger = "usbport";
		};

		wifi2g {
			label = "rt-ac51u:blue:wifi2g";
			gpios = <&gpio3 0 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x28>;
};

&state_default {
	gpio {
		groups = "i2c", "wled", "uartf";
		function = "gpio";
	};
};

&pcie0 {
	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
	};
};
