From bd30f19a006fb52bac80c6463c49dd2f4159f4ac Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Sun, 28 Jul 2013 16:26:41 +0200
Subject: [PATCH 06/53] MIPS: ralink: add cpu frequency scaling

This feature will break udelay() and cause the delay loop to have longer delays
when the frequency is scaled causing a performance hit.

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 arch/mips/ralink/cevt-rt3352.c |   38 ++++++++++++++++++++++++++++++++++++++
 1 file changed, 38 insertions(+)

--- a/arch/mips/ralink/cevt-rt3352.c
+++ b/arch/mips/ralink/cevt-rt3352.c
@@ -29,6 +29,10 @@
 /* enable the counter */
 #define CFG_CNT_EN		0x1
 
+/* mt7620 frequency scaling defines */
+#define CLK_LUT_CFG	0x40
+#define SLEEP_EN	BIT(31)
+
 struct systick_device {
 	void __iomem *membase;
 	struct clock_event_device dev;
@@ -36,21 +40,53 @@ struct systick_device {
 	int freq_scale;
 };
 
+static void (*systick_freq_scaling)(struct systick_device *sdev, int status);
+
 static int systick_set_oneshot(struct clock_event_device *evt);
 static int systick_shutdown(struct clock_event_device *evt);
 
+static inline void mt7620_freq_scaling(struct systick_device *sdev, int status)
+{
+	if (sdev->freq_scale == status)
+		return;
+
+	sdev->freq_scale = status;
+
+	pr_info("%s: %s autosleep mode\n", sdev->dev.name,
+			(status) ? ("enable") : ("disable"));
+	if (status)
+		rt_sysc_w32(rt_sysc_r32(CLK_LUT_CFG) | SLEEP_EN, CLK_LUT_CFG);
+	else
+		rt_sysc_w32(rt_sysc_r32(CLK_LUT_CFG) & ~SLEEP_EN, CLK_LUT_CFG);
+}
+
+static inline unsigned int read_count(struct systick_device *sdev)
+{
+	return ioread32(sdev->membase + SYSTICK_COUNT);
+}
+
+static inline unsigned int read_compare(struct systick_device *sdev)
+{
+	return ioread32(sdev->membase + SYSTICK_COMPARE);
+}
+
+static inline void write_compare(struct systick_device *sdev, unsigned int val)
+{
+	iowrite32(val, sdev->membase + SYSTICK_COMPARE);
+}
+
 static int systick_next_event(unsigned long delta,
 				struct clock_event_device *evt)
 {
 	struct systick_device *sdev;
-	u32 count;
+	int res;
 
 	sdev = container_of(evt, struct systick_device, dev);
-	count = ioread32(sdev->membase + SYSTICK_COUNT);
-	count = (count + delta) % SYSTICK_FREQ;
-	iowrite32(count, sdev->membase + SYSTICK_COMPARE);
+	delta += read_count(sdev);
+	write_compare(sdev, delta);
+	res = ((int)(read_count(sdev) - delta) >= 0) ? -ETIME : 0;
 
-	return 0;
+	return res;
 }
 
 static void systick_event_handler(struct clock_event_device *dev)
@@ -60,20 +96,25 @@ static void systick_event_handler(struct
 
 static irqreturn_t systick_interrupt(int irq, void *dev_id)
 {
-	struct clock_event_device *dev = (struct clock_event_device *) dev_id;
+	int ret = 0;
+	struct clock_event_device *cdev;
+	struct systick_device *sdev;
 
-	dev->event_handler(dev);
+	if (read_c0_cause() & STATUSF_IP7) {
+		cdev = (struct clock_event_device *) dev_id;
+		sdev = container_of(cdev, struct systick_device, dev);
+
+		/* Clear Count/Compare Interrupt */
+		write_compare(sdev, read_compare(sdev));
+		cdev->event_handler(cdev);
+		ret = 1;
+	}
 
-	return IRQ_HANDLED;
+	return IRQ_RETVAL(ret);
 }
 
 static struct systick_device systick = {
 	.dev = {
-		/*
-		 * cevt-r4k uses 300, make sure systick
-		 * gets used if available
-		 */
-		.rating			= 310,
 		.features		= CLOCK_EVT_FEAT_ONESHOT,
 		.set_next_event		= systick_next_event,
 		.set_state_shutdown	= systick_shutdown,
@@ -95,9 +136,15 @@ static int systick_shutdown(struct clock
 	sdev = container_of(evt, struct systick_device, dev);
 
 	if (sdev->irq_requested)
-		free_irq(systick.dev.irq, &systick_irqaction);
+		remove_irq(systick.dev.irq, &systick_irqaction);
 	sdev->irq_requested = 0;
-	iowrite32(0, systick.membase + SYSTICK_CONFIG);
+	iowrite32(CFG_CNT_EN, systick.membase + SYSTICK_CONFIG);
+
+	if (systick_freq_scaling)
+		systick_freq_scaling(sdev, 0);
+
+	if (systick_freq_scaling)
+		systick_freq_scaling(sdev, 1);
 
 	return 0;
 }
@@ -117,34 +164,48 @@ static int systick_set_oneshot(struct cl
 	return 0;
 }
 
+static const struct of_device_id systick_match[] = {
+	{ .compatible = "ralink,mt7620a-systick", .data = mt7620_freq_scaling},
+	{},
+};
+
 static int __init ralink_systick_init(struct device_node *np)
 {
+	const struct of_device_id *match;
+	int rating = 200;
 	int ret;
 
 	systick.membase = of_iomap(np, 0);
 	if (!systick.membase)
 		return -ENXIO;
 
-	systick_irqaction.name = np->name;
-	systick.dev.name = np->name;
-	clockevents_calc_mult_shift(&systick.dev, SYSTICK_FREQ, 60);
-	systick.dev.max_delta_ns = clockevent_delta2ns(0x7fff, &systick.dev);
-	systick.dev.max_delta_ticks = 0x7fff;
-	systick.dev.min_delta_ns = clockevent_delta2ns(0x3, &systick.dev);
-	systick.dev.min_delta_ticks = 0x3;
+	match = of_match_node(systick_match, np);
+	if (match) {
+		systick_freq_scaling = match->data;
+		/*
+		 * cevt-r4k uses 300, make sure systick
+		 * gets used if available
+		 */
+		rating = 310;
+	}
+
+	/* enable counter than register clock source */
+	iowrite32(CFG_CNT_EN, systick.membase + SYSTICK_CONFIG);
+	clocksource_mmio_init(systick.membase + SYSTICK_COUNT, np->name,
+			SYSTICK_FREQ, rating, 16, clocksource_mmio_readl_up);
+
+	/* register clock event */
 	systick.dev.irq = irq_of_parse_and_map(np, 0);
 	if (!systick.dev.irq) {
 		pr_err("%s: request_irq failed", np->name);
 		return -EINVAL;
 	}
 
-	ret = clocksource_mmio_init(systick.membase + SYSTICK_COUNT, np->name,
-				    SYSTICK_FREQ, 301, 16,
-				    clocksource_mmio_readl_up);
-	if (ret)
-		return ret;
-
-	clockevents_register_device(&systick.dev);
+	systick_irqaction.name = np->name;
+	systick.dev.name = np->name;
+	systick.dev.rating = rating;
+	systick.dev.cpumask = cpumask_of(0);
+	clockevents_config_and_register(&systick.dev, SYSTICK_FREQ, 0x3, 0x7fff);
 
 	pr_info("%s: running - mult: %d, shift: %d\n",
 			np->name, systick.dev.mult, systick.dev.shift);
