From 17abc9ec68b73ddeb262a507a62421016b9c54d5 Mon Sep 17 00:00:00 2001
From: Tomasz Duszynski <tduszyns@gmail.com>
Date: Fri, 14 Dec 2018 19:28:01 +0100
Subject: [PATCH] iio: add IIO_MASSCONCENTRATION channel type

Measuring particulate matter in ug / m3 (micro-grams per cubic meter)
is de facto standard. Existing air quality sensors usually follow
this convention and are capable of returning measurements using
this unit.

IIO currently does not offer suitable channel type for this
type of measurements hence this patch adds this.

In addition, extra modifiers are introduced used for distinguishing
between fine pm1, pm2p5 and coarse pm4, pm10 particle measurements, i.e
IIO_MOD_PM1, IIO_MOD_PM25 and IIO_MOD_PM4, IIO_MOD_PM10.

pmX consists of particles with aerodynamic diameter less or equal to
X micrometers.

Signed-off-by: Tomasz Duszynski <tduszyns@gmail.com>
Acked-by: Matt Ranostay <matt.ranostay@konsulko.com>
Signed-off-by: Jonathan Cameron <Jonathan.Cameron@huawei.com>
---
 Documentation/ABI/testing/sysfs-bus-iio | 17 ++++++++++++++++-
 drivers/iio/industrialio-core.c         |  5 +++++
 include/uapi/linux/iio/types.h          |  5 +++++
 tools/iio/iio_event_monitor.c           | 10 ++++++++++
 4 files changed, 36 insertions(+), 1 deletion(-)

--- a/Documentation/ABI/testing/sysfs-bus-iio
+++ b/Documentation/ABI/testing/sysfs-bus-iio
@@ -1684,4 +1684,19 @@ KernelVersion:	4.18
 Contact:	linux-iio@vger.kernel.org
 Description:
 		Raw (unscaled) phase difference reading from channel Y
-		that can be processed to radians.
\ No newline at end of file
+		that can be processed to radians.
+
+What:		/sys/bus/iio/devices/iio:deviceX/in_massconcentration_pm1_input
+What:		/sys/bus/iio/devices/iio:deviceX/in_massconcentrationY_pm1_input
+What:		/sys/bus/iio/devices/iio:deviceX/in_massconcentration_pm2p5_input
+What:		/sys/bus/iio/devices/iio:deviceX/in_massconcentrationY_pm2p5_input
+What:		/sys/bus/iio/devices/iio:deviceX/in_massconcentration_pm4_input
+What:		/sys/bus/iio/devices/iio:deviceX/in_massconcentrationY_pm4_input
+What:		/sys/bus/iio/devices/iio:deviceX/in_massconcentration_pm10_input
+What:		/sys/bus/iio/devices/iio:deviceX/in_massconcentrationY_pm10_input
+KernelVersion:	4.22
+Contact:	linux-iio@vger.kernel.org
+Description:
+		Mass concentration reading of particulate matter in ug / m3.
+		pmX consists of particles with aerodynamic diameter less or
+		equal to X micrometers.
--- a/drivers/iio/industrialio-core.c
+++ b/drivers/iio/industrialio-core.c
@@ -87,6 +87,7 @@ static const char * const iio_chan_type_
 	[IIO_GRAVITY]  = "gravity",
 	[IIO_POSITIONRELATIVE]  = "positionrelative",
 	[IIO_PHASE] = "phase",
+	[IIO_MASSCONCENTRATION] = "massconcentration",
 };
 
 static const char * const iio_modifier_names[] = {
@@ -127,6 +128,10 @@ static const char * const iio_modifier_n
 	[IIO_MOD_Q] = "q",
 	[IIO_MOD_CO2] = "co2",
 	[IIO_MOD_VOC] = "voc",
+	[IIO_MOD_PM1] = "pm1",
+	[IIO_MOD_PM2P5] = "pm2p5",
+	[IIO_MOD_PM4] = "pm4",
+	[IIO_MOD_PM10] = "pm10",
 };
 
 /* relies on pairs of these shared then separate */
--- a/include/uapi/linux/iio/types.h
+++ b/include/uapi/linux/iio/types.h
@@ -46,6 +46,7 @@ enum iio_chan_type {
 	IIO_GRAVITY,
 	IIO_POSITIONRELATIVE,
 	IIO_PHASE,
+	IIO_MASSCONCENTRATION,
 };
 
 enum iio_modifier {
@@ -87,6 +88,10 @@ enum iio_modifier {
 	IIO_MOD_VOC,
 	IIO_MOD_LIGHT_UV,
 	IIO_MOD_LIGHT_DUV,
+	IIO_MOD_PM1,
+	IIO_MOD_PM2P5,
+	IIO_MOD_PM4,
+	IIO_MOD_PM10,
 };
 
 enum iio_event_type {
--- a/tools/iio/iio_event_monitor.c
+++ b/tools/iio/iio_event_monitor.c
@@ -60,6 +60,7 @@ static const char * const iio_chan_type_
 	[IIO_GRAVITY] = "gravity",
 	[IIO_POSITIONRELATIVE] = "positionrelative",
 	[IIO_PHASE] = "phase",
+	[IIO_MASSCONCENTRATION] = "massconcentration",
 };
 
 static const char * const iio_ev_type_text[] = {
@@ -115,6 +116,10 @@ static const char * const iio_modifier_n
 	[IIO_MOD_Q] = "q",
 	[IIO_MOD_CO2] = "co2",
 	[IIO_MOD_VOC] = "voc",
+	[IIO_MOD_PM1] = "pm1",
+	[IIO_MOD_PM2P5] = "pm2p5",
+	[IIO_MOD_PM4] = "pm4",
+	[IIO_MOD_PM10] = "pm10",
 };
 
 static bool event_is_known(struct iio_event_data *event)
@@ -156,6 +161,7 @@ static bool event_is_known(struct iio_ev
 	case IIO_GRAVITY:
 	case IIO_POSITIONRELATIVE:
 	case IIO_PHASE:
+	case IIO_MASSCONCENTRATION:
 		break;
 	default:
 		return false;
@@ -200,6 +206,10 @@ static bool event_is_known(struct iio_ev
 	case IIO_MOD_Q:
 	case IIO_MOD_CO2:
 	case IIO_MOD_VOC:
+	case IIO_MOD_PM1:
+	case IIO_MOD_PM2P5:
+	case IIO_MOD_PM4:
+	case IIO_MOD_PM10:
 		break;
 	default:
 		return false;
