From fa6e98cee558622565c97924e922b97340aeabd8 Mon Sep 17 00:00:00 2001
From: Heiner Kallweit <hkallweit1@gmail.com>
Date: Tue, 22 Oct 2019 11:31:07 -0700
Subject: [PATCH] net: phy: add support for clause 37 auto-negotiation
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This patch adds support for clause 37 1000Base-X auto-negotiation.

Signed-off-by: Heiner Kallweit <hkallweit1@gmail.com>
Signed-off-by: Tao Ren <taoren@fb.com>
Tested-by: René van Dorst <opensource@vdorst.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/phy_device.c | 139 +++++++++++++++++++++++++++++++++++
 include/linux/phy.h          |   4 +
 2 files changed, 143 insertions(+)

--- a/drivers/net/phy/phy_device.c
+++ b/drivers/net/phy/phy_device.c
@@ -1681,6 +1681,40 @@ static int genphy_config_advert(struct p
 }
 
 /**
+ * genphy_c37_config_advert - sanitize and advertise auto-negotiation parameters
+ * @phydev: target phy_device struct
+ *
+ * Description: Writes MII_ADVERTISE with the appropriate values,
+ *   after sanitizing the values to make sure we only advertise
+ *   what is supported.  Returns < 0 on error, 0 if the PHY's advertisement
+ *   hasn't changed, and > 0 if it has changed. This function is intended
+ *   for Clause 37 1000Base-X mode.
+ */
+static int genphy_c37_config_advert(struct phy_device *phydev)
+{
+	u16 adv = 0;
+
+	/* Only allow advertising what this PHY supports */
+	linkmode_and(phydev->advertising, phydev->advertising,
+		     phydev->supported);
+
+	if (linkmode_test_bit(ETHTOOL_LINK_MODE_1000baseX_Full_BIT,
+			      phydev->advertising))
+		adv |= ADVERTISE_1000XFULL;
+	if (linkmode_test_bit(ETHTOOL_LINK_MODE_Pause_BIT,
+			      phydev->advertising))
+		adv |= ADVERTISE_1000XPAUSE;
+	if (linkmode_test_bit(ETHTOOL_LINK_MODE_Asym_Pause_BIT,
+			      phydev->advertising))
+		adv |= ADVERTISE_1000XPSE_ASYM;
+
+	return phy_modify_changed(phydev, MII_ADVERTISE,
+				  ADVERTISE_1000XFULL | ADVERTISE_1000XPAUSE |
+				  ADVERTISE_1000XHALF | ADVERTISE_1000XPSE_ASYM,
+				  adv);
+}
+
+/**
  * genphy_config_eee_advert - disable unwanted eee mode advertisement
  * @phydev: target phy_device struct
  *
@@ -1789,6 +1823,54 @@ int __genphy_config_aneg(struct phy_devi
 EXPORT_SYMBOL(__genphy_config_aneg);
 
 /**
+ * genphy_c37_config_aneg - restart auto-negotiation or write BMCR
+ * @phydev: target phy_device struct
+ *
+ * Description: If auto-negotiation is enabled, we configure the
+ *   advertising, and then restart auto-negotiation.  If it is not
+ *   enabled, then we write the BMCR. This function is intended
+ *   for use with Clause 37 1000Base-X mode.
+ */
+int genphy_c37_config_aneg(struct phy_device *phydev)
+{
+	int err, changed;
+
+	if (phydev->autoneg != AUTONEG_ENABLE)
+		return genphy_setup_forced(phydev);
+
+	err = phy_modify(phydev, MII_BMCR, BMCR_SPEED1000 | BMCR_SPEED100,
+			 BMCR_SPEED1000);
+	if (err)
+		return err;
+
+	changed = genphy_c37_config_advert(phydev);
+	if (changed < 0) /* error */
+		return changed;
+
+	if (!changed) {
+		/* Advertisement hasn't changed, but maybe aneg was never on to
+		 * begin with?  Or maybe phy was isolated?
+		 */
+		int ctl = phy_read(phydev, MII_BMCR);
+
+		if (ctl < 0)
+			return ctl;
+
+		if (!(ctl & BMCR_ANENABLE) || (ctl & BMCR_ISOLATE))
+			changed = 1; /* do restart aneg */
+	}
+
+	/* Only restart aneg if we are advertising something different
+	 * than we were before.
+	 */
+	if (changed > 0)
+		return genphy_restart_aneg(phydev);
+
+	return 0;
+}
+EXPORT_SYMBOL(genphy_c37_config_aneg);
+
+/**
  * genphy_aneg_done - return auto-negotiation status
  * @phydev: target phy_device struct
  *
@@ -1960,6 +2042,63 @@ int genphy_read_status(struct phy_device
 EXPORT_SYMBOL(genphy_read_status);
 
 /**
+ * genphy_c37_read_status - check the link status and update current link state
+ * @phydev: target phy_device struct
+ *
+ * Description: Check the link, then figure out the current state
+ *   by comparing what we advertise with what the link partner
+ *   advertises. This function is for Clause 37 1000Base-X mode.
+ */
+int genphy_c37_read_status(struct phy_device *phydev)
+{
+	int lpa, err, old_link = phydev->link;
+
+	/* Update the link, but return if there was an error */
+	err = genphy_update_link(phydev);
+	if (err)
+		return err;
+
+	/* why bother the PHY if nothing can have changed */
+	if (phydev->autoneg == AUTONEG_ENABLE && old_link && phydev->link)
+		return 0;
+
+	phydev->duplex = DUPLEX_UNKNOWN;
+	phydev->pause = 0;
+	phydev->asym_pause = 0;
+
+	if (phydev->autoneg == AUTONEG_ENABLE && phydev->autoneg_complete) {
+		lpa = phy_read(phydev, MII_LPA);
+		if (lpa < 0)
+			return lpa;
+
+		linkmode_mod_bit(ETHTOOL_LINK_MODE_Autoneg_BIT,
+				 phydev->lp_advertising, lpa & LPA_LPACK);
+		linkmode_mod_bit(ETHTOOL_LINK_MODE_1000baseX_Full_BIT,
+				 phydev->lp_advertising, lpa & LPA_1000XFULL);
+		linkmode_mod_bit(ETHTOOL_LINK_MODE_Pause_BIT,
+				 phydev->lp_advertising, lpa & LPA_1000XPAUSE);
+		linkmode_mod_bit(ETHTOOL_LINK_MODE_Asym_Pause_BIT,
+				 phydev->lp_advertising,
+				 lpa & LPA_1000XPAUSE_ASYM);
+
+		phy_resolve_aneg_linkmode(phydev);
+	} else if (phydev->autoneg == AUTONEG_DISABLE) {
+		int bmcr = phy_read(phydev, MII_BMCR);
+
+		if (bmcr < 0)
+			return bmcr;
+
+		if (bmcr & BMCR_FULLDPLX)
+			phydev->duplex = DUPLEX_FULL;
+		else
+			phydev->duplex = DUPLEX_HALF;
+	}
+
+	return 0;
+}
+EXPORT_SYMBOL(genphy_c37_read_status);
+
+/**
  * genphy_soft_reset - software reset the PHY via BMCR_RESET bit
  * @phydev: target phy_device struct
  *
--- a/include/linux/phy.h
+++ b/include/linux/phy.h
@@ -1120,6 +1120,10 @@ int genphy_read_mmd_unsupported(struct p
 int genphy_write_mmd_unsupported(struct phy_device *phdev, int devnum,
 				 u16 regnum, u16 val);
 
+/* Clause 37 */
+int genphy_c37_config_aneg(struct phy_device *phydev);
+int genphy_c37_read_status(struct phy_device *phydev);
+
 /* Clause 45 PHY */
 int genphy_c45_restart_aneg(struct phy_device *phydev);
 int genphy_c45_check_and_restart_aneg(struct phy_device *phydev, bool restart);
