--- a/drivers/net/phy/Kconfig
+++ b/drivers/net/phy/Kconfig
@@ -524,6 +524,13 @@ config XILINX_GMII2RGMII
 	  the Reduced Gigabit Media Independent Interface(RGMII) between
 	  Ethernet physical media devices and the Gigabit Ethernet controller.
 
+config MDIO_IPQ40XX
+	tristate "Qualcomm Atheros ipq40xx MDIO interface"
+	depends on HAS_IOMEM && OF
+	---help---
+	  This driver supports the MDIO interface found in Qualcomm
+	  Atheros ipq40xx Soc chip.
+
 endif # PHYLIB
 
 config MICREL_KS8995MA
--- a/drivers/net/phy/Makefile
+++ b/drivers/net/phy/Makefile
@@ -48,6 +48,7 @@ obj-$(CONFIG_MDIO_CAVIUM)	+= mdio-cavium
 obj-$(CONFIG_MDIO_GPIO)		+= mdio-gpio.o
 obj-$(CONFIG_MDIO_HISI_FEMAC)	+= mdio-hisi-femac.o
 obj-$(CONFIG_MDIO_I2C)		+= mdio-i2c.o
+obj-$(CONFIG_MDIO_IPQ40XX)	+= mdio-ipq40xx.o
 obj-$(CONFIG_MDIO_MOXART)	+= mdio-moxart.o
 obj-$(CONFIG_MDIO_MSCC_MIIM)	+= mdio-mscc-miim.o
 obj-$(CONFIG_MDIO_OCTEON)	+= mdio-octeon.o
--- /dev/null
+++ b/drivers/net/phy/mdio-ipq40xx.c
@@ -0,0 +1,196 @@
+/*
+ * Copyright (c) 2015-2016, The Linux Foundation. All rights reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for
+ * any purpose with or without fee is hereby granted, provided that the
+ * above copyright notice and this permission notice appear in all copies.
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
+ * ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
+ * ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT
+ * OF OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ */
+
+#include <linux/delay.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/mutex.h>
+#include <linux/io.h>
+#include <linux/of_address.h>
+#include <linux/of_mdio.h>
+#include <linux/phy.h>
+#include <linux/platform_device.h>
+
+#define MDIO_CTRL_0_REG		0x40
+#define MDIO_CTRL_1_REG		0x44
+#define MDIO_CTRL_2_REG		0x48
+#define MDIO_CTRL_3_REG		0x4c
+#define MDIO_CTRL_4_REG		0x50
+#define MDIO_CTRL_4_ACCESS_BUSY		BIT(16)
+#define MDIO_CTRL_4_ACCESS_START		BIT(8)
+#define MDIO_CTRL_4_ACCESS_CODE_READ		0
+#define MDIO_CTRL_4_ACCESS_CODE_WRITE	1
+#define CTRL_0_REG_DEFAULT_VALUE	0x150FF
+
+#define IPQ40XX_MDIO_RETRY	1000
+#define IPQ40XX_MDIO_DELAY	10
+
+struct ipq40xx_mdio_data {
+	struct mii_bus	*mii_bus;
+	void __iomem	*membase;
+	struct device	*dev;
+};
+
+static int ipq40xx_mdio_wait_busy(struct ipq40xx_mdio_data *am)
+{
+	int i;
+
+	for (i = 0; i < IPQ40XX_MDIO_RETRY; i++) {
+		unsigned int busy;
+
+		busy = readl(am->membase + MDIO_CTRL_4_REG) &
+			MDIO_CTRL_4_ACCESS_BUSY;
+		if (!busy)
+			return 0;
+
+		/* BUSY might take to be cleard by 15~20 times of loop */
+		udelay(IPQ40XX_MDIO_DELAY);
+	}
+
+	dev_err(am->dev, "%s: MDIO operation timed out\n", am->mii_bus->name);
+
+	return -ETIMEDOUT;
+}
+
+static int ipq40xx_mdio_read(struct mii_bus *bus, int mii_id, int regnum)
+{
+	struct ipq40xx_mdio_data *am = bus->priv;
+	int value = 0;
+	unsigned int cmd = 0;
+
+	lockdep_assert_held(&bus->mdio_lock);
+
+	if (ipq40xx_mdio_wait_busy(am))
+		return -ETIMEDOUT;
+
+	/* issue the phy address and reg */
+	writel((mii_id << 8) | regnum, am->membase + MDIO_CTRL_1_REG);
+
+	cmd = MDIO_CTRL_4_ACCESS_START|MDIO_CTRL_4_ACCESS_CODE_READ;
+
+	/* issue read command */
+	writel(cmd, am->membase + MDIO_CTRL_4_REG);
+
+	/* Wait read complete */
+	if (ipq40xx_mdio_wait_busy(am))
+		return -ETIMEDOUT;
+
+	/* Read data */
+	value = readl(am->membase + MDIO_CTRL_3_REG);
+
+	return value;
+}
+
+static int ipq40xx_mdio_write(struct mii_bus *bus, int mii_id, int regnum,
+			    u16 value)
+{
+	struct ipq40xx_mdio_data *am = bus->priv;
+	unsigned int cmd = 0;
+
+	lockdep_assert_held(&bus->mdio_lock);
+
+	if (ipq40xx_mdio_wait_busy(am))
+		return -ETIMEDOUT;
+
+	/* issue the phy address and reg */
+	writel((mii_id << 8) | regnum, am->membase + MDIO_CTRL_1_REG);
+
+	/* issue write data */
+	writel(value, am->membase + MDIO_CTRL_2_REG);
+
+	cmd = MDIO_CTRL_4_ACCESS_START|MDIO_CTRL_4_ACCESS_CODE_WRITE;
+	/* issue write command */
+	writel(cmd, am->membase + MDIO_CTRL_4_REG);
+
+	/* Wait write complete */
+	if (ipq40xx_mdio_wait_busy(am))
+		return -ETIMEDOUT;
+
+	return 0;
+}
+
+static int ipq40xx_mdio_probe(struct platform_device *pdev)
+{
+	struct ipq40xx_mdio_data *am;
+	struct resource *res;
+	int i;
+
+	am = devm_kzalloc(&pdev->dev, sizeof(*am), GFP_KERNEL);
+	if (!am)
+		return -ENOMEM;
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	if (!res) {
+		dev_err(&pdev->dev, "no iomem resource found\n");
+		return -ENXIO;
+	}
+
+	am->membase = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(am->membase)) {
+		dev_err(&pdev->dev, "unable to ioremap registers\n");
+		return PTR_ERR(am->membase);
+	}
+
+	am->mii_bus = devm_mdiobus_alloc(&pdev->dev);
+	if (!am->mii_bus)
+		return  -ENOMEM;
+
+	writel(CTRL_0_REG_DEFAULT_VALUE, am->membase + MDIO_CTRL_0_REG);
+
+	am->mii_bus->name = "ipq40xx_mdio";
+	am->mii_bus->read = ipq40xx_mdio_read;
+	am->mii_bus->write = ipq40xx_mdio_write;
+	am->mii_bus->priv = am;
+	am->mii_bus->parent = &pdev->dev;
+	snprintf(am->mii_bus->id, MII_BUS_ID_SIZE, "%s", dev_name(&pdev->dev));
+
+	am->dev = &pdev->dev;
+	platform_set_drvdata(pdev, am);
+
+	return of_mdiobus_register(am->mii_bus, pdev->dev.of_node);
+}
+
+static int ipq40xx_mdio_remove(struct platform_device *pdev)
+{
+	struct ipq40xx_mdio_data *am = platform_get_drvdata(pdev);
+
+	mdiobus_unregister(am->mii_bus);
+
+	return 0;
+}
+
+static const struct of_device_id ipq40xx_mdio_dt_ids[] = {
+	{ .compatible = "qcom,ipq4019-mdio" },
+	{ }
+};
+MODULE_DEVICE_TABLE(of, ipq40xx_mdio_dt_ids);
+
+static struct platform_driver ipq40xx_mdio_driver = {
+	.probe = ipq40xx_mdio_probe,
+	.remove = ipq40xx_mdio_remove,
+	.driver = {
+		.name = "ipq40xx-mdio",
+		.of_match_table = ipq40xx_mdio_dt_ids,
+	},
+};
+
+module_platform_driver(ipq40xx_mdio_driver);
+
+#define DRV_VERSION     "1.0"
+
+MODULE_DESCRIPTION("IPQ40XX MDIO interface driver");
+MODULE_AUTHOR("Qualcomm Atheros");
+MODULE_VERSION(DRV_VERSION);
+MODULE_LICENSE("Dual BSD/GPL");
