From: Dan Haab <dan.haab@legrand.com>
Date: Wed, 2 Oct 2019 09:57:26 -0600
Subject: [PATCH] ARM: dts: BCM5301X: Add DT for Luxul XWC-2000

It's a simple network device based on BCM47094 with just a single
Ethernet port.

Signed-off-by: Dan Haab <dan.haab@legrand.com>
---
 arch/arm/boot/dts/Makefile                    |  1 +
 arch/arm/boot/dts/bcm47094-luxul-xwc-2000.dts | 53 +++++++++++++++++++
 2 files changed, 54 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm47094-luxul-xwc-2000.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -111,6 +111,7 @@ dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm47094-luxul-abr-4500.dtb \
 	bcm47094-luxul-xap-1610.dtb \
 	bcm47094-luxul-xbr-4500.dtb \
+	bcm47094-luxul-xwc-2000.dtb \
 	bcm47094-luxul-xwr-3100.dtb \
 	bcm47094-luxul-xwr-3150-v1.dtb \
 	bcm47094-netgear-r8500.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/bcm47094-luxul-xwc-2000.dts
@@ -0,0 +1,53 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+/*
+ * Copyright 2019 Legrand AV Inc.
+ */
+
+/dts-v1/;
+
+#include "bcm47094.dtsi"
+#include "bcm5301x-nand-cs0-bch8.dtsi"
+
+/ {
+	compatible = "luxul,xwc-2000-v1", "brcm,bcm47094", "brcm,bcm4708";
+	model = "Luxul XWC-2000 V1";
+
+	chosen {
+		bootargs = "earlycon";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000
+		       0x88000000 0x18000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		status	{
+			label = "bcm53xx:green:status";
+			gpios = <&chipcommon 18 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "timer";
+		};
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&chipcommon 19 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+&uart1 {
+	status = "okay";
+};
+
+&spi_nor {
+	status = "okay";
+};
