From 04b3b72b5b8fdb883bfdc619cb29b03641b1cc6a Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Thu, 15 Aug 2019 19:28:23 +0200
Subject: [PATCH] ARM: dts: qcom: ipq4019: Add SDHCI controller node

IPQ4019 has a built in SD/eMMC controller which is supported by the
SDHCI MSM driver, by the "qcom,sdhci-msm-v4" binding.
So lets add the appropriate node for it.

Signed-off-by: Robert Marko <robimarko@gmail.com>
Signed-off-by: Bjorn Andersson <bjorn.andersson@linaro.org>
---
 arch/arm/boot/dts/qcom-ipq4019.dtsi | 12 ++++++++++++
 1 file changed, 12 insertions(+)

--- a/arch/arm/boot/dts/qcom-ipq4019.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq4019.dtsi
@@ -209,6 +209,18 @@
 			interrupts = <GIC_SPI 208 IRQ_TYPE_LEVEL_HIGH>;
 		};
 
+		sdhci: sdhci@7824900 {
+			compatible = "qcom,sdhci-msm-v4";
+			reg = <0x7824900 0x11c>, <0x7824000 0x800>;
+			interrupts = <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 138 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "hc_irq", "pwr_irq";
+			bus-width = <8>;
+			clocks = <&gcc GCC_SDCC1_APPS_CLK>, <&gcc GCC_SDCC1_AHB_CLK>,
+				 <&gcc GCC_DCD_XO_CLK>;
+			clock-names = "core", "iface", "xo";
+			status = "disabled";
+		};
+
 		blsp_dma: dma@7884000 {
 			compatible = "qcom,bam-v1.7.0";
 			reg = <0x07884000 0x23000>;
