From: Felix Fietkau <nbd@nbd.name>
Date: Fri, 24 Jul 2020 20:25:07 +0200
Subject: [PATCH] mac80211: improve AQL tx airtime estimation

AQL does not take into account that most HT/VHT/HE traffic is A-MPDU aggregated.
Because of that, the per-packet airtime overhead is vastly overestimated.
Improve it by assuming an average aggregation length of 16 for non-legacy
traffic if not using the VO AC queue.
This should improve performance with high data rates, especially with multiple
stations

Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/net/mac80211/airtime.c
+++ b/net/mac80211/airtime.c
@@ -551,7 +551,7 @@ EXPORT_SYMBOL_GPL(ieee80211_calc_tx_airt
 u32 ieee80211_calc_expected_tx_airtime(struct ieee80211_hw *hw,
 				       struct ieee80211_vif *vif,
 				       struct ieee80211_sta *pubsta,
-				       int len)
+				       int len, bool ampdu)
 {
 	struct ieee80211_supported_band *sband;
 	struct ieee80211_chanctx_conf *conf;
@@ -572,10 +572,26 @@ u32 ieee80211_calc_expected_tx_airtime(s
 	if (pubsta) {
 		struct sta_info *sta = container_of(pubsta, struct sta_info,
 						    sta);
+		struct ieee80211_tx_rate *rate = &sta->tx_stats.last_rate;
+		u32 airtime;
 
-		return ieee80211_calc_tx_airtime_rate(hw,
-						      &sta->tx_stats.last_rate,
-						      band, len);
+		if (!(rate->flags & (IEEE80211_TX_RC_VHT_MCS |
+				     IEEE80211_TX_RC_MCS)))
+			ampdu = false;
+
+		/*
+		 * Assume that HT/VHT transmission on any AC except VO will
+		 * use aggregation. Since we don't have reliable reporting
+		 * of aggregation length, assume an average of 16.
+		 * This will not be very accurate, but much better than simply
+		 * assuming un-aggregated tx.
+		 */
+		airtime = ieee80211_calc_tx_airtime_rate(hw, rate, band,
+							 ampdu ? len * 16 : len);
+		if (ampdu)
+			airtime /= 16;
+
+		return airtime;
 	}
 
 	if (!conf)
--- a/net/mac80211/ieee80211_i.h
+++ b/net/mac80211/ieee80211_i.h
@@ -2278,7 +2278,7 @@ extern const struct ethtool_ops ieee8021
 u32 ieee80211_calc_expected_tx_airtime(struct ieee80211_hw *hw,
 				       struct ieee80211_vif *vif,
 				       struct ieee80211_sta *pubsta,
-				       int len);
+				       int len, bool ampdu);
 #ifdef CPTCFG_MAC80211_NOINLINE
 #define debug_noinline noinline
 #else
--- a/net/mac80211/tx.c
+++ b/net/mac80211/tx.c
@@ -3694,10 +3694,11 @@ encap_out:
 
 	if (vif &&
 	    wiphy_ext_feature_isset(local->hw.wiphy, NL80211_EXT_FEATURE_AQL)) {
+		bool ampdu = txq->ac != IEEE80211_AC_VO;
 		u32 airtime;
 
 		airtime = ieee80211_calc_expected_tx_airtime(hw, vif, txq->sta,
-							     skb->len);
+							     skb->len, ampdu);
 		if (airtime) {
 			airtime = ieee80211_info_set_tx_time_est(info, airtime);
 			ieee80211_sta_update_pending_airtime(local, tx.sta,
