// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca956x.dtsi"

/ {
	compatible = "tplink,archer-c5x", "qca,qca9560";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		label-mac-device = &eth1;
	};

	led_spi {
		compatible = "spi-gpio";
		#address-cells = <1>;
		#size-cells = <0>;

		sck-gpios = <&gpio 18 GPIO_ACTIVE_HIGH>;
		mosi-gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
		cs-gpios = <&gpio 20 GPIO_ACTIVE_HIGH>;
		num-chipselects = <1>;

		led_gpio: led_gpio@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			gpio-controller;
			#gpio-cells = <2>;
			registers-number = <1>;
			spi-max-frequency = <10000000>;
		};
	};

	leds: leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "tp-link:green:power";
			gpios = <&led_gpio 0 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan2g {
			label = "tp-link:green:wlan2g";
			gpios = <&led_gpio 1 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g {
			label = "tp-link:green:wlan5g";
			gpios = <&led_gpio 2 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wan_green {
			label = "tp-link:green:wan";
			gpios = <&led_gpio 4 GPIO_ACTIVE_LOW>;
		};

		wan_amber {
			label = "tp-link:amber:wan";
			gpios = <&led_gpio 5 GPIO_ACTIVE_LOW>;
		};

		lan {
			label = "tp-link:green:lan";
			gpios = <&led_gpio 3 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "tp-link:green:wps";
			gpios = <&led_gpio 6 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "WPS button";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		wifi {
			label = "WiFi button";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
		};
	};

	gpio-export {
		compatible = "gpio-export";

		gpio_shift_register_oe {
			gpio-export,name = "tp-link:oe:sr";
			gpio-export,output = <0>;
			gpios = <&gpio 16 GPIO_ACTIVE_HIGH>;
		};

		gpio_shift_register_reset {
			gpio-export,name = "tp-link:reset:sr";
			gpio-export,output = <1>;
			gpios = <&gpio 19 GPIO_ACTIVE_HIGH>;
		};
	};
};

&uart {
	status = "okay";
};

&pcie {
	status = "okay";
};

&eth0 {
	status = "okay";

	phy-handle = <&swphy0>;

	mtd-mac-address = <&mac 0x8>;
	mtd-mac-address-increment = <1>;

	gmac-config {
		device = <&gmac>;

		switch-phy-addr-swap = <1>;
		switch-phy-swap = <1>;
	};
};

&eth1 {
	status = "okay";

	mtd-mac-address = <&mac 0x8>;
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	mtd-mac-address = <&mac 0x8>;
};
