From e4a3e9ff5ba9f6b67595ec2768ed4be2054c2aa5 Mon Sep 17 00:00:00 2001
From: YueHaibing <yuehaibing@huawei.com>
Date: Thu, 22 Nov 2018 14:42:00 +0800
Subject: [PATCH] net: mvneta: remove redundant check for
 eee->tx_lpi_timer < 0

fixes the smatch warning:

drivers/net/ethernet/marvell/mvneta.c:4252 mvneta_ethtool_set_eee() warn:
 unsigned 'eee->tx_lpi_timer' is never less than zero.

Signed-off-by: YueHaibing <yuehaibing@huawei.com>
Acked-by: Thomas Petazzoni <thomas.petazzoni@bootlin.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/marvell/mvneta.c | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

--- a/drivers/net/ethernet/marvell/mvneta.c
+++ b/drivers/net/ethernet/marvell/mvneta.c
@@ -4267,8 +4267,7 @@ static int mvneta_ethtool_set_eee(struct
 
 	/* The Armada 37x documents do not give limits for this other than
 	 * it being an 8-bit register. */
-	if (eee->tx_lpi_enabled &&
-	    (eee->tx_lpi_timer < 0 || eee->tx_lpi_timer > 255))
+	if (eee->tx_lpi_enabled && eee->tx_lpi_timer > 255)
 		return -EINVAL;
 
 	lpi_ctl0 = mvreg_read(pp, MVNETA_LPI_CTRL_0);
