// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include "mt7620a_iptime.dtsi"

/ {
	compatible = "iptime,a1004ns", "ralink,mt7620a-soc";
	model = "ipTIME A1004ns";

	aliases {
		led-boot = &led_cpu;
		led-failsafe = &led_cpu;
		led-running = &led_cpu;
		led-upgrade = &led_cpu;
	};

	leds {
		compatible = "gpio-leds";

		led_cpu: cpu {
			label = "a1004ns:blue:cpu";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
		};

		usb {
			label = "a1004ns:blue:usb";
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
			trigger-sources = <&ohci_port1>, <&ehci_port1>;
			linux,default-trigger = "usbport";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};
};

&firmware {
	reg = <0x30000 0xfd0000>;
};

&state_default {
	gpio {
		groups = "i2c", "uartf", "spi refclk";
		function = "gpio";
	};
};

&ethernet {
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii1_pins &mdio_pins>;

	port@5 {
		status = "okay";
		mediatek,fixed-link = <1000 1 1 1>;
		phy-mode = "rgmii";
	};

	mdio-bus {
		status = "okay";

		ethernet-phy@0 {
			reg = <0>;
			phy-mode = "rgmii";
		};

		ethernet-phy@1 {
			reg = <1>;
			phy-mode = "rgmii";
		};

		ethernet-phy@2 {
			reg = <2>;
			phy-mode = "rgmii";
		};

		ethernet-phy@3 {
			reg = <3>;
			phy-mode = "rgmii";
		};

		ethernet-phy@4 {
			reg = <4>;
			phy-mode = "rgmii";
		};

		ethernet-phy@1f {
			reg = <0x1f>;
			phy-mode = "rgmii";
		};
	};
};
