From eb5df3d026824832831376bbdf04e01a52776eea Mon Sep 17 00:00:00 2001
From: Russell King <rmk+kernel@armlinux.org.uk>
Date: Tue, 28 May 2019 10:57:29 +0100
Subject: [PATCH 608/660] net: phy: allow Clause 45 access via mii ioctl

Allow userspace to generate Clause 45 MII access cycles via phylib.
This is useful for tools such as mii-diag to be able to inspect Clause
45 PHYs.

Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Russell King <rmk+kernel@armlinux.org.uk>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Russell King <rmk+kernel@armlinux.org.uk>
---
 drivers/net/phy/phy.c | 33 ++++++++++++++++++++++++---------
 1 file changed, 24 insertions(+), 9 deletions(-)

--- a/drivers/net/phy/phy.c
+++ b/drivers/net/phy/phy.c
@@ -397,6 +397,7 @@ int phy_mii_ioctl(struct phy_device *phy
 	struct mii_ioctl_data *mii_data = if_mii(ifr);
 	u16 val = mii_data->val_in;
 	bool change_autoneg = false;
+	int prtad, devad;
 
 	switch (cmd) {
 	case SIOCGMIIPHY:
@@ -404,14 +405,29 @@ int phy_mii_ioctl(struct phy_device *phy
 		/* fall through */
 
 	case SIOCGMIIREG:
-		mii_data->val_out = mdiobus_read(phydev->mdio.bus,
-						 mii_data->phy_id,
-						 mii_data->reg_num);
+		if (mdio_phy_id_is_c45(mii_data->phy_id)) {
+			prtad = mdio_phy_id_prtad(mii_data->phy_id);
+			devad = mdio_phy_id_devad(mii_data->phy_id);
+			devad = MII_ADDR_C45 | devad << 16 | mii_data->reg_num;
+		} else {
+			prtad = mii_data->phy_id;
+			devad = mii_data->reg_num;
+		}
+		mii_data->val_out = mdiobus_read(phydev->mdio.bus, prtad,
+						 devad);
 		return 0;
 
 	case SIOCSMIIREG:
-		if (mii_data->phy_id == phydev->mdio.addr) {
-			switch (mii_data->reg_num) {
+		if (mdio_phy_id_is_c45(mii_data->phy_id)) {
+			prtad = mdio_phy_id_prtad(mii_data->phy_id);
+			devad = mdio_phy_id_devad(mii_data->phy_id);
+			devad = MII_ADDR_C45 | devad << 16 | mii_data->reg_num;
+		} else {
+			prtad = mii_data->phy_id;
+			devad = mii_data->reg_num;
+		}
+		if (prtad == phydev->mdio.addr) {
+			switch (devad) {
 			case MII_BMCR:
 				if ((val & (BMCR_RESET | BMCR_ANENABLE)) == 0) {
 					if (phydev->autoneg == AUTONEG_ENABLE)
@@ -443,11 +459,10 @@ int phy_mii_ioctl(struct phy_device *phy
 			}
 		}
 
-		mdiobus_write(phydev->mdio.bus, mii_data->phy_id,
-			      mii_data->reg_num, val);
+		mdiobus_write(phydev->mdio.bus, prtad, devad, val);
 
-		if (mii_data->phy_id == phydev->mdio.addr &&
-		    mii_data->reg_num == MII_BMCR &&
+		if (prtad == phydev->mdio.addr &&
+		    devad == MII_BMCR &&
 		    val & BMCR_RESET)
 			return phy_init_hw(phydev);
 
