diff -Nur linux-2.4.32/include/linux/netdevice.h linux-2.4.32-we/include/linux/netdevice.h
--- linux-2.4.32/include/linux/netdevice.h	2004-11-17 12:54:22.000000000 +0100
+++ linux-2.4.32-we/include/linux/netdevice.h	2006-03-13 12:10:57.000000000 +0100
@@ -295,7 +295,9 @@
 
 	/* List of functions to handle Wireless Extensions (instead of ioctl).
 	 * See <net/iw_handler.h> for details. Jean II */
-	struct iw_handler_def *	wireless_handlers;
+	const struct iw_handler_def *	wireless_handlers;
+	/* Instance data managed by the core of Wireless Extensions. */
+	struct iw_public_data *	wireless_data;
 
 	struct ethtool_ops *ethtool_ops;
 
diff -Nur linux-2.4.32/include/linux/wireless.h linux-2.4.32-we/include/linux/wireless.h
--- linux-2.4.32/include/linux/wireless.h	2003-11-28 19:26:21.000000000 +0100
+++ linux-2.4.32-we/include/linux/wireless.h	2006-03-13 12:11:02.000000000 +0100
@@ -1,10 +1,10 @@
 /*
  * This file define a set of standard wireless extensions
  *
- * Version :	16	2.4.03
+ * Version :	18	12.3.05
  *
  * Authors :	Jean Tourrilhes - HPL - <jt@hpl.hp.com>
- * Copyright (c) 1997-2002 Jean Tourrilhes, All Rights Reserved.
+ * Copyright (c) 1997-2005 Jean Tourrilhes, All Rights Reserved.
  */
 
 #ifndef _LINUX_WIRELESS_H
@@ -47,12 +47,12 @@
  *	# include/net/iw_handler.h
  *
  * Note as well that /proc/net/wireless implementation has now moved in :
- *	# include/linux/wireless.c
+ *	# net/core/wireless.c
  *
  * Wireless Events (2002 -> onward) :
  * --------------------------------
  * Events are defined at the end of this file, and implemented in :
- *	# include/linux/wireless.c
+ *	# net/core/wireless.c
  *
  * Other comments :
  * --------------
@@ -82,7 +82,7 @@
  * (there is some stuff that will be added in the future...)
  * I just plan to increment with each new version.
  */
-#define WIRELESS_EXT	16
+#define WIRELESS_EXT	18
 
 /*
  * Changes :
@@ -175,6 +175,28 @@
  *	- Remove IW_MAX_GET_SPY because conflict with enhanced spy support
  *	- Add SIOCSIWTHRSPY/SIOCGIWTHRSPY and "struct iw_thrspy"
  *	- Add IW_ENCODE_TEMP and iw_range->encoding_login_index
+ *
+ * V16 to V17
+ * ----------
+ *	- Add flags to frequency -> auto/fixed
+ *	- Document (struct iw_quality *)->updated, add new flags (INVALID)
+ *	- Wireless Event capability in struct iw_range
+ *	- Add support for relative TxPower (yick !)
+ *
+ * V17 to V18 (From Jouni Malinen <jkmaline@cc.hut.fi>)
+ * ----------
+ *	- Add support for WPA/WPA2
+ *	- Add extended encoding configuration (SIOCSIWENCODEEXT and
+ *	  SIOCGIWENCODEEXT)
+ *	- Add SIOCSIWGENIE/SIOCGIWGENIE
+ *	- Add SIOCSIWMLME
+ *	- Add SIOCSIWPMKSA
+ *	- Add struct iw_range bit field for supported encoding capabilities
+ *	- Add optional scan request parameters for SIOCSIWSCAN
+ *	- Add SIOCSIWAUTH/SIOCGIWAUTH for setting authentication and WPA
+ *	  related parameters (extensible up to 4096 parameter values)
+ *	- Add wireless events: IWEVGENIE, IWEVMICHAELMICFAILURE,
+ *	  IWEVASSOCREQIE, IWEVASSOCRESPIE, IWEVPMKIDCAND
  */
 
 /**************************** CONSTANTS ****************************/
@@ -249,9 +271,33 @@
 #define SIOCSIWPOWER	0x8B2C		/* set Power Management settings */
 #define SIOCGIWPOWER	0x8B2D		/* get Power Management settings */
 
+/* WPA : Generic IEEE 802.11 informatiom element (e.g., for WPA/RSN/WMM).
+ * This ioctl uses struct iw_point and data buffer that includes IE id and len
+ * fields. More than one IE may be included in the request. Setting the generic
+ * IE to empty buffer (len=0) removes the generic IE from the driver. Drivers
+ * are allowed to generate their own WPA/RSN IEs, but in these cases, drivers
+ * are required to report the used IE as a wireless event, e.g., when
+ * associating with an AP. */
+#define SIOCSIWGENIE	0x8B30		/* set generic IE */
+#define SIOCGIWGENIE	0x8B31		/* get generic IE */
+
+/* WPA : IEEE 802.11 MLME requests */
+#define SIOCSIWMLME	0x8B16		/* request MLME operation; uses
+					 * struct iw_mlme */
+/* WPA : Authentication mode parameters */
+#define SIOCSIWAUTH	0x8B32		/* set authentication mode params */
+#define SIOCGIWAUTH	0x8B33		/* get authentication mode params */
+
+/* WPA : Extended version of encoding configuration */
+#define SIOCSIWENCODEEXT 0x8B34		/* set encoding token & mode */
+#define SIOCGIWENCODEEXT 0x8B35		/* get encoding token & mode */
+
+/* WPA2 : PMKSA cache management */
+#define SIOCSIWPMKSA	0x8B36		/* PMKSA cache operation */
+
 /* -------------------- DEV PRIVATE IOCTL LIST -------------------- */
 
-/* These 16 ioctl are wireless device private.
+/* These 32 ioctl are wireless device private, for 16 commands.
  * Each driver is free to use them for whatever purpose it chooses,
  * however the driver *must* export the description of those ioctls
  * with SIOCGIWPRIV and *must* use arguments as defined below.
@@ -266,8 +312,8 @@
  * We now have 32 commands, so a bit more space ;-).
  * Also, all 'odd' commands are only usable by root and don't return the
  * content of ifr/iwr to user (but you are not obliged to use the set/get
- * convention, just use every other two command).
- * And I repeat : you are not obliged to use them with iwspy, but you
+ * convention, just use every other two command). More details in iwpriv.c.
+ * And I repeat : you are not forced to use them with iwpriv, but you
  * must be compliant with it.
  */
 
@@ -290,6 +336,34 @@
 #define IWEVCUSTOM	0x8C02		/* Driver specific ascii string */
 #define IWEVREGISTERED	0x8C03		/* Discovered a new node (AP mode) */
 #define IWEVEXPIRED	0x8C04		/* Expired a node (AP mode) */
+#define IWEVGENIE	0x8C05		/* Generic IE (WPA, RSN, WMM, ..)
+					 * (scan results); This includes id and
+					 * length fields. One IWEVGENIE may
+					 * contain more than one IE. Scan
+					 * results may contain one or more
+					 * IWEVGENIE events. */
+#define IWEVMICHAELMICFAILURE 0x8C06	/* Michael MIC failure
+					 * (struct iw_michaelmicfailure)
+					 */
+#define IWEVASSOCREQIE	0x8C07		/* IEs used in (Re)Association Request.
+					 * The data includes id and length
+					 * fields and may contain more than one
+					 * IE. This event is required in
+					 * Managed mode if the driver
+					 * generates its own WPA/RSN IE. This
+					 * should be sent just before
+					 * IWEVREGISTERED event for the
+					 * association. */
+#define IWEVASSOCRESPIE	0x8C08		/* IEs used in (Re)Association
+					 * Response. The data includes id and
+					 * length fields and may contain more
+					 * than one IE. This may be sent
+					 * between IWEVASSOCREQIE and
+					 * IWEVREGISTERED events for the
+					 * association. */
+#define IWEVPMKIDCAND	0x8C09		/* PMKID candidate for RSN
+					 * pre-authentication
+					 * (struct iw_pmkid_cand) */
 
 #define IWEVFIRST	0x8C00
 
@@ -352,6 +426,18 @@
 #define IW_MODE_SECOND	5	/* Secondary master/repeater (backup) */
 #define IW_MODE_MONITOR	6	/* Passive monitor (listen only) */
 
+/* Statistics flags (bitmask in updated) */
+#define IW_QUAL_QUAL_UPDATED	0x1	/* Value was updated since last read */
+#define IW_QUAL_LEVEL_UPDATED	0x2
+#define IW_QUAL_NOISE_UPDATED	0x4
+#define IW_QUAL_QUAL_INVALID	0x10	/* Driver doesn't provide value */
+#define IW_QUAL_LEVEL_INVALID	0x20
+#define IW_QUAL_NOISE_INVALID	0x40
+
+/* Frequency flags */
+#define IW_FREQ_AUTO		0x00	/* Let the driver decides */
+#define IW_FREQ_FIXED		0x01	/* Force a specific value */
+
 /* Maximum number of size of encoding token available
  * they are listed in the range structure */
 #define IW_MAX_ENCODING_SIZES	8
@@ -390,6 +476,7 @@
 #define IW_TXPOW_TYPE		0x00FF	/* Type of value */
 #define IW_TXPOW_DBM		0x0000	/* Value is in dBm */
 #define IW_TXPOW_MWATT		0x0001	/* Value is in mW */
+#define IW_TXPOW_RELATIVE	0x0002	/* Value is in arbitrary units */
 #define IW_TXPOW_RANGE		0x1000	/* Range of value between min/max */
 
 /* Retry limits and lifetime flags available */
@@ -412,12 +499,113 @@
 #define IW_SCAN_THIS_MODE	0x0020	/* Scan only this Mode */
 #define IW_SCAN_ALL_RATE	0x0040	/* Scan all Bit-Rates */
 #define IW_SCAN_THIS_RATE	0x0080	/* Scan only this Bit-Rate */
+/* struct iw_scan_req scan_type */
+#define IW_SCAN_TYPE_ACTIVE 0
+#define IW_SCAN_TYPE_PASSIVE 1
 /* Maximum size of returned data */
 #define IW_SCAN_MAX_DATA	4096	/* In bytes */
 
 /* Max number of char in custom event - use multiple of them if needed */
 #define IW_CUSTOM_MAX		256	/* In bytes */
 
+/* Generic information element */
+#define IW_GENERIC_IE_MAX	1024
+
+/* MLME requests (SIOCSIWMLME / struct iw_mlme) */
+#define IW_MLME_DEAUTH		0
+#define IW_MLME_DISASSOC	1
+
+/* SIOCSIWAUTH/SIOCGIWAUTH struct iw_param flags */
+#define IW_AUTH_INDEX		0x0FFF
+#define IW_AUTH_FLAGS		0xF000
+/* SIOCSIWAUTH/SIOCGIWAUTH parameters (0 .. 4095)
+ * (IW_AUTH_INDEX mask in struct iw_param flags; this is the index of the
+ * parameter that is being set/get to; value will be read/written to
+ * struct iw_param value field) */
+#define IW_AUTH_WPA_VERSION		0
+#define IW_AUTH_CIPHER_PAIRWISE		1
+#define IW_AUTH_CIPHER_GROUP		2
+#define IW_AUTH_KEY_MGMT		3
+#define IW_AUTH_TKIP_COUNTERMEASURES	4
+#define IW_AUTH_DROP_UNENCRYPTED	5
+#define IW_AUTH_80211_AUTH_ALG		6
+#define IW_AUTH_WPA_ENABLED		7
+#define IW_AUTH_RX_UNENCRYPTED_EAPOL	8
+#define IW_AUTH_ROAMING_CONTROL		9
+#define IW_AUTH_PRIVACY_INVOKED		10
+
+/* IW_AUTH_WPA_VERSION values (bit field) */
+#define IW_AUTH_WPA_VERSION_DISABLED	0x00000001
+#define IW_AUTH_WPA_VERSION_WPA		0x00000002
+#define IW_AUTH_WPA_VERSION_WPA2	0x00000004
+
+/* IW_AUTH_PAIRWISE_CIPHER and IW_AUTH_GROUP_CIPHER values (bit field) */
+#define IW_AUTH_CIPHER_NONE	0x00000001
+#define IW_AUTH_CIPHER_WEP40	0x00000002
+#define IW_AUTH_CIPHER_TKIP	0x00000004
+#define IW_AUTH_CIPHER_CCMP	0x00000008
+#define IW_AUTH_CIPHER_WEP104	0x00000010
+
+/* IW_AUTH_KEY_MGMT values (bit field) */
+#define IW_AUTH_KEY_MGMT_802_1X	1
+#define IW_AUTH_KEY_MGMT_PSK	2
+
+/* IW_AUTH_80211_AUTH_ALG values (bit field) */
+#define IW_AUTH_ALG_OPEN_SYSTEM	0x00000001
+#define IW_AUTH_ALG_SHARED_KEY	0x00000002
+#define IW_AUTH_ALG_LEAP	0x00000004
+
+/* IW_AUTH_ROAMING_CONTROL values */
+#define IW_AUTH_ROAMING_ENABLE	0	/* driver/firmware based roaming */
+#define IW_AUTH_ROAMING_DISABLE	1	/* user space program used for roaming
+					 * control */
+
+/* SIOCSIWENCODEEXT definitions */
+#define IW_ENCODE_SEQ_MAX_SIZE	8
+/* struct iw_encode_ext ->alg */
+#define IW_ENCODE_ALG_NONE	0
+#define IW_ENCODE_ALG_WEP	1
+#define IW_ENCODE_ALG_TKIP	2
+#define IW_ENCODE_ALG_CCMP	3
+/* struct iw_encode_ext ->ext_flags */
+#define IW_ENCODE_EXT_TX_SEQ_VALID	0x00000001
+#define IW_ENCODE_EXT_RX_SEQ_VALID	0x00000002
+#define IW_ENCODE_EXT_GROUP_KEY		0x00000004
+#define IW_ENCODE_EXT_SET_TX_KEY	0x00000008
+
+/* IWEVMICHAELMICFAILURE : struct iw_michaelmicfailure ->flags */
+#define IW_MICFAILURE_KEY_ID	0x00000003 /* Key ID 0..3 */
+#define IW_MICFAILURE_GROUP	0x00000004
+#define IW_MICFAILURE_PAIRWISE	0x00000008
+#define IW_MICFAILURE_STAKEY	0x00000010
+#define IW_MICFAILURE_COUNT	0x00000060 /* 1 or 2 (0 = count not supported)
+					    */
+
+/* Bit field values for enc_capa in struct iw_range */
+#define IW_ENC_CAPA_WPA		0x00000001
+#define IW_ENC_CAPA_WPA2	0x00000002
+#define IW_ENC_CAPA_CIPHER_TKIP	0x00000004
+#define IW_ENC_CAPA_CIPHER_CCMP	0x00000008
+
+/* Event capability macros - in (struct iw_range *)->event_capa
+ * Because we have more than 32 possible events, we use an array of
+ * 32 bit bitmasks. Note : 32 bits = 0x20 = 2^5. */
+#define IW_EVENT_CAPA_BASE(cmd)		((cmd >= SIOCIWFIRSTPRIV) ? \
+					 (cmd - SIOCIWFIRSTPRIV + 0x60) : \
+					 (cmd - SIOCSIWCOMMIT))
+#define IW_EVENT_CAPA_INDEX(cmd)	(IW_EVENT_CAPA_BASE(cmd) >> 5)
+#define IW_EVENT_CAPA_MASK(cmd)		(1 << (IW_EVENT_CAPA_BASE(cmd) & 0x1F))
+/* Event capability constants - event autogenerated by the kernel
+ * This list is valid for most 802.11 devices, customise as needed... */
+#define IW_EVENT_CAPA_K_0	(IW_EVENT_CAPA_MASK(0x8B04) | \
+				 IW_EVENT_CAPA_MASK(0x8B06) | \
+				 IW_EVENT_CAPA_MASK(0x8B1A))
+#define IW_EVENT_CAPA_K_1	(IW_EVENT_CAPA_MASK(0x8B2A))
+/* "Easy" macro to set events in iw_range (less efficient) */
+#define IW_EVENT_CAPA_SET(event_capa, cmd) (event_capa[IW_EVENT_CAPA_INDEX(cmd)] |= IW_EVENT_CAPA_MASK(cmd))
+#define IW_EVENT_CAPA_SET_KERNEL(event_capa) {event_capa[0] |= IW_EVENT_CAPA_K_0; event_capa[1] |= IW_EVENT_CAPA_K_1; }
+
+
 /****************************** TYPES ******************************/
 
 /* --------------------------- SUBTYPES --------------------------- */
@@ -456,7 +644,7 @@
 	__s32		m;		/* Mantissa */
 	__s16		e;		/* Exponent */
 	__u8		i;		/* List index (when in range struct) */
-	__u8		pad;		/* Unused - just for alignement */
+	__u8		flags;		/* Flags (fixed/auto) */
 };
 
 /*
@@ -507,6 +695,132 @@
 	struct iw_quality	high;		/* High threshold */
 };
 
+/*
+ *	Optional data for scan request
+ *
+ *	Note: these optional parameters are controlling parameters for the
+ *	scanning behavior, these do not apply to getting scan results
+ *	(SIOCGIWSCAN). Drivers are expected to keep a local BSS table and
+ *	provide a merged results with all BSSes even if the previous scan
+ *	request limited scanning to a subset, e.g., by specifying an SSID.
+ *	Especially, scan results are required to include an entry for the
+ *	current BSS if the driver is in Managed mode and associated with an AP.
+ */
+struct	iw_scan_req
+{
+	__u8		scan_type; /* IW_SCAN_TYPE_{ACTIVE,PASSIVE} */
+	__u8		essid_len;
+	__u8		num_channels; /* num entries in channel_list;
+				       * 0 = scan all allowed channels */
+	__u8		flags; /* reserved as padding; use zero, this may
+				* be used in the future for adding flags
+				* to request different scan behavior */
+	struct sockaddr	bssid; /* ff:ff:ff:ff:ff:ff for broadcast BSSID or
+				* individual address of a specific BSS */
+
+	/*
+	 * Use this ESSID if IW_SCAN_THIS_ESSID flag is used instead of using
+	 * the current ESSID. This allows scan requests for specific ESSID
+	 * without having to change the current ESSID and potentially breaking
+	 * the current association.
+	 */
+	__u8		essid[IW_ESSID_MAX_SIZE];
+
+	/*
+	 * Optional parameters for changing the default scanning behavior.
+	 * These are based on the MLME-SCAN.request from IEEE Std 802.11.
+	 * TU is 1.024 ms. If these are set to 0, driver is expected to use
+	 * reasonable default values. min_channel_time defines the time that
+	 * will be used to wait for the first reply on each channel. If no
+	 * replies are received, next channel will be scanned after this. If
+	 * replies are received, total time waited on the channel is defined by
+	 * max_channel_time.
+	 */
+	__u32		min_channel_time; /* in TU */
+	__u32		max_channel_time; /* in TU */
+
+	struct iw_freq	channel_list[IW_MAX_FREQUENCIES];
+};
+
+/* ------------------------- WPA SUPPORT ------------------------- */
+
+/*
+ *	Extended data structure for get/set encoding (this is used with
+ *	SIOCSIWENCODEEXT/SIOCGIWENCODEEXT. struct iw_point and IW_ENCODE_*
+ *	flags are used in the same way as with SIOCSIWENCODE/SIOCGIWENCODE and
+ *	only the data contents changes (key data -> this structure, including
+ *	key data).
+ *
+ *	If the new key is the first group key, it will be set as the default
+ *	TX key. Otherwise, default TX key index is only changed if
+ *	IW_ENCODE_EXT_SET_TX_KEY flag is set.
+ *
+ *	Key will be changed with SIOCSIWENCODEEXT in all cases except for
+ *	special "change TX key index" operation which is indicated by setting
+ *	key_len = 0 and ext_flags |= IW_ENCODE_EXT_SET_TX_KEY.
+ *
+ *	tx_seq/rx_seq are only used when respective
+ *	IW_ENCODE_EXT_{TX,RX}_SEQ_VALID flag is set in ext_flags. Normal
+ *	TKIP/CCMP operation is to set RX seq with SIOCSIWENCODEEXT and start
+ *	TX seq from zero whenever key is changed. SIOCGIWENCODEEXT is normally
+ *	used only by an Authenticator (AP or an IBSS station) to get the
+ *	current TX sequence number. Using TX_SEQ_VALID for SIOCSIWENCODEEXT and
+ *	RX_SEQ_VALID for SIOCGIWENCODEEXT are optional, but can be useful for
+ *	debugging/testing.
+ */
+struct	iw_encode_ext
+{
+	__u32		ext_flags; /* IW_ENCODE_EXT_* */
+	__u8		tx_seq[IW_ENCODE_SEQ_MAX_SIZE]; /* LSB first */
+	__u8		rx_seq[IW_ENCODE_SEQ_MAX_SIZE]; /* LSB first */
+	struct sockaddr	addr; /* ff:ff:ff:ff:ff:ff for broadcast/multicast
+			       * (group) keys or unicast address for
+			       * individual keys */
+	__u16		alg; /* IW_ENCODE_ALG_* */
+	__u16		key_len;
+	__u8		key[0];
+};
+
+/* SIOCSIWMLME data */
+struct	iw_mlme
+{
+	__u16		cmd; /* IW_MLME_* */
+	__u16		reason_code;
+	struct sockaddr	addr;
+};
+
+/* SIOCSIWPMKSA data */
+#define IW_PMKSA_ADD		1
+#define IW_PMKSA_REMOVE		2
+#define IW_PMKSA_FLUSH		3
+
+#define IW_PMKID_LEN	16
+
+struct	iw_pmksa
+{
+	__u32		cmd; /* IW_PMKSA_* */
+	struct sockaddr	bssid;
+	__u8		pmkid[IW_PMKID_LEN];
+};
+
+/* IWEVMICHAELMICFAILURE data */
+struct	iw_michaelmicfailure
+{
+	__u32		flags;
+	struct sockaddr	src_addr;
+	__u8		tsc[IW_ENCODE_SEQ_MAX_SIZE]; /* LSB first */
+};
+
+/* IWEVPMKIDCAND data */
+#define IW_PMKID_CAND_PREAUTH	0x00000001 /* RNS pre-authentication enabled */
+struct	iw_pmkid_cand
+{
+	__u32		flags; /* IW_PMKID_CAND_* */
+	__u32		index; /* the smaller the index, the higher the
+				* priority */
+	struct sockaddr	bssid;
+};
+
 /* ------------------------ WIRELESS STATS ------------------------ */
 /*
  * Wireless statistics (used for /proc/net/wireless)
@@ -610,11 +924,12 @@
 	/* Old Frequency (backward compat - moved lower ) */
 	__u16		old_num_channels;
 	__u8		old_num_frequency;
-	/* Filler to keep "version" at the same offset */
-	__s32		old_freq[6];
+
+	/* Wireless event capability bitmasks */
+	__u32		event_capa[6];
 
 	/* signal level threshold range */
-	__s32	sensitivity;
+	__s32		sensitivity;
 
 	/* Quality of link & SNR stuff */
 	/* Quality range (link, level, noise)
@@ -685,6 +1000,8 @@
 	struct iw_freq	freq[IW_MAX_FREQUENCIES];	/* list */
 	/* Note : this frequency list doesn't need to fit channel numbers,
 	 * because each entry contain its channel index */
+
+	__u32		enc_capa; /* IW_ENC_CAPA_* bit field */
 };
 
 /*
diff -Nur linux-2.4.32/include/net/iw_handler.h linux-2.4.32-we/include/net/iw_handler.h
--- linux-2.4.32/include/net/iw_handler.h	2003-11-28 19:26:21.000000000 +0100
+++ linux-2.4.32-we/include/net/iw_handler.h	2006-03-13 12:10:57.000000000 +0100
@@ -1,10 +1,10 @@
 /*
  * This file define the new driver API for Wireless Extensions
  *
- * Version :	5	4.12.02
+ * Version :	6	21.6.04
  *
  * Authors :	Jean Tourrilhes - HPL - <jt@hpl.hp.com>
- * Copyright (c) 2001-2002 Jean Tourrilhes, All Rights Reserved.
+ * Copyright (c) 2001-2004 Jean Tourrilhes, All Rights Reserved.
  */
 
 #ifndef _IW_HANDLER_H
@@ -206,7 +206,7 @@
  * will be needed...
  * I just plan to increment with each new version.
  */
-#define IW_HANDLER_VERSION	5
+#define IW_HANDLER_VERSION	6
 
 /*
  * Changes :
@@ -224,11 +224,18 @@
  * V4 to V5
  * --------
  *	- Add new spy support : struct iw_spy_data & prototypes
+ *
+ * V5 to V6
+ * --------
+ *	- Change the way we get to spy_data method for added safety
+ *	- Remove spy #ifdef, they are always on -> cleaner code
+ *	- Add IW_DESCR_FLAG_NOMAX flag for very large requests
+ *	- Start migrating get_wireless_stats to struct iw_handler_def
  */
 
 /**************************** CONSTANTS ****************************/
 
-/* Enable enhanced spy support. Disable to reduce footprint */
+/* Enhanced spy support available */
 #define IW_WIRELESS_SPY
 #define IW_WIRELESS_THRSPY
 
@@ -258,6 +265,7 @@
 #define IW_DESCR_FLAG_EVENT	0x0002	/* Generate an event on SET */
 #define IW_DESCR_FLAG_RESTRICT	0x0004	/* GET : request is ROOT only */
 				/* SET : Omit payload from generated iwevent */
+#define IW_DESCR_FLAG_NOMAX	0x0008	/* GET : no limit on request size */
 /* Driver level flags */
 #define IW_DESCR_FLAG_WAIT	0x0100	/* Wait for driver event */
 
@@ -311,23 +319,25 @@
 	/* Array of handlers for standard ioctls
 	 * We will call dev->wireless_handlers->standard[ioctl - SIOCSIWNAME]
 	 */
-	iw_handler *		standard;
+	const iw_handler *	standard;
 
 	/* Array of handlers for private ioctls
 	 * Will call dev->wireless_handlers->private[ioctl - SIOCIWFIRSTPRIV]
 	 */
-	iw_handler *		private;
+	const iw_handler *	private;
 
 	/* Arguments of private handler. This one is just a list, so you
 	 * can put it in any order you want and should not leave holes...
 	 * We will automatically export that to user space... */
-	struct iw_priv_args *	private_args;
+	const struct iw_priv_args *	private_args;
 
-	/* Driver enhanced spy support */
-	long			spy_offset;	/* Spy data offset */
+	/* This field will be *removed* in the next version of WE */
+	long			spy_offset;	/* DO NOT USE */
 
-	/* In the long term, get_wireless_stats will move from
-	 * 'struct net_device' to here, to minimise bloat. */
+	/* New location of get_wireless_stats, to de-bloat struct net_device.
+	 * The old pointer in struct net_device will be gradually phased
+	 * out, and drivers are encouraged to use this one... */
+	struct iw_statistics*	(*get_wireless_stats)(struct net_device *dev);
 };
 
 /* ---------------------- IOCTL DESCRIPTION ---------------------- */
@@ -374,18 +384,29 @@
  */
 struct iw_spy_data
 {
-#ifdef IW_WIRELESS_SPY
 	/* --- Standard spy support --- */
 	int			spy_number;
 	u_char			spy_address[IW_MAX_SPY][ETH_ALEN];
 	struct iw_quality	spy_stat[IW_MAX_SPY];
-#ifdef IW_WIRELESS_THRSPY
 	/* --- Enhanced spy support (event) */
 	struct iw_quality	spy_thr_low;	/* Low threshold */
 	struct iw_quality	spy_thr_high;	/* High threshold */
 	u_char			spy_thr_under[IW_MAX_SPY];
-#endif /* IW_WIRELESS_THRSPY */
-#endif /* IW_WIRELESS_SPY */
+};
+
+/* --------------------- DEVICE WIRELESS DATA --------------------- */
+/*
+ * This is all the wireless data specific to a device instance that
+ * is managed by the core of Wireless Extensions.
+ * We only keep pointer to those structures, so that a driver is free
+ * to share them between instances.
+ * This structure should be initialised before registering the device.
+ * Access to this data follow the same rules as any other struct net_device
+ * data (i.e. valid as long as struct net_device exist, same locking rules).
+ */
+struct iw_public_data {
+	/* Driver enhanced spy support */
+	struct iw_spy_data *	spy_data;
 };
 
 /**************************** PROTOTYPES ****************************/
diff -Nur linux-2.4.32/net/core/dev.c linux-2.4.32-we/net/core/dev.c
--- linux-2.4.32/net/core/dev.c	2005-04-04 03:42:20.000000000 +0200
+++ linux-2.4.32-we/net/core/dev.c	2006-03-13 12:10:57.000000000 +0100
@@ -2426,7 +2426,7 @@
 				/* Follow me in net/core/wireless.c */
 				ret = wireless_process_ioctl(&ifr, cmd);
 				rtnl_unlock();
-				if (!ret && IW_IS_GET(cmd) &&
+				if (IW_IS_GET(cmd) &&
 				    copy_to_user(arg, &ifr, sizeof(struct ifreq)))
 					return -EFAULT;
 				return ret;
diff -Nur linux-2.4.32/net/core/wireless.c linux-2.4.32-we/net/core/wireless.c
--- linux-2.4.32/net/core/wireless.c	2003-11-28 19:26:21.000000000 +0100
+++ linux-2.4.32-we/net/core/wireless.c	2006-03-13 12:11:02.000000000 +0100
@@ -2,7 +2,7 @@
  * This file implement the Wireless Extensions APIs.
  *
  * Authors :	Jean Tourrilhes - HPL - <jt@hpl.hp.com>
- * Copyright (c) 1997-2003 Jean Tourrilhes, All Rights Reserved.
+ * Copyright (c) 1997-2005 Jean Tourrilhes, All Rights Reserved.
  *
  * (As all part of the Linux kernel, this file is GPL)
  */
@@ -48,6 +48,16 @@
  *	o Add common spy support : iw_handler_set_spy(), wireless_spy_update()
  *	o Add enhanced spy support : iw_handler_set_thrspy() and event.
  *	o Add WIRELESS_EXT version display in /proc/net/wireless
+ *
+ * v6 - 18.06.04 - Jean II
+ *	o Change get_spydata() method for added safety
+ *	o Remove spy #ifdef, they are always on -> cleaner code
+ *	o Allow any size GET request if user specifies length > max
+ *		and if request has IW_DESCR_FLAG_NOMAX flag or is SIOCGIWPRIV
+ *	o Start migrating get_wireless_stats to struct iw_handler_def
+ *	o Add wmb() in iw_handler_set_spy() for non-coherent archs/cpus
+ * Based on patch from Pavel Roskin <proski@gnu.org> :
+ *	o Fix kernel data leak to user space in private handler handling
  */
 
 /***************************** INCLUDES *****************************/
@@ -64,11 +74,7 @@
 
 /**************************** CONSTANTS ****************************/
 
-/* Enough lenience, let's make sure things are proper... */
-#define WE_STRICT_WRITE		/* Check write buffer size */
-/* I'll probably drop both the define and kernel message in the next version */
-
-/* Debuging stuff */
+/* Debugging stuff */
 #undef WE_IOCTL_DEBUG		/* Debug IOCTL API */
 #undef WE_EVENT_DEBUG		/* Debug Event dispatcher */
 #undef WE_SPY_DEBUG		/* Debug enhanced spy support */
@@ -131,14 +137,14 @@
 	{ IW_HEADER_TYPE_ADDR, 0, 0, 0, 0, 0},
 	/* SIOCGIWAP */
 	{ IW_HEADER_TYPE_ADDR, 0, 0, 0, 0, IW_DESCR_FLAG_DUMP},
-	/* -- hole -- */
-	{ IW_HEADER_TYPE_NULL, 0, 0, 0, 0, 0},
+	/* SIOCSIWMLME */
+	{ IW_HEADER_TYPE_POINT, 0, 1, sizeof(struct iw_mlme), sizeof(struct iw_mlme), 0},
 	/* SIOCGIWAPLIST */
-	{ IW_HEADER_TYPE_POINT, 0, (sizeof(struct sockaddr) + sizeof(struct iw_quality)), 0, IW_MAX_AP, 0},
+	{ IW_HEADER_TYPE_POINT, 0, (sizeof(struct sockaddr) + sizeof(struct iw_quality)), 0, IW_MAX_AP, IW_DESCR_FLAG_NOMAX},
 	/* SIOCSIWSCAN */
-	{ IW_HEADER_TYPE_PARAM, 0, 0, 0, 0, 0},
+	{ IW_HEADER_TYPE_POINT, 0, 1, 0, sizeof(struct iw_scan_req), 0},
 	/* SIOCGIWSCAN */
-	{ IW_HEADER_TYPE_POINT, 0, 1, 0, IW_SCAN_MAX_DATA, 0},
+	{ IW_HEADER_TYPE_POINT, 0, 1, 0, IW_SCAN_MAX_DATA, IW_DESCR_FLAG_NOMAX},
 	/* SIOCSIWESSID */
 	{ IW_HEADER_TYPE_POINT, 0, 1, 0, IW_ESSID_MAX_SIZE + 1, IW_DESCR_FLAG_EVENT},
 	/* SIOCGIWESSID */
@@ -179,6 +185,25 @@
 	{ IW_HEADER_TYPE_PARAM, 0, 0, 0, 0, 0},
 	/* SIOCGIWPOWER */
 	{ IW_HEADER_TYPE_PARAM, 0, 0, 0, 0, 0},
+	/* -- hole -- */
+	{ IW_HEADER_TYPE_NULL, 0, 0, 0, 0, 0},
+	/* -- hole -- */
+	{ IW_HEADER_TYPE_NULL, 0, 0, 0, 0, 0},
+	/* SIOCSIWGENIE */
+	{ IW_HEADER_TYPE_POINT, 0, 1, 0, IW_GENERIC_IE_MAX, 0},
+	/* SIOCGIWGENIE */
+	{ IW_HEADER_TYPE_POINT, 0, 1, 0, IW_GENERIC_IE_MAX, 0},
+	/* SIOCSIWAUTH */
+	{ IW_HEADER_TYPE_PARAM, 0, 0, 0, 0, 0},
+	/* SIOCGIWAUTH */
+	{ IW_HEADER_TYPE_PARAM, 0, 0, 0, 0, 0},
+	/* SIOCSIWENCODEEXT */
+	{ IW_HEADER_TYPE_POINT, 0, 1, sizeof(struct iw_encode_ext), sizeof(struct iw_encode_ext) + IW_ENCODING_TOKEN_MAX, 0},
+	/* SIOCGIWENCODEEXT */
+	{ IW_HEADER_TYPE_POINT, 0, 1, sizeof(struct iw_encode_ext), sizeof(struct iw_encode_ext) + IW_ENCODING_TOKEN_MAX, 0},
+	/* SIOCSIWPMKSA */
+	{ IW_HEADER_TYPE_POINT, 0, 1, sizeof(struct iw_pmksa), sizeof(struct iw_pmksa), 0},
+	/* -- hole -- */
 };
 static const int standard_ioctl_num = (sizeof(standard_ioctl) /
 				       sizeof(struct iw_ioctl_description));
@@ -198,12 +223,22 @@
 	{ IW_HEADER_TYPE_ADDR, 0, 0, 0, 0, 0},
 	/* IWEVEXPIRED */
 	{ IW_HEADER_TYPE_ADDR, 0, 0, 0, 0, 0},
+	/* IWEVGENIE */
+	{ IW_HEADER_TYPE_POINT, 0, 1, 0, IW_GENERIC_IE_MAX, 0},
+	/* IWEVMICHAELMICFAILURE */
+	{ IW_HEADER_TYPE_POINT, 0, 1, 0, sizeof(struct iw_michaelmicfailure), 0},
+	/* IWEVASSOCREQIE */
+	{ IW_HEADER_TYPE_POINT, 0, 1, 0, IW_GENERIC_IE_MAX, 0},
+	/* IWEVASSOCRESPIE */
+	{ IW_HEADER_TYPE_POINT, 0, 1, 0, IW_GENERIC_IE_MAX, 0},
+	/* IWEVPMKIDCAND */
+	{ IW_HEADER_TYPE_POINT, 0, 1, 0, sizeof(struct iw_pmkid_cand), 0},
 };
 static const int standard_event_num = (sizeof(standard_event) /
 				       sizeof(struct iw_ioctl_description));
 
 /* Size (in bytes) of the various private data types */
-static const char priv_type_size[] = {
+static const char iw_priv_type_size[] = {
 	0,				/* IW_PRIV_TYPE_NONE */
 	1,				/* IW_PRIV_TYPE_BYTE */
 	1,				/* IW_PRIV_TYPE_CHAR */
@@ -270,12 +305,15 @@
  */
 static inline struct iw_statistics *get_wireless_stats(struct net_device *dev)
 {
+	/* New location */
+	if((dev->wireless_handlers != NULL) &&
+	   (dev->wireless_handlers->get_wireless_stats != NULL))
+		return dev->wireless_handlers->get_wireless_stats(dev);
+
+	/* Old location, will be phased out in next WE */
 	return (dev->get_wireless_stats ?
 		dev->get_wireless_stats(dev) :
 		(struct iw_statistics *) NULL);
-	/* In the future, get_wireless_stats may move from 'struct net_device'
-	 * to 'struct iw_handler_def', to de-bloat struct net_device.
-	 * Definitely worse a thought... */
 }
 
 /* ---------------------------------------------------------------- */
@@ -310,14 +348,32 @@
 
 /* ---------------------------------------------------------------- */
 /*
- * Number of private arguments
+ * Calculate size of private arguments
  */
 static inline int get_priv_size(__u16	args)
 {
 	int	num = args & IW_PRIV_SIZE_MASK;
 	int	type = (args & IW_PRIV_TYPE_MASK) >> 12;
 
-	return num * priv_type_size[type];
+	return num * iw_priv_type_size[type];
+}
+
+/* ---------------------------------------------------------------- */
+/*
+ * Re-calculate the size of private arguments
+ */
+static inline int adjust_priv_size(__u16		args,
+				   union iwreq_data *	wrqu)
+{
+	int	num = wrqu->data.length;
+	int	max = args & IW_PRIV_SIZE_MASK;
+	int	type = (args & IW_PRIV_TYPE_MASK) >> 12;
+
+	/* Make sure the driver doesn't goof up */
+	if (max < num)
+		num = max;
+
+	return num * iw_priv_type_size[type];
 }
 
 
@@ -350,11 +406,14 @@
 			       dev->name,
 			       stats->status,
 			       stats->qual.qual,
-			       stats->qual.updated & 1 ? '.' : ' ',
+			       stats->qual.updated & IW_QUAL_QUAL_UPDATED
+			       ? '.' : ' ',
 			       ((__u8) stats->qual.level),
-			       stats->qual.updated & 2 ? '.' : ' ',
+			       stats->qual.updated & IW_QUAL_LEVEL_UPDATED
+			       ? '.' : ' ',
 			       ((__u8) stats->qual.noise),
-			       stats->qual.updated & 4 ? '.' : ' ',
+			       stats->qual.updated & IW_QUAL_NOISE_UPDATED
+			       ? '.' : ' ',
 			       stats->discard.nwid,
 			       stats->discard.code,
 			       stats->discard.fragment,
@@ -470,13 +529,15 @@
 	/* Check NULL pointer */
 	if(iwr->u.data.pointer == NULL)
 		return -EFAULT;
-#ifdef WE_STRICT_WRITE
+
 	/* Check if there is enough buffer up there */
 	if(iwr->u.data.length < dev->wireless_handlers->num_private_args) {
-		printk(KERN_ERR "%s (WE) : Buffer for request SIOCGIWPRIV too small (%d<%d)\n", dev->name, iwr->u.data.length, dev->wireless_handlers->num_private_args);
+		/* User space can't know in advance how large the buffer
+		 * needs to be. Give it a hint, so that we can support
+		 * any size buffer we want somewhat efficiently... */
+		iwr->u.data.length = dev->wireless_handlers->num_private_args;
 		return -E2BIG;
 	}
-#endif	/* WE_STRICT_WRITE */
 
 	/* Set the number of available ioctls. */
 	iwr->u.data.length = dev->wireless_handlers->num_private_args;
@@ -505,7 +566,6 @@
 	const struct iw_ioctl_description *	descr;
 	struct iw_request_info			info;
 	int					ret = -EINVAL;
-	int					user_size = 0;
 
 	/* Get the description of the IOCTL */
 	if((cmd - SIOCIWFIRST) >= standard_ioctl_num)
@@ -536,8 +596,14 @@
 #endif	/* WE_SET_EVENT */
 	} else {
 		char *	extra;
+		int	extra_size;
+		int	user_length = 0;
 		int	err;
 
+		/* Calculate space needed by arguments. Always allocate
+		 * for max space. Easier, and won't last long... */
+		extra_size = descr->max_tokens * descr->token_size;
+
 		/* Check what user space is giving us */
 		if(IW_IS_SET(cmd)) {
 			/* Check NULL pointer */
@@ -554,18 +620,33 @@
 			if(iwr->u.data.pointer == NULL)
 				return -EFAULT;
 			/* Save user space buffer size for checking */
-			user_size = iwr->u.data.length;
+			user_length = iwr->u.data.length;
+
+			/* Don't check if user_length > max to allow forward
+			 * compatibility. The test user_length < min is
+			 * implied by the test at the end. */
+
+			/* Support for very large requests */
+			if((descr->flags & IW_DESCR_FLAG_NOMAX) &&
+			   (user_length > descr->max_tokens)) {
+				/* Allow userspace to GET more than max so
+				 * we can support any size GET requests.
+				 * There is still a limit : -ENOMEM. */
+				extra_size = user_length * descr->token_size;
+				/* Note : user_length is originally a __u16,
+				 * and token_size is controlled by us,
+				 * so extra_size won't get negative and
+				 * won't overflow... */
+			}
 		}
 
 #ifdef WE_IOCTL_DEBUG
 		printk(KERN_DEBUG "%s (WE) : Malloc %d bytes\n",
-		       dev->name, descr->max_tokens * descr->token_size);
+		       dev->name, extra_size);
 #endif	/* WE_IOCTL_DEBUG */
 
-		/* Always allocate for max space. Easier, and won't last
-		 * long... */
-		extra = kmalloc(descr->max_tokens * descr->token_size,
-				GFP_KERNEL);
+		/* Create the kernel buffer */
+		extra = kmalloc(extra_size, GFP_KERNEL);
 		if (extra == NULL) {
 			return -ENOMEM;
 		}
@@ -591,14 +672,11 @@
 
 		/* If we have something to return to the user */
 		if (!ret && IW_IS_GET(cmd)) {
-#ifdef WE_STRICT_WRITE
 			/* Check if there is enough buffer up there */
-			if(user_size < iwr->u.data.length) {
-				printk(KERN_ERR "%s (WE) : Buffer for request %04X too small (%d<%d)\n", dev->name, cmd, user_size, iwr->u.data.length);
+			if(user_length < iwr->u.data.length) {
 				kfree(extra);
 				return -E2BIG;
 			}
-#endif	/* WE_STRICT_WRITE */
 
 			err = copy_to_user(iwr->u.data.pointer, extra,
 					   iwr->u.data.length *
@@ -661,7 +739,7 @@
 				     iw_handler		handler)
 {
 	struct iwreq *			iwr = (struct iwreq *) ifr;
-	struct iw_priv_args *		descr = NULL;
+	const struct iw_priv_args *	descr = NULL;
 	struct iw_request_info		info;
 	int				extra_size = 0;
 	int				i;
@@ -701,7 +779,7 @@
 			   ((extra_size + offset) <= IFNAMSIZ))
 				extra_size = 0;
 		} else {
-			/* Size of set arguments */
+			/* Size of get arguments */
 			extra_size = get_priv_size(descr->get_args);
 
 			/* Does it fits in iwr ? */
@@ -771,6 +849,14 @@
 
 		/* If we have something to return to the user */
 		if (!ret && IW_IS_GET(cmd)) {
+
+			/* Adjust for the actual length if it's variable,
+			 * avoid leaking kernel bits outside. */
+			if (!(descr->get_args & IW_PRIV_SIZE_FIXED)) {
+				extra_size = adjust_priv_size(descr->get_args,
+							      &(iwr->u));
+			}
+
 			err = copy_to_user(iwr->u.data.pointer, extra,
 					   extra_size);
 			if (err)
@@ -1042,9 +1128,25 @@
  * One of the main advantage of centralising spy support here is that
  * it becomes much easier to improve and extend it without having to touch
  * the drivers. One example is the addition of the Spy-Threshold events.
- * Note : IW_WIRELESS_SPY is defined in iw_handler.h
  */
 
+/* ---------------------------------------------------------------- */
+/*
+ * Return the pointer to the spy data in the driver.
+ * Because this is called on the Rx path via wireless_spy_update(),
+ * we want it to be efficient...
+ */
+static inline struct iw_spy_data * get_spydata(struct net_device *dev)
+{
+	/* This is the new way */
+	if(dev->wireless_data)
+		return(dev->wireless_data->spy_data);
+
+	/* This is the old way. Doesn't work for multi-headed drivers.
+	 * It will be removed in the next version of WE. */
+	return (dev->priv + dev->wireless_handlers->spy_offset);
+}
+
 /*------------------------------------------------------------------*/
 /*
  * Standard Wireless Handler : set Spy List
@@ -1054,16 +1156,26 @@
 		       union iwreq_data *	wrqu,
 		       char *			extra)
 {
-#ifdef IW_WIRELESS_SPY
-	struct iw_spy_data *	spydata = (dev->priv +
-					   dev->wireless_handlers->spy_offset);
+	struct iw_spy_data *	spydata = get_spydata(dev);
 	struct sockaddr *	address = (struct sockaddr *) extra;
 
+	/* Make sure driver is not buggy or using the old API */
+	if(!spydata)
+		return -EOPNOTSUPP;
+
 	/* Disable spy collection while we copy the addresses.
-	 * As we don't disable interrupts, we need to do this to avoid races.
-	 * As we are the only writer, this is good enough. */
+	 * While we copy addresses, any call to wireless_spy_update()
+	 * will NOP. This is OK, as anyway the addresses are changing. */
 	spydata->spy_number = 0;
 
+	/* We want to operate without locking, because wireless_spy_update()
+	 * most likely will happen in the interrupt handler, and therefore
+	 * have its own locking constraints and needs performance.
+	 * The rtnl_lock() make sure we don't race with the other iw_handlers.
+	 * This make sure wireless_spy_update() "see" that the spy list
+	 * is temporarily disabled. */
+	wmb();
+
 	/* Are there are addresses to copy? */
 	if(wrqu->data.length > 0) {
 		int i;
@@ -1089,13 +1201,14 @@
 			       spydata->spy_address[i][5]);
 #endif	/* WE_SPY_DEBUG */
 	}
+
+	/* Make sure above is updated before re-enabling */
+	wmb();
+
 	/* Enable addresses */
 	spydata->spy_number = wrqu->data.length;
 
 	return 0;
-#else /* IW_WIRELESS_SPY */
-	return -EOPNOTSUPP;
-#endif /* IW_WIRELESS_SPY */
 }
 
 /*------------------------------------------------------------------*/
@@ -1107,12 +1220,14 @@
 		       union iwreq_data *	wrqu,
 		       char *			extra)
 {
-#ifdef IW_WIRELESS_SPY
-	struct iw_spy_data *	spydata = (dev->priv +
-					   dev->wireless_handlers->spy_offset);
+	struct iw_spy_data *	spydata = get_spydata(dev);
 	struct sockaddr *	address = (struct sockaddr *) extra;
 	int			i;
 
+	/* Make sure driver is not buggy or using the old API */
+	if(!spydata)
+		return -EOPNOTSUPP;
+
 	wrqu->data.length = spydata->spy_number;
 
 	/* Copy addresses. */
@@ -1129,9 +1244,6 @@
 	for(i = 0; i < spydata->spy_number; i++)
 		spydata->spy_stat[i].updated = 0;
 	return 0;
-#else /* IW_WIRELESS_SPY */
-	return -EOPNOTSUPP;
-#endif /* IW_WIRELESS_SPY */
 }
 
 /*------------------------------------------------------------------*/
@@ -1143,11 +1255,13 @@
 			  union iwreq_data *	wrqu,
 			  char *		extra)
 {
-#ifdef IW_WIRELESS_THRSPY
-	struct iw_spy_data *	spydata = (dev->priv +
-					   dev->wireless_handlers->spy_offset);
+	struct iw_spy_data *	spydata = get_spydata(dev);
 	struct iw_thrspy *	threshold = (struct iw_thrspy *) extra;
 
+	/* Make sure driver is not buggy or using the old API */
+	if(!spydata)
+		return -EOPNOTSUPP;
+
 	/* Just do it */
 	memcpy(&(spydata->spy_thr_low), &(threshold->low),
 	       2 * sizeof(struct iw_quality));
@@ -1160,9 +1274,6 @@
 #endif	/* WE_SPY_DEBUG */
 
 	return 0;
-#else /* IW_WIRELESS_THRSPY */
-	return -EOPNOTSUPP;
-#endif /* IW_WIRELESS_THRSPY */
 }
 
 /*------------------------------------------------------------------*/
@@ -1174,22 +1285,20 @@
 			  union iwreq_data *	wrqu,
 			  char *		extra)
 {
-#ifdef IW_WIRELESS_THRSPY
-	struct iw_spy_data *	spydata = (dev->priv +
-					   dev->wireless_handlers->spy_offset);
+	struct iw_spy_data *	spydata = get_spydata(dev);
 	struct iw_thrspy *	threshold = (struct iw_thrspy *) extra;
 
+	/* Make sure driver is not buggy or using the old API */
+	if(!spydata)
+		return -EOPNOTSUPP;
+
 	/* Just do it */
 	memcpy(&(threshold->low), &(spydata->spy_thr_low),
 	       2 * sizeof(struct iw_quality));
 
 	return 0;
-#else /* IW_WIRELESS_THRSPY */
-	return -EOPNOTSUPP;
-#endif /* IW_WIRELESS_THRSPY */
 }
 
-#ifdef IW_WIRELESS_THRSPY
 /*------------------------------------------------------------------*/
 /*
  * Prepare and send a Spy Threshold event
@@ -1227,7 +1336,6 @@
 	/* Send event to user space */
 	wireless_send_event(dev, SIOCGIWTHRSPY, &wrqu, (char *) &threshold);
 }
-#endif /* IW_WIRELESS_THRSPY */
 
 /* ---------------------------------------------------------------- */
 /*
@@ -1240,12 +1348,14 @@
 			 unsigned char *	address,
 			 struct iw_quality *	wstats)
 {
-#ifdef IW_WIRELESS_SPY
-	struct iw_spy_data *	spydata = (dev->priv +
-					   dev->wireless_handlers->spy_offset);
+	struct iw_spy_data *	spydata = get_spydata(dev);
 	int			i;
 	int			match = -1;
 
+	/* Make sure driver is not buggy or using the old API */
+	if(!spydata)
+		return;
+
 #ifdef WE_SPY_DEBUG
 	printk(KERN_DEBUG "wireless_spy_update() :  offset %ld, spydata %p, address %02X:%02X:%02X:%02X:%02X:%02X\n", dev->wireless_handlers->spy_offset, spydata, address[0], address[1], address[2], address[3], address[4], address[5]);
 #endif	/* WE_SPY_DEBUG */
@@ -1257,7 +1367,7 @@
 			       sizeof(struct iw_quality));
 			match = i;
 		}
-#ifdef IW_WIRELESS_THRSPY
+
 	/* Generate an event if we cross the spy threshold.
 	 * To avoid event storms, we have a simple hysteresis : we generate
 	 * event only when we go under the low threshold or above the
@@ -1277,6 +1387,4 @@
 			}
 		}
 	}
-#endif /* IW_WIRELESS_THRSPY */
-#endif /* IW_WIRELESS_SPY */
 }
