diff -Nur linux-2.6.19.2/drivers/mtd/Kconfig.old linux-2.6.19.2/drivers/mtd/Kconfig
--- linux-2.6.19.2/drivers/mtd/Kconfig.old	2007-03-25 08:13:02.000000000 +0200
+++ linux-2.6.19.2/drivers/mtd/Kconfig	2007-03-26 13:37:47.000000000 +0200
@@ -157,6 +157,22 @@
 	  for your particular device. It won't happen automatically. The
 	  'armflash' map driver (CONFIG_MTD_ARMFLASH) does this, for example.
 
+config MTD_MYLOADER_PARTS
+	tristate "MyLoader partition parsing"
+	depends on MIPS_ADM5120 && MTD_PARTITIONS
+	---help---
+	  MyLoader is a bootloader which allows the user to define partitions
+	  in flash devices, by putting a table in the second erase block
+	  on the device, similar to a partition table. This table gives the 
+	  offsets and lengths of the user defined partitions.
+
+	  If you need code which can detect and parse these tables, and
+	  register MTD 'partitions' corresponding to each image detected,
+	  enable this option.
+
+	  You will still need the parsing functions to be called by the driver
+	  for your particular device. It won't happen automatically.
+
 comment "User Modules And Translation Layers"
 	depends on MTD
 
diff -Nur linux-2.6.19.2/drivers/mtd/Makefile.old linux-2.6.19.2/drivers/mtd/Makefile
--- linux-2.6.19.2/drivers/mtd/Makefile.old	2007-01-10 20:10:37.000000000 +0100
+++ linux-2.6.19.2/drivers/mtd/Makefile	2007-03-26 13:28:23.000000000 +0200
@@ -12,6 +12,7 @@
 obj-$(CONFIG_MTD_REDBOOT_PARTS) += redboot.o
 obj-$(CONFIG_MTD_CMDLINE_PARTS) += cmdlinepart.o
 obj-$(CONFIG_MTD_AFS_PARTS)	+= afs.o
+obj-$(CONFIG_MTD_MYLOADER_PARTS) += myloader.o
 
 # 'Users' - code which presents functionality to userspace.
 obj-$(CONFIG_MTD_CHAR)		+= mtdchar.o
