diff -Nur linux-2.6.15/arch/mips/pci/fixup-aruba.c linux-2.6.15-openwrt/arch/mips/pci/fixup-aruba.c
--- linux-2.6.15/arch/mips/pci/fixup-aruba.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.15-openwrt/arch/mips/pci/fixup-aruba.c	2006-01-10 00:34:41.000000000 +0100
@@ -0,0 +1,115 @@
+/**************************************************************************
+ *
+ *  BRIEF MODULE DESCRIPTION
+ *     PCI fixups for IDT EB434 board
+ *
+ *  Copyright 2004 IDT Inc. (rischelp@idt.com)
+ *         
+ *  This program is free software; you can redistribute  it and/or modify it
+ *  under  the terms of  the GNU General  Public License as published by the
+ *  Free Software Foundation;  either version 2 of the  License, or (at your
+ *  option) any later version.
+ *
+ *  THIS  SOFTWARE  IS PROVIDED   ``AS  IS'' AND   ANY  EXPRESS OR IMPLIED
+ *  WARRANTIES,   INCLUDING, BUT NOT  LIMITED  TO, THE IMPLIED WARRANTIES OF
+ *  MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN
+ *  NO  EVENT  SHALL   THE AUTHOR  BE    LIABLE FOR ANY   DIRECT, INDIRECT,
+ *  INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ *  NOT LIMITED   TO, PROCUREMENT OF  SUBSTITUTE GOODS  OR SERVICES; LOSS OF
+ *  USE, DATA,  OR PROFITS; OR  BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ *  ANY THEORY OF LIABILITY, WHETHER IN  CONTRACT, STRICT LIABILITY, OR TORT
+ *  (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ *  THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ *  You should have received a copy of the  GNU General Public License along
+ *  with this program; if not, write  to the Free Software Foundation, Inc.,
+ *  675 Mass Ave, Cambridge, MA 02139, USA.
+ *
+ *
+ **************************************************************************
+ * May 2004 rkt, neb
+ *
+ * Initial Release
+ *
+ * 
+ *
+ **************************************************************************
+ */
+
+#include <linux/autoconf.h>
+#include <linux/types.h>
+#include <linux/pci.h>
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <asm/idt-boards/rc32434/rc32434.h>
+#include <asm/idt-boards/rc32434/rc32434_pci.h> 
+
+int __init pcibios_map_irq(struct pci_dev *dev, u8 slot, u8 pin)
+{
+	
+	if (dev->bus->number != 0) {
+		return 0;
+	}
+	
+	slot = PCI_SLOT(dev->devfn);
+	dev->irq = 0;
+	
+	if (slot > 0 && slot <= 15) {
+#if 1
+		if(slot == 10) {
+			if(pin == 1) dev->irq = GROUP4_IRQ_BASE + 9; // intA
+		} else if(slot == 11) {
+			if(pin == 1) dev->irq = GROUP4_IRQ_BASE + 10; // intA
+			if(pin == 2) dev->irq = GROUP4_IRQ_BASE + 10; // intA
+			if(pin == 3) dev->irq = GROUP4_IRQ_BASE + 10; // intA
+		} else if(slot == 12) {
+			if(pin == 1) dev->irq = GROUP4_IRQ_BASE + 11; // intA
+			if(pin == 2) dev->irq = GROUP4_IRQ_BASE + 12; // intB
+		} else if (slot == 13) {
+			if(pin == 1) dev->irq = GROUP4_IRQ_BASE + 12; // intA
+			if(pin == 2) dev->irq = GROUP4_IRQ_BASE + 11; // intB
+		} else {
+			dev->irq = GROUP4_IRQ_BASE + 11;
+		}
+#else
+                                switch (pin) {
+                                case 1: /* INTA*/
+                                        dev->irq = GROUP4_IRQ_BASE + 11;
+                                        break;
+                                case 2: /* INTB */
+                                        dev->irq = GROUP4_IRQ_BASE + 11;
+                                        break;
+                                case 3: /* INTC */
+                                        dev->irq = GROUP4_IRQ_BASE + 11;
+                                        break;
+                                case 4: /* INTD */
+                                        dev->irq = GROUP4_IRQ_BASE + 11;
+                                        break;
+                                default:
+                                        dev->irq = 0xff;
+                                        break;
+                                }
+#endif
+#ifdef DEBUG
+		printk("irq fixup: slot %d, pin %d, irq %d\n",
+		       slot, pin, dev->irq);
+#endif
+		pci_write_config_byte(dev, PCI_INTERRUPT_LINE,dev->irq);
+	}
+	return (dev->irq);
+}
+
+struct pci_fixup pcibios_fixups[] = {
+	{0}
+};
+
+
+
+
+
+
+
+
+
+
+
diff -Nur linux-2.6.15/arch/mips/pci/Makefile linux-2.6.15-openwrt/arch/mips/pci/Makefile
--- linux-2.6.15/arch/mips/pci/Makefile	2006-01-03 04:21:10.000000000 +0100
+++ linux-2.6.15-openwrt/arch/mips/pci/Makefile	2006-01-10 00:32:32.000000000 +0100
@@ -53,3 +53,4 @@
 obj-$(CONFIG_VICTOR_MPC30X)	+= fixup-mpc30x.o
 obj-$(CONFIG_ZAO_CAPCELLA)	+= fixup-capcella.o
 obj-$(CONFIG_WR_PPMC)		+= fixup-wrppmc.o
+obj-$(CONFIG_MACH_ARUBA)        += fixup-aruba.o ops-aruba.o pci-aruba.o
diff -Nur linux-2.6.15/arch/mips/pci/ops-aruba.c linux-2.6.15-openwrt/arch/mips/pci/ops-aruba.c
--- linux-2.6.15/arch/mips/pci/ops-aruba.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.15-openwrt/arch/mips/pci/ops-aruba.c	2006-01-10 00:32:32.000000000 +0100
@@ -0,0 +1,204 @@
+/**************************************************************************
+ *
+ *  BRIEF MODULE DESCRIPTION
+ *     pci_ops for IDT EB434 board
+ *
+ *  Copyright 2004 IDT Inc. (rischelp@idt.com)
+ *         
+ *  This program is free software; you can redistribute  it and/or modify it
+ *  under  the terms of  the GNU General  Public License as published by the
+ *  Free Software Foundation;  either version 2 of the  License, or (at your
+ *  option) any later version.
+ *
+ *  THIS  SOFTWARE  IS PROVIDED   ``AS  IS'' AND   ANY  EXPRESS OR IMPLIED
+ *  WARRANTIES,   INCLUDING, BUT NOT  LIMITED  TO, THE IMPLIED WARRANTIES OF
+ *  MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN
+ *  NO  EVENT  SHALL   THE AUTHOR  BE    LIABLE FOR ANY   DIRECT, INDIRECT,
+ *  INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ *  NOT LIMITED   TO, PROCUREMENT OF  SUBSTITUTE GOODS  OR SERVICES; LOSS OF
+ *  USE, DATA,  OR PROFITS; OR  BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ *  ANY THEORY OF LIABILITY, WHETHER IN  CONTRACT, STRICT LIABILITY, OR TORT
+ *  (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ *  THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ *  You should have received a copy of the  GNU General Public License along
+ *  with this program; if not, write  to the Free Software Foundation, Inc.,
+ *  675 Mass Ave, Cambridge, MA 02139, USA.
+ *
+ *
+ **************************************************************************
+ * May 2004 rkt, neb
+ *
+ * Initial Release
+ *
+ * 
+ *
+ **************************************************************************
+ */
+
+#include <linux/autoconf.h>
+#include <linux/init.h>
+#include <linux/pci.h>
+#include <linux/types.h>
+#include <linux/delay.h>
+
+#include <asm/cpu.h>
+#include <asm/io.h>
+
+#include <asm/idt-boards/rc32434/rc32434.h>
+#include <asm/idt-boards/rc32434/rc32434_pci.h>
+
+#define PCI_ACCESS_READ  0
+#define PCI_ACCESS_WRITE 1
+
+
+#define PCI_CFG_SET(slot,func,off) \
+	(rc32434_pci->pcicfga = (0x80000000 | ((slot)<<11) | \
+			    ((func)<<8) | (off)))
+
+static int config_access(unsigned char access_type, struct pci_bus *bus,
+                         unsigned int devfn, unsigned char where,
+                         u32 * data)
+{ 
+	/*
+	 * config cycles are on 4 byte boundary only
+	 */
+	unsigned int slot = PCI_SLOT(devfn);
+	u8 func = PCI_FUNC(devfn);
+	
+	if (slot < 2 || slot > 15) {
+		*data = 0xFFFFFFFF;
+		return -1;
+	}
+	/* Setup address */
+	PCI_CFG_SET(slot, func, where);
+	rc32434_sync();
+	
+	if (access_type == PCI_ACCESS_WRITE) {
+		rc32434_sync();	
+		rc32434_pci->pcicfgd = *data;
+	} else {
+		rc32434_sync();	
+		*data = rc32434_pci->pcicfgd;
+	}
+	
+	rc32434_sync();
+	
+	return 0;
+}
+
+
+/*
+ * We can't address 8 and 16 bit words directly.  Instead we have to
+ * read/write a 32bit word and mask/modify the data we actually want.
+ */
+static int read_config_byte(struct pci_bus *bus, unsigned int devfn,
+                            int where, u8 * val)
+{
+	u32 data;
+	int ret;
+	
+	ret = config_access(PCI_ACCESS_READ, bus, devfn, where, &data);
+	*val = (data >> ((where & 3) << 3)) & 0xff;
+	return ret;
+}
+
+static int read_config_word(struct pci_bus *bus, unsigned int devfn,
+                            int where, u16 * val)
+{
+	u32 data;
+	int ret;
+	
+	ret = config_access(PCI_ACCESS_READ, bus, devfn, where, &data);
+	*val = (data >> ((where & 3) << 3)) & 0xffff;
+	return ret;
+}
+
+static int read_config_dword(struct pci_bus *bus, unsigned int devfn,
+                             int where, u32 * val)
+{
+	int ret;
+	
+	ret = config_access(PCI_ACCESS_READ, bus, devfn, where, val);
+	return ret;
+}
+
+static int
+write_config_byte(struct pci_bus *bus, unsigned int devfn, int where,
+                  u8 val)
+{
+	u32 data = 0;
+	
+	if (config_access(PCI_ACCESS_READ, bus, devfn, where, &data))
+		return -1;
+	
+	data = (data & ~(0xff << ((where & 3) << 3))) |
+		(val << ((where & 3) << 3));
+	
+	if (config_access(PCI_ACCESS_WRITE, bus, devfn, where, &data))
+		return -1;
+	
+	return PCIBIOS_SUCCESSFUL;
+}
+
+
+static int
+write_config_word(struct pci_bus *bus, unsigned int devfn, int where,
+                  u16 val)
+{
+	u32 data = 0;
+	
+	if (config_access(PCI_ACCESS_READ, bus, devfn, where, &data))
+		return -1;
+	
+	data = (data & ~(0xffff << ((where & 3) << 3))) |
+		(val << ((where & 3) << 3));
+	
+	if (config_access(PCI_ACCESS_WRITE, bus, devfn, where, &data))
+		return -1;
+	
+	
+	return PCIBIOS_SUCCESSFUL;
+}
+
+
+static int 
+write_config_dword(struct pci_bus *bus, unsigned int devfn, int where,
+                   u32 val)
+{
+	if (config_access(PCI_ACCESS_WRITE, bus, devfn, where, &val))
+		return -1;
+	
+	return PCIBIOS_SUCCESSFUL;
+}
+
+static int pci_config_read(struct pci_bus *bus, unsigned int devfn,
+			   int where, int size, u32 * val)
+{
+	switch (size) {
+	case 1: 
+		return read_config_byte(bus, devfn, where, (u8 *) val);
+	case 2: 
+		return read_config_word(bus, devfn, where, (u16 *) val);
+	default:
+		return read_config_dword(bus, devfn, where, val);
+	}
+}
+
+static int pci_config_write(struct pci_bus *bus, unsigned int devfn,
+			    int where, int size, u32 val)
+{
+	switch (size) {
+	case 1: 
+		return write_config_byte(bus, devfn, where, (u8) val);
+	case 2: 
+		return write_config_word(bus, devfn, where, (u16) val);
+	default:
+		return write_config_dword(bus, devfn, where, val);
+	}
+}
+
+struct pci_ops rc32434_pci_ops = {
+	.read =  pci_config_read,
+	.write = pci_config_write,
+};
diff -Nur linux-2.6.15/arch/mips/pci/pci-aruba.c linux-2.6.15-openwrt/arch/mips/pci/pci-aruba.c
--- linux-2.6.15/arch/mips/pci/pci-aruba.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.15-openwrt/arch/mips/pci/pci-aruba.c	2006-01-10 00:32:32.000000000 +0100
@@ -0,0 +1,235 @@
+/**************************************************************************
+ *
+ *  BRIEF MODULE DESCRIPTION
+ *     PCI initialization for IDT EB434 board
+ *
+ *  Copyright 2004 IDT Inc. (rischelp@idt.com)
+ *         
+ *  This program is free software; you can redistribute  it and/or modify it
+ *  under  the terms of  the GNU General  Public License as published by the
+ *  Free Software Foundation;  either version 2 of the  License, or (at your
+ *  option) any later version.
+ *
+ *  THIS  SOFTWARE  IS PROVIDED   ``AS  IS'' AND   ANY  EXPRESS OR IMPLIED
+ *  WARRANTIES,   INCLUDING, BUT NOT  LIMITED  TO, THE IMPLIED WARRANTIES OF
+ *  MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN
+ *  NO  EVENT  SHALL   THE AUTHOR  BE    LIABLE FOR ANY   DIRECT, INDIRECT,
+ *  INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ *  NOT LIMITED   TO, PROCUREMENT OF  SUBSTITUTE GOODS  OR SERVICES; LOSS OF
+ *  USE, DATA,  OR PROFITS; OR  BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ *  ANY THEORY OF LIABILITY, WHETHER IN  CONTRACT, STRICT LIABILITY, OR TORT
+ *  (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ *  THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ *  You should have received a copy of the  GNU General Public License along
+ *  with this program; if not, write  to the Free Software Foundation, Inc.,
+ *  675 Mass Ave, Cambridge, MA 02139, USA.
+ *
+ *
+ **************************************************************************
+ * May 2004 rkt, neb
+ *
+ * Initial Release
+ *
+ * 
+ *
+ **************************************************************************
+ */
+
+#include <linux/autoconf.h>
+#include <linux/types.h>
+#include <linux/pci.h>
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <asm/idt-boards/rc32434/rc32434.h>
+#include <asm/idt-boards/rc32434/rc32434_pci.h> 
+
+#define PCI_ACCESS_READ  0
+#define PCI_ACCESS_WRITE 1
+
+#undef DEBUG
+#ifdef DEBUG
+#define DBG(x...) printk(x)
+#else
+#define DBG(x...)
+#endif
+/* define an unsigned array for the PCI registers */
+unsigned int korinaCnfgRegs[25] = {
+	KORINA_CNFG1,	 KORINA_CNFG2,  KORINA_CNFG3,  KORINA_CNFG4,
+	KORINA_CNFG5,	 KORINA_CNFG6,  KORINA_CNFG7,  KORINA_CNFG8,
+	KORINA_CNFG9,	 KORINA_CNFG10, KORINA_CNFG11, KORINA_CNFG12,
+	KORINA_CNFG13, KORINA_CNFG14, KORINA_CNFG15, KORINA_CNFG16,
+	KORINA_CNFG17, KORINA_CNFG18, KORINA_CNFG19, KORINA_CNFG20,
+	KORINA_CNFG21, KORINA_CNFG22, KORINA_CNFG23, KORINA_CNFG24
+};
+
+static struct resource rc32434_res_pci_mem2;
+
+static struct resource rc32434_res_pci_mem1 = {
+	.name = "PCI MEM1",
+	.start = 0x50000000,
+	.end = 0x5FFFFFFF,
+	.flags = IORESOURCE_MEM,
+	.child = &rc32434_res_pci_mem2,
+};
+static struct resource rc32434_res_pci_mem2 = {
+	.name = "PCI MEM2",
+	.start = 0x60000000,
+	.end = 0x6FFFFFFF,
+	.flags = IORESOURCE_MEM,
+	.parent = &rc32434_res_pci_mem1,
+};
+static struct resource rc32434_res_pci_io1 = {
+	.name = "PCI I/O1",
+	.start = 0x18800000,
+	.end = 0x188FFFFF,
+	.flags = IORESOURCE_IO,
+};
+
+extern struct pci_ops rc32434_pci_ops;
+
+struct pci_controller rc32434_controller = {
+	.pci_ops = &rc32434_pci_ops,
+	.mem_resource = &rc32434_res_pci_mem1,
+	.io_resource = &rc32434_res_pci_io1,
+	.mem_offset     = 0x00000000UL,
+	.io_offset      = 0x00000000UL,
+};
+
+extern unsigned int arch_has_pci;
+
+static int __init rc32434_pcibridge_init(void)
+{
+	
+	unsigned int pciConfigAddr = 0;/*used for writing pci config values */
+	int	     loopCount=0    ;/*used for the loop */
+	
+	unsigned int pcicValue, pcicData=0;
+	unsigned int dummyRead, pciCntlVal = 0;
+
+	if (!arch_has_pci) return 0;
+
+	printk("PCI: Initializing PCI\n");
+	
+	/* Disable the IP bus error for PCI scaning */
+	pciCntlVal=rc32434_pci->pcic;
+	pciCntlVal &= 0xFFFFFF7;
+	rc32434_pci->pcic = pciCntlVal;
+	
+	ioport_resource.start = rc32434_res_pci_io1.start;
+	ioport_resource.end = rc32434_res_pci_io1.end;
+/*
+	iomem_resource.start = rc32434_res_pci_mem1.start;
+	iomem_resource.end = rc32434_res_pci_mem1.end;
+*/
+	
+	pcicValue = rc32434_pci->pcic;
+	pcicValue = (pcicValue >> PCIM_SHFT) & PCIM_BIT_LEN;
+	if (!((pcicValue == PCIM_H_EA) ||
+	      (pcicValue == PCIM_H_IA_FIX) ||
+	      (pcicValue == PCIM_H_IA_RR))) {
+		/* Not in Host Mode, return ERROR */
+		return -1;
+	}
+	
+	/* Enables the Idle Grant mode, Arbiter Parking */
+	pcicData |=(PCIC_igm_m|PCIC_eap_m|PCIC_en_m);
+	rc32434_pci->pcic = pcicData; /* Enable the PCI bus Interface */
+	/* Zero out the PCI status & PCI Status Mask */
+	for(;;) {
+		pcicData = rc32434_pci->pcis;
+		if (!(pcicData & PCIS_rip_m))
+			break;
+	}
+	
+	rc32434_pci->pcis = 0;
+	rc32434_pci->pcism = 0xFFFFFFFF;
+	/* Zero out the PCI decoupled registers */
+	rc32434_pci->pcidac=0; /* disable PCI decoupled accesses at initialization */
+	rc32434_pci->pcidas=0; /* clear the status */
+	rc32434_pci->pcidasm=0x0000007F; /* Mask all the interrupts */
+	/* Mask PCI Messaging Interrupts */
+	rc32434_pci_msg->pciiic = 0;
+	rc32434_pci_msg->pciiim = 0xFFFFFFFF;
+	rc32434_pci_msg->pciioic = 0;
+	rc32434_pci_msg->pciioim = 0;
+	
+	/* Setup PCILB0 as Memory Window */
+	rc32434_pci->pcilba[0].a = (unsigned int) (PCI_ADDR_START);
+	
+	/* setup the PCI map address as same as the local address */
+	
+	rc32434_pci->pcilba[0].m = (unsigned int) (PCI_ADDR_START);
+	
+	/* Setup PCILBA1 as MEM */
+#ifdef __MIPSEB__
+	rc32434_pci->pcilba[0].c = ( ((SIZE_16MB & 0x1f) << PCILBAC_size_b) | PCILBAC_sb_m);
+#else
+	rc32434_pci->pcilba[0].c = ( ((SIZE_16MB & 0x1f) << PCILBAC_size_b));
+#endif
+	dummyRead = rc32434_pci->pcilba[0].c; /* flush the CPU write Buffers */
+	
+	rc32434_pci->pcilba[1].a = 0x60000000;
+	
+	rc32434_pci->pcilba[1].m = 0x60000000;
+	/* setup PCILBA2 as IO Window*/
+#ifdef __MIPSEB__
+	rc32434_pci->pcilba[1].c = ( ((SIZE_256MB & 0x1f) << PCILBAC_size_b) |  PCILBAC_sb_m);
+#else
+	rc32434_pci->pcilba[1].c = ((SIZE_256MB & 0x1f) << PCILBAC_size_b);
+#endif
+	dummyRead = rc32434_pci->pcilba[1].c; /* flush the CPU write Buffers */
+	rc32434_pci->pcilba[2].a = 0x18C00000;
+	
+	rc32434_pci->pcilba[2].m = 0x18FFFFFF;
+	/* setup PCILBA2 as IO Window*/
+#ifdef __MIPSEB__
+	rc32434_pci->pcilba[2].c = ( ((SIZE_4MB & 0x1f) << PCILBAC_size_b)  |  PCILBAC_sb_m);
+#else
+	rc32434_pci->pcilba[2].c = ((SIZE_4MB & 0x1f) << PCILBAC_size_b);
+#endif  
+	
+	dummyRead = rc32434_pci->pcilba[2].c; /* flush the CPU write Buffers */
+	
+	
+	rc32434_pci->pcilba[3].a = 0x18800000;
+	
+	rc32434_pci->pcilba[3].m = 0x18800000;
+	/* Setup PCILBA3 as IO Window */
+	
+#ifdef __MIPSEB__
+	rc32434_pci->pcilba[3].c = ( (((SIZE_1MB & 0x1ff) << PCILBAC_size_b) | PCILBAC_msi_m)   |  PCILBAC_sb_m);
+#else
+	rc32434_pci->pcilba[3].c = (((SIZE_1MB & 0x1ff) << PCILBAC_size_b) | PCILBAC_msi_m);
+#endif
+	dummyRead = rc32434_pci->pcilba[2].c; /* flush the CPU write Buffers */
+	
+	pciConfigAddr = (unsigned int)(0x80000004);
+	for(loopCount = 0; loopCount < 24; loopCount++){
+		rc32434_pci->pcicfga = pciConfigAddr;
+		dummyRead = rc32434_pci->pcicfga;
+		rc32434_pci->pcicfgd = korinaCnfgRegs[loopCount];
+		dummyRead=rc32434_pci->pcicfgd;
+		pciConfigAddr += 4;
+	}
+	rc32434_pci->pcitc=(unsigned int)((PCITC_RTIMER_VAL&0xff) << PCITC_rtimer_b) |
+		((PCITC_DTIMER_VAL&0xff)<<PCITC_dtimer_b);
+	
+	pciCntlVal = rc32434_pci->pcic;
+	pciCntlVal &= ~(PCIC_tnr_m);
+	rc32434_pci->pcic = pciCntlVal;
+	pciCntlVal = rc32434_pci->pcic;
+	
+	register_pci_controller(&rc32434_controller);
+	
+	rc32434_sync();  
+	return 0;
+}
+
+arch_initcall(rc32434_pcibridge_init);
+
+/* Do platform specific device initialization at pci_enable_device() time */
+int pcibios_plat_dev_init(struct pci_dev *dev)
+{
+        return 0;
+}
diff -Nur linux-2.6.15/drivers/pci/access.c linux-2.6.15-openwrt/drivers/pci/access.c
--- linux-2.6.15/drivers/pci/access.c	2006-01-03 04:21:10.000000000 +0100
+++ linux-2.6.15-openwrt/drivers/pci/access.c	2006-01-10 00:43:10.000000000 +0100
@@ -21,6 +21,7 @@
 #define PCI_word_BAD (pos & 1)
 #define PCI_dword_BAD (pos & 3)
 
+#ifdef __MIPSEB__
 #define PCI_OP_READ(size,type,len) \
 int pci_bus_read_config_##size \
 	(struct pci_bus *bus, unsigned int devfn, int pos, type *value)	\
@@ -31,11 +32,32 @@
 	if (PCI_##size##_BAD) return PCIBIOS_BAD_REGISTER_NUMBER;	\
 	spin_lock_irqsave(&pci_lock, flags);				\
 	res = bus->ops->read(bus, devfn, pos, len, &data);		\
+	if (len == 1)							\
+	 *value = (type)((data >> 24) & 0xff);				\
+	 else if (len == 2)						\
+	 *value = (type)((data >> 16) & 0xffff);			\
+	else								\
 	*value = (type)data;						\
 	spin_unlock_irqrestore(&pci_lock, flags);			\
 	return res;							\
 }
+#else
 
+#define PCI_OP_READ(size,type,len) \
+int pci_bus_read_config_##size \
+	(struct pci_bus *bus, unsigned int devfn, int pos, type *value) \
+{									\
+	int res;							\
+	unsigned long flags;						\
+	u32 data = 0;							\
+	if (PCI_##size##_BAD) return PCIBIOS_BAD_REGISTER_NUMBER;	\
+	spin_lock_irqsave(&pci_lock, flags);				\
+	res = bus->ops->read(bus, devfn, pos, len, &data);		\
+	*value = (type)data;						\
+	spin_unlock_irqrestore(&pci_lock, flags);			\
+	return res;							\
+}
+#endif
 #define PCI_OP_WRITE(size,type,len) \
 int pci_bus_write_config_##size \
 	(struct pci_bus *bus, unsigned int devfn, int pos, type value)	\
