/dts-v1/;

#include "danube.dtsi"

#include <dt-bindings/input/input.h>

/ {
	compatible = "arcadyan,arv8539pw22", "lantiq,xway", "lantiq,danube";
	model = "Speedport W 504V Typ A";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_green;

		led-dsl = &dsl_green;
		led-internet = &online_green;
		led-wifi = &wireless_green;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		wlan {
			label = "wlan";
			gpios = <&gpio 29 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
		reset {
			label = "reset";
			gpios = <&gpio 30 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
		/* key DECT is missing */
	};

	leds {
		compatible = "gpio-leds";

		power_green: power-green {
			label = "arv8539pw22:green:power";
			gpios = <&gpio 24 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		power_red: power-red {
			label = "arv8539pw22:red:power";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		dsl_green: dsl-green {
			label = "arv8539pw22:green:dsl";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};

		online_green: online-green {
			label = "arv8539pw22:green:online";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};

		wireless_green: wireless-green {
			label = "arv8539pw22:green:wlan";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
		/*
			telefonie green is missing
		*/
	};

	usb_vbus: regulator-usb-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpio = <&gpio 14 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		pci_rst {
			lantiq,pins = "io21";
			lantiq,pull = <2>;
			lantiq,output = <1>;
		};
		relay {
			lantiq,pins = "io31";
			lantiq,output = <1>;
		};
	};
};

&gsw {
	phy-mode = "mii";
	mtd-mac-address = <&art 0x16>;
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x800000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x00000 0x30000>;	/* 192 KiB */
				read-only;
			};

			partition@30000 {
				label = "uboot";
				reg = <0x30000 0x10000>;	/* 64 KiB */
				read-only;
			};

			partition@40000 {
				label = "firmware";
				reg = <0x40000 0x7b0000>;       /* 7872 KiB */
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x10000>;       /* 64 KiB*/
				read-only;
			};
		};
	};
};

&pci0 {
	status = "okay";

	pinctrl-0 = <&pci_gnt1_pins>, <&pci_req1_pins>;
	pinctrl-names = "default";

	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;

	wifi@168c,0029 {
		compatible = "pci168c,0029";
		reg = <0x7000 0 0 0 0>;
		qca,no-eeprom; /* load from ath9k-eeprom-pci-0000:00:0e.0.bin */
		mtd-mac-address = <&art 0x16>;
		mtd-mac-address-increment = <1>;
	};
};

&usb_phy {
	status = "okay";
};

&usb {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};

&vmmc {
	status = "okay";
	gpios = <&gpio 31 GPIO_ACTIVE_HIGH>;
};
