From 794b9e55c77bf0ef34dfdb3b151a845c004b3ce3 Mon Sep 17 00:00:00 2001
From: Li Yang <leoyang.li@nxp.com>
Date: Thu, 2 May 2019 16:01:01 -0500
Subject: [PATCH] arm64: dts: ls1043a: accumulated change for ls1043a boards

commit 118e2f48ee8da3f5547c24888bd6fdb78f03b7ce
Author: Peng Ma <peng.ma@nxp.com>
Date:   Wed Jul 25 08:53:07 2018 +0000

    dts: fsl-ls1021a, fsl-ls1043a, fsl-ls1046a: add multi block node
support

    add block-offset to support different virtual block offset for qdma
    base on soc;
    the interrupt named "qdma-queueN(N:0,1,2,3)" correspond to a virtual
    block,N based on block number of qdma;

    Signed-off-by: Peng Ma <peng.ma@nxp.com>

Author: Zhang Ying-22455 <ying.zhang22455@nxp.com>
Date:   Mon Apr 2 16:22:40 2018 +0800

    arm64: dts: ls1043a: add dts entry for A-010650

    Signed-off-by: Zhang Ying-22455 <ying.zhang22455@nxp.com>

commit a47e4bd0b5d076feb6d81601c16d5b79e53a92c8
Author: Rajesh Bhagat <rajesh.bhagat@freescale.com>
Date:   Wed Jan 27 11:37:25 2016 +0530

    arm64: dts: ls1043a: Add configure-gfladj property to USB3 node

    Add "configure-gfladj" boolean property to USB3 node. This property
    is used to determine whether frame length adjustent is required
    or not

    Signed-off-by: Rajesh Bhagat <rajesh.bhagat@nxp.com>
    Signed-off-by: Ran Wang <ran.wang_1@nxp.com>

commit 38566bbd5ca6747b30d2f0c251bbcfe0723df8c6
Author: Changming Huang <jerry.huang@nxp.com>
Date:   Wed Apr 19 12:49:50 2017 +0800

    arm/arm64: dts: Add property snps incr burst type adjustment for
INCR burst type for dwc3

    Signed-off-by: yinbo.zhu <yinbo.zhu@nxp.com>
    Signed-off-by: Ran Wang <ran.wang_1@nxp.com>

commit 8632d84e0fe187aa023a24f0dad0040c53e12450
Author: Abhimanyu Saini <abhimanyu.saini@nxp.com>
Date:   Thu Jan 25 11:31:13 2018 +0530

    arm64: dts: freescale: ls1043a: Modify DT nodes for qspi

    Signed-off-by: Abhimanyu Saini <abhimanyu.saini@nxp.com>

commit b1dc1ebed79e9aaab75fd06837d794ec2f1b624d
Author: Ran Wang <ran.wang_1@nxp.com>
Date:   Fri Jan 5 15:14:48 2018 +0800

    arm64: dts: ls1043a: Enable usb3-lpm-capable for usb3 node

    Enable USB3 HW LPM feature for ls1043a and active patch for
    snps erratum A-010131. It will disable U1/U2 temperary when
    initiate U3 request.

    Signed-off-by: Ran Wang <ran.wang_1@nxp.com>

commit 9b17a5fcf8da5656ff99ebef3d63ba040e9f676d
Author: Zhang Ying-22455 <ying.zhang22455@nxp.com>
Date:   Tue Jun 13 13:14:26 2017 +0800

    arm64: dts: correct the register range of dcfg

    Signed-off-by: Zhang Ying-22455 <ying.zhang22455@nxp.com>

commit f60e39fd51ad702e3a2613faaca40871a4763735
Author: Zhang Ying-22455 <ying.zhang22455@nxp.com>
Date:   Tue Aug 22 18:04:02 2017 +0800

    arm64: dts: ls1043a: add pcf85263 rtc nodes

    Signed-off-by: Zhang Ying-22455 <ying.zhang22455@nxp.com>

commit 67c82e3c7b376139d7cee624589bedbc311f8868
Author: jiaheng.fan <jiaheng.fan@nxp.com>
Date:   Thu May 11 17:36:33 2017 +0800

    arm64: dts: ls1021/ls1043/ls1046: add qdma nodes
    Signed-off-by: jiaheng.fan <jiaheng.fan@nxp.com>

commit c6d9c2498ee83669f9853100301edff9a5905caf
Author: Wang Dongsheng <dongsheng.wang@nxp.com>
Date:   Fri Apr 21 13:26:07 2017 +0800

    arm64: dts: ls1043a: add ftm0 nodes

    Add rcpm and ftm0 nodes. The Power Management related features
    need these nodes.

    Signed-off-by: Zhang Ying-22455 <ying.zhang22455@nxp.com>

commit 3bcdc4de0a1c9e6f4a4ddc916e8efe8044d8bbfd
Author: Po Liu <po.liu@nxp.com>
Date:   Fri Sep 30 17:11:36 2016 +0800

    arm64: dts: ls1043/ls2080: add pcie aer/pme interrupt-name property

    Some platforms(NXP Layerscape for example) aer/pme interrupts was
not
    MSI/MSI-X/INTx but using interrupt line independently. This patch
    add "aer", "pme" interrupt-names for aer/pme interrupt.

    With the interrupt-names "aer", "pme" code could probe aer/pme
interrupt
    line for pcie root port, replace the aer/pme interrupt service irqs.

    This is intend to fixup the Layerscape platforms which aer/pmes
interrupts
    was not MSI/MSI-X/INTx, but using interrupt line independently.

    Since the interrupt-names "intr" never been used. Remove it.

    Signed-off-by: Po Liu <po.liu@nxp.com>
    Signed-off-by: Hou Zhiqiang <Zhiqiang.Hou@nxp.com>

commit 4d20ecf029f1255520b30c103e1724c618b981c7
Author: Zhao Qiang <qiang.zhao@nxp.com>
Date:   Sun Jun 12 15:51:44 2016 +0800

    arm64: dts: ls1043ardb: add ds26522 node

    add ds26522 node to fsl-ls1043a-rdb.dts

    Signed-off-by: Zhao Qiang <qiang.zhao@nxp.com>

commit ca470562646ab058814fc4a1195016fb3266cdf5
Author: Zhao Qiang <qiang.zhao@nxp.com>
Date:   Sun Jun 12 15:44:11 2016 +0800

    arm64: dts: ls1043ardb: add qe node

    Signed-off-by: Zhao Qiang <qiang.zhao@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1043a-qds.dts | 162 ++++++++++++++++++++++
 arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts |  36 +++++
 arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi    | 108 +++++++++++++--
 3 files changed, 295 insertions(+), 11 deletions(-)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a-qds.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a-qds.dts
@@ -24,6 +24,22 @@
 		serial1 = &duart1;
 		serial2 = &duart2;
 		serial3 = &duart3;
+		sgmii_riser_s1_p1 = &sgmii_phy_s1_p1;
+		sgmii_riser_s2_p1 = &sgmii_phy_s2_p1;
+		sgmii_riser_s3_p1 = &sgmii_phy_s3_p1;
+		sgmii_riser_s4_p1 = &sgmii_phy_s4_p1;
+		qsgmii_s1_p1 = &qsgmii_phy_s1_p1;
+		qsgmii_s1_p2 = &qsgmii_phy_s1_p2;
+		qsgmii_s1_p3 = &qsgmii_phy_s1_p3;
+		qsgmii_s1_p4 = &qsgmii_phy_s1_p4;
+		qsgmii_s2_p1 = &qsgmii_phy_s2_p1;
+		qsgmii_s2_p2 = &qsgmii_phy_s2_p2;
+		qsgmii_s2_p3 = &qsgmii_phy_s2_p3;
+		qsgmii_s2_p4 = &qsgmii_phy_s2_p4;
+		emi1_slot1 = &ls1043mdio_s1;
+		emi1_slot2 = &ls1043mdio_s2;
+		emi1_slot3 = &ls1043mdio_s3;
+		emi1_slot4 = &ls1043mdio_s4;
 	};
 
 	chosen {
@@ -64,6 +80,8 @@
 	fpga: board-control@2,0 {
 		compatible = "fsl,ls1043aqds-fpga", "fsl,fpga-qixis";
 		reg = <0x2 0x0 0x0000100>;
+		#address-cells = <1>;
+		#size-cells = <1>;
 	};
 };
 
@@ -149,3 +167,147 @@
 };
 
 #include "fsl-ls1043-post.dtsi"
+
+&fman0 {
+	ethernet@e0000 {
+		phy-handle = <&qsgmii_phy_s2_p1>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@e2000 {
+		phy-handle = <&qsgmii_phy_s2_p2>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@e4000 {
+		phy-handle = <&rgmii_phy1>;
+		phy-connection-type = "rgmii";
+	};
+
+	ethernet@e6000 {
+		phy-handle = <&rgmii_phy2>;
+		phy-connection-type = "rgmii";
+	};
+
+	ethernet@e8000 {
+		phy-handle = <&qsgmii_phy_s2_p3>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@ea000 {
+		phy-handle = <&qsgmii_phy_s2_p4>;
+		phy-connection-type = "sgmii";
+	};
+
+	ethernet@f0000 { /* DTSEC9/10GEC1 */
+		fixed-link = <1 1 10000 0 0>;
+		phy-connection-type = "xgmii";
+	};
+};
+
+&fpga {
+	mdio-mux-emi1 {
+		compatible = "mdio-mux-mmioreg", "mdio-mux";
+		mdio-parent-bus = <&mdio0>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0x54 1>;    /* BRDCFG4 */
+		mux-mask = <0xe0>; /* EMI1 */
+
+		/* On-board RGMII1 PHY */
+		ls1043mdio0: mdio@0 {
+			reg = <0>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			rgmii_phy1: ethernet-phy@1 { /* MAC3 */
+				reg = <0x1>;
+			};
+		};
+
+		/* On-board RGMII2 PHY */
+		ls1043mdio1: mdio@1 {
+			reg = <0x20>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			rgmii_phy2: ethernet-phy@2 { /* MAC4 */
+				reg = <0x2>;
+			};
+		};
+
+		/* Slot 1 */
+		ls1043mdio_s1: mdio@2 {
+			reg = <0x40>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			qsgmii_phy_s1_p1: ethernet-phy@4 {
+				reg = <0x4>;
+			};
+			qsgmii_phy_s1_p2: ethernet-phy@5 {
+				reg = <0x5>;
+			};
+			qsgmii_phy_s1_p3: ethernet-phy@6 {
+				reg = <0x6>;
+			};
+			qsgmii_phy_s1_p4: ethernet-phy@7 {
+				reg = <0x7>;
+			};
+
+			sgmii_phy_s1_p1: ethernet-phy@1c {
+				reg = <0x1c>;
+			};
+		};
+
+		/* Slot 2 */
+		ls1043mdio_s2: mdio@3 {
+			reg = <0x60>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			qsgmii_phy_s2_p1: ethernet-phy@8 {
+				reg = <0x8>;
+			};
+			qsgmii_phy_s2_p2: ethernet-phy@9 {
+				reg = <0x9>;
+			};
+			qsgmii_phy_s2_p3: ethernet-phy@a {
+				reg = <0xa>;
+			};
+			qsgmii_phy_s2_p4: ethernet-phy@b {
+				reg = <0xb>;
+			};
+
+			sgmii_phy_s2_p1: ethernet-phy@1c {
+				reg = <0x1c>;
+			};
+		};
+
+		/* Slot 3 */
+		ls1043mdio_s3: mdio@4 {
+			reg = <0x80>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			sgmii_phy_s3_p1: ethernet-phy@1c {
+				reg = <0x1c>;
+			};
+		};
+
+		/* Slot 4 */
+		ls1043mdio_s4: mdio@5 {
+			reg = <0xa0>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			sgmii_phy_s4_p1: ethernet-phy@1c {
+				reg = <0x1c>;
+			};
+		};
+	};
+};
--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts
@@ -49,6 +49,10 @@
 		compatible = "pericom,pt7c4338";
 		reg = <0x68>;
 	};
+	rtc@51 {
+		compatible = "nxp,pcf85263";
+		reg = <0x51>;
+	};
 };
 
 &ifc {
@@ -94,6 +98,38 @@
 		reg = <0>;
 		spi-max-frequency = <1000000>; /* input clock */
 	};
+
+	slic@2 {
+		compatible = "maxim,ds26522";
+		reg = <2>;
+		spi-max-frequency = <2000000>;
+		fsl,spi-cs-sck-delay = <100>;
+		fsl,spi-sck-cs-delay = <50>;
+	};
+
+	slic@3 {
+		compatible = "maxim,ds26522";
+		reg = <3>;
+		spi-max-frequency = <2000000>;
+		fsl,spi-cs-sck-delay = <100>;
+		fsl,spi-sck-cs-delay = <50>;
+	};
+};
+
+&uqe {
+	ucc_hdlc: ucc@2000 {
+		compatible = "fsl,ucc-hdlc";
+		rx-clock-name = "clk8";
+		tx-clock-name = "clk9";
+		fsl,rx-sync-clock = "rsync_pin";
+		fsl,tx-sync-clock = "tsync_pin";
+		fsl,tx-timeslot-mask = <0xfffffffe>;
+		fsl,rx-timeslot-mask = <0xfffffffe>;
+		fsl,tdm-framer-type = "e1";
+		fsl,tdm-id = <0>;
+		fsl,siram-entry-id = <0>;
+		fsl,tdm-interface;
+	};
 };
 
 &duart0 {
--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
@@ -277,7 +277,7 @@
 
 		dcfg: dcfg@1ee0000 {
 			compatible = "fsl,ls1043a-dcfg", "syscon";
-			reg = <0x0 0x1ee0000 0x0 0x10000>;
+			reg = <0x0 0x1ee0000 0x0 0x1000>;
 			big-endian;
 		};
 
@@ -411,7 +411,7 @@
 		};
 
 		i2c0: i2c@2180000 {
-			compatible = "fsl,vf610-i2c";
+			compatible = "fsl,vf610-i2c", "fsl,ls1043a-vf610-i2c";
 			#address-cells = <1>;
 			#size-cells = <0>;
 			reg = <0x0 0x2180000 0x0 0x10000>;
@@ -421,6 +421,7 @@
 			dmas = <&edma0 1 39>,
 			       <&edma0 1 38>;
 			dma-names = "tx", "rx";
+			scl-gpios = <&gpio4 12 0>;
 			status = "disabled";
 		};
 
@@ -525,6 +526,72 @@
 			#interrupt-cells = <2>;
 		};
 
+		uqe: uqe@2400000 {
+			#address-cells = <1>;
+			#size-cells = <1>;
+			device_type = "qe";
+			compatible = "fsl,qe", "simple-bus";
+			ranges = <0x0 0x0 0x2400000 0x40000>;
+			reg = <0x0 0x2400000 0x0 0x480>;
+			brg-frequency = <100000000>;
+			bus-frequency = <200000000>;
+
+			fsl,qe-num-riscs = <1>;
+			fsl,qe-num-snums = <28>;
+
+			qeic: qeic@80 {
+				compatible = "fsl,qe-ic";
+				reg = <0x80 0x80>;
+				#address-cells = <0>;
+				interrupt-controller;
+				#interrupt-cells = <1>;
+				interrupts = <0 77 0x04 0 77 0x04>;
+			};
+
+			si1: si@700 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,ls1043-qe-si",
+						"fsl,t1040-qe-si";
+				reg = <0x700 0x80>;
+			};
+
+			siram1: siram@1000 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "fsl,ls1043-qe-siram",
+						"fsl,t1040-qe-siram";
+				reg = <0x1000 0x800>;
+			};
+
+			ucc@2000 {
+				cell-index = <1>;
+				reg = <0x2000 0x200>;
+				interrupts = <32>;
+				interrupt-parent = <&qeic>;
+			};
+
+			ucc@2200 {
+				cell-index = <3>;
+				reg = <0x2200 0x200>;
+				interrupts = <34>;
+				interrupt-parent = <&qeic>;
+			};
+
+			muram@10000 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "fsl,qe-muram", "fsl,cpm-muram";
+				ranges = <0x0 0x10000 0x6000>;
+
+				data-only@0 {
+					compatible = "fsl,qe-muram-data",
+					"fsl,cpm-muram-data";
+					reg = <0x0 0x6000>;
+				};
+			};
+		};
+
 		lpuart0: serial@2950000 {
 			compatible = "fsl,ls1021a-lpuart";
 			reg = <0x0 0x2950000 0x0 0x1000>;
@@ -579,6 +646,16 @@
 			status = "disabled";
 		};
 
+		ftm0: ftm0@29d0000 {
+			compatible = "fsl,ftm-alarm";
+			reg = <0x0 0x29d0000 0x0 0x10000>,
+			      <0x0 0x1ee2140 0x0 0x4>;
+			reg-names = "ftm", "FlexTimer1";
+			interrupts = <0 86 0x4>;
+			big-endian;
+			status = "okay";
+		};
+
 		wdog0: wdog@2ad0000 {
 			compatible = "fsl,ls1043a-wdt", "fsl,imx21-wdt";
 			reg = <0x0 0x2ad0000 0x0 0x10000>;
@@ -611,7 +688,10 @@
 			dr_mode = "host";
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
+			usb3-lpm-capable;
+			snps,dis-u1u2-when-u3-quirk;
 			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			configure-gfladj;
 		};
 
 		usb1: usb3@3000000 {
@@ -621,7 +701,10 @@
 			dr_mode = "host";
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
+			usb3-lpm-capable;
+			snps,dis-u1u2-when-u3-quirk;
 			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			configure-gfladj;
 		};
 
 		usb2: usb3@3100000 {
@@ -631,7 +714,10 @@
 			dr_mode = "host";
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
+			usb3-lpm-capable;
+			snps,dis-u1u2-when-u3-quirk;
 			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			configure-gfladj;
 		};
 
 		sata: sata@3200000 {
@@ -670,9 +756,9 @@
 			reg = <0x00 0x03400000 0x0 0x00100000   /* controller registers */
 			       0x40 0x00000000 0x0 0x00002000>; /* configuration space */
 			reg-names = "regs", "config";
-			interrupts = <0 118 0x4>, /* controller interrupt */
-				     <0 117 0x4>; /* PME interrupt */
-			interrupt-names = "intr", "pme";
+			interrupts = <0 117 0x4>, /* PME interrupt */
+				     <0 118 0x4>; /* aer interrupt */
+			interrupt-names = "pme", "aer";
 			#address-cells = <3>;
 			#size-cells = <2>;
 			device_type = "pci";
@@ -696,9 +782,9 @@
 			reg = <0x00 0x03500000 0x0 0x00100000   /* controller registers */
 			       0x48 0x00000000 0x0 0x00002000>; /* configuration space */
 			reg-names = "regs", "config";
-			interrupts = <0 128 0x4>,
-				     <0 127 0x4>;
-			interrupt-names = "intr", "pme";
+			interrupts = <0 127 0x4>,
+				     <0 128 0x4>;
+			interrupt-names = "pme", "aer";
 			#address-cells = <3>;
 			#size-cells = <2>;
 			device_type = "pci";
@@ -722,9 +808,9 @@
 			reg = <0x00 0x03600000 0x0 0x00100000   /* controller registers */
 			       0x50 0x00000000 0x0 0x00002000>; /* configuration space */
 			reg-names = "regs", "config";
-			interrupts = <0 162 0x4>,
-				     <0 161 0x4>;
-			interrupt-names = "intr", "pme";
+			interrupts = <0 161 0x4>,
+				     <0 162 0x4>;
+			interrupt-names = "pme", "aer";
 			#address-cells = <3>;
 			#size-cells = <2>;
 			device_type = "pci";
