From afde0ffa449eef528deb2fe455a512acd0569be4 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Wed, 25 Sep 2019 09:49:58 +0100
Subject: [PATCH] dma-direct: Temporary DMA fix on arm64

See: https://github.com/raspberrypi/linux/issues/3251

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 kernel/dma/direct.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/kernel/dma/direct.c
+++ b/kernel/dma/direct.c
@@ -398,7 +398,7 @@ int dma_direct_supported(struct device *
 	if (IS_ENABLED(CONFIG_ZONE_DMA))
 		min_mask = DMA_BIT_MASK(ARCH_ZONE_DMA_BITS);
 	else
-		min_mask = DMA_BIT_MASK(32);
+		min_mask = DMA_BIT_MASK(30);
 
 	min_mask = min_t(u64, min_mask, (max_pfn - 1) << PAGE_SHIFT);
 
