From 67f4c228c2bf515386cd54073104dc2e6eae85ea Mon Sep 17 00:00:00 2001
From: David Bauer <mail@david-bauer.net>
Date: Fri, 10 Jul 2020 14:58:30 +0200
Subject: [PATCH] rockchip: rk3328: Add support for FriendlyARM NanoPi R2S

This adds support for the NanoPi R2S from FriendlyArm.

Rockchip RK3328 SoC
1GB DDR4 RAM
Gigabit Ethernet (WAN)
Gigabit Ethernet (USB3) (LAN)
USB 2.0 Host Port
MicroSD slot
Reset button
WAN - LAN - SYS LED

Signed-off-by: David Bauer <mail@david-bauer.net>
---
 arch/arm/dts/Makefile                      |   1 +
 arch/arm/dts/rk3328-nanopi-r2s-u-boot.dtsi |  34 +++
 arch/arm/dts/rk3328-nanopi-r2s.dts         | 334 +++++++++++++++++++++
 board/rockchip/evb_rk3328/MAINTAINERS      |   7 +
 configs/nanopi-r2s-rk3328_defconfig        |  99 ++++++
 5 files changed, 475 insertions(+)
 create mode 100644 arch/arm/dts/rk3328-nanopi-r2s-u-boot.dtsi
 create mode 100644 arch/arm/dts/rk3328-nanopi-r2s.dts
 create mode 100644 configs/nanopi-r2s-rk3328_defconfig

--- a/arch/arm/dts/Makefile
+++ b/arch/arm/dts/Makefile
@@ -106,6 +106,7 @@ dtb-$(CONFIG_ROCKCHIP_RK3308) += \
 
 dtb-$(CONFIG_ROCKCHIP_RK3328) += \
 	rk3328-evb.dtb \
+	rk3328-nanopi-r2s.dtb \
 	rk3328-roc-cc.dtb \
 	rk3328-rock64.dtb \
 	rk3328-rock-pi-e.dtb
--- /dev/null
+++ b/arch/arm/dts/rk3328-nanopi-r2s-u-boot.dtsi
@@ -0,0 +1,34 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * (C) Copyright 2018-2019 Rockchip Electronics Co., Ltd
+ * (C) Copyright 2020 David Bauer
+ */
+
+#include "rk3328-u-boot.dtsi"
+#include "rk3328-sdram-ddr4-666.dtsi"
+/ {
+	chosen {
+		u-boot,spl-boot-order = "same-as-spl", &sdmmc, &emmc;
+	};
+};
+
+&gpio0 {
+	u-boot,dm-spl;
+};
+
+&pinctrl {
+	u-boot,dm-spl;
+};
+
+&sdmmc0m1_gpio {
+	u-boot,dm-spl;
+};
+
+&pcfg_pull_up_4ma {
+	u-boot,dm-spl;
+};
+
+/* Need this and all the pinctrl/gpio stuff above to set pinmux */
+&vcc_sd {
+	u-boot,dm-spl;
+};
--- /dev/null
+++ b/arch/arm/dts/rk3328-nanopi-r2s.dts
@@ -0,0 +1,334 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Copyright (c) 2020 David Bauer <mail@david-bauer.net>
+ */
+
+/dts-v1/;
+
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/gpio/gpio.h>
+#include "rk3328.dtsi"
+
+/ {
+	model = "FriendlyARM NanoPi R2S";
+	compatible = "friendlyarm,nanopi-r2s", "rockchip,rk3328";
+
+	chosen {
+		stdout-path = "serial2:1500000n8";
+	};
+
+	gmac_clkin: external-gmac-clock {
+		compatible = "fixed-clock";
+		clock-frequency = <125000000>;
+		clock-output-names = "gmac_clkin";
+		#clock-cells = <0>;
+	};
+
+	vcc_sd: sdmmc-regulator {
+		compatible = "regulator-fixed";
+		gpio = <&gpio0 RK_PD6 GPIO_ACTIVE_LOW>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&sdmmc0m1_gpio>;
+		regulator-name = "vcc_sd";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vcc_io>;
+	};
+
+	vcc_sdio: sdmmcio-regulator {
+		compatible = "regulator-gpio";
+		gpios = <&gpio1 RK_PD4 GPIO_ACTIVE_HIGH>;
+		enable-active-high;
+		states = <1800000 0x1
+			  3300000 0x0>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&sdio_vcc_pin>;
+		regulator-always-on;
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-name = "vcc_sdio";
+		regulator-settling-time-us = <5000>;
+		regulator-type = "voltage";
+		vin-supply = <&vcc_io>;
+	};
+
+	vcc_sys: vcc-sys {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc_sys";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		pinctrl-names = "default";
+		pinctrl-0 = <&led_pins>;
+
+		sys {
+			gpios = <&gpio0 RK_PA2 GPIO_ACTIVE_HIGH>;
+			label = "nanopi-r2s:red:sys";
+		};
+
+		lan {
+			gpios = <&gpio2 RK_PB7 GPIO_ACTIVE_HIGH>;
+			label = "nanopi-r2s:green:lan";
+		};
+
+		wan {
+			gpios = <&gpio2 RK_PC2 GPIO_ACTIVE_HIGH>;
+			label = "nanopi-r2s:green:wan";
+		};
+	};
+
+	gpio_keys {
+		compatible = "gpio-keys-polled";
+		poll-interval = <100>;
+
+		pinctrl-names = "default";
+		pinctrl-0 = <&button_pins>;
+
+		reset {
+			label = "Reset Button";
+			gpios = <&gpio0 RK_PA0 GPIO_ACTIVE_LOW>;
+			linux,code = <KEY_RESTART>;
+			debounce-interval = <50>;
+		};
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu1 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu2 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu3 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&gmac2io {
+	assigned-clocks = <&cru SCLK_MAC2IO>, <&cru SCLK_MAC2IO_EXT>;
+	assigned-clock-parents = <&gmac_clkin>, <&gmac_clkin>;
+	clock_in_out = "input";
+	phy-supply = <&vcc_io>;
+	phy-handle = <&rtl8211e>;
+	phy-mode = "rgmii";
+	pinctrl-names = "default";
+	pinctrl-0 = <&rgmiim1_pins>;
+	snps,aal;
+	snps,reset-gpio = <&gpio1 RK_PC2 GPIO_ACTIVE_LOW>;
+	snps,reset-active-low;
+	snps,reset-delays-us = <0 10000 50000>;
+	tx_delay = <0x24>;
+	rx_delay = <0x18>;
+	status = "okay";
+
+	mdio {
+		compatible = "snps,dwmac-mdio";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		rtl8211e: ethernet-phy@0 {
+			reg = <0>;
+		};
+	};
+};
+
+&i2c1 {
+	status = "okay";
+
+	rk805: rk805@18 {
+		compatible = "rockchip,rk805";
+		reg = <0x18>;
+		interrupt-parent = <&gpio2>;
+		interrupts = <6 IRQ_TYPE_LEVEL_LOW>;
+		#clock-cells = <1>;
+		clock-output-names = "xin32k", "rk805-clkout2";
+		gpio-controller;
+		#gpio-cells = <2>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pmic_int_l>;
+		rockchip,system-power-controller;
+		wakeup-source;
+
+		vcc1-supply = <&vcc_sys>;
+		vcc2-supply = <&vcc_sys>;
+		vcc3-supply = <&vcc_sys>;
+		vcc4-supply = <&vcc_sys>;
+		vcc5-supply = <&vcc_io>;
+		vcc6-supply = <&vcc_sys>;
+
+		regulators {
+			vdd_logic: DCDC_REG1 {
+				regulator-name = "vdd_logic";
+				regulator-min-microvolt = <712500>;
+				regulator-max-microvolt = <1450000>;
+				regulator-ramp-delay = <12500>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1000000>;
+				};
+			};
+
+			vdd_arm: DCDC_REG2 {
+				regulator-name = "vdd_arm";
+				regulator-min-microvolt = <712500>;
+				regulator-max-microvolt = <1450000>;
+				regulator-ramp-delay = <12500>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <950000>;
+				};
+			};
+
+			vcc_ddr: DCDC_REG3 {
+				regulator-name = "vcc_ddr";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+				};
+			};
+
+			vcc_io: DCDC_REG4 {
+				regulator-name = "vcc_io";
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <3300000>;
+				};
+			};
+
+			vcc_18: LDO_REG1 {
+				regulator-name = "vcc_18";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vcc18_emmc: LDO_REG2 {
+				regulator-name = "vcc18_emmc";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vdd_10: LDO_REG3 {
+				regulator-name = "vdd_10";
+				regulator-min-microvolt = <1000000>;
+				regulator-max-microvolt = <1000000>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1000000>;
+				};
+			};
+		};
+	};
+};
+
+&io_domains {
+	status = "okay";
+
+	vccio1-supply = <&vcc_io>;
+	vccio2-supply = <&vcc18_emmc>;
+	vccio3-supply = <&vcc_sdio>;
+	vccio4-supply = <&vcc_18>;
+	vccio5-supply = <&vcc_io>;
+	vccio6-supply = <&vcc_io>;
+	pmuio-supply = <&vcc_io>;
+};
+
+&pinctrl {
+	leds {
+		led_pins: led-pins {
+			rockchip,pins = <0 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>,
+							<2 RK_PB7 RK_FUNC_GPIO &pcfg_pull_none>,
+							<2 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	button {
+		button_pins: button-pins {
+			rockchip,pins = <0 RK_PA0 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	pmic {
+		pmic_int_l: pmic-int-l {
+			rockchip,pins = <2 RK_PA6 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	sd {
+		sdio_vcc_pin: sdio-vcc-pin {
+			rockchip,pins = <1 RK_PD4 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+};
+
+&sdmmc {
+	bus-width = <4>;
+	cap-mmc-highspeed;
+	cap-sd-highspeed;
+	disable-wp;
+	max-frequency = <150000000>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdmmc0_clk &sdmmc0_cmd &sdmmc0_dectn &sdmmc0_bus4>;
+	vmmc-supply = <&vcc_sd>;
+	vqmmc-supply = <&vcc_sdio>;
+	status = "okay";
+};
+
+&tsadc {
+	rockchip,hw-tshut-mode = <0>;
+	rockchip,hw-tshut-polarity = <0>;
+	status = "okay";
+};
+
+&uart2 {
+	status = "okay";
+};
+
+&u2phy {
+	status = "okay";
+
+	u2phy_host: host-port {
+		status = "okay";
+	};
+};
+
+&usb_host0_ehci {
+	status = "okay";
+};
+
+&usb_host0_ohci {
+	status = "okay";
+};
--- a/board/rockchip/evb_rk3328/MAINTAINERS
+++ b/board/rockchip/evb_rk3328/MAINTAINERS
@@ -5,6 +5,13 @@ F:      board/rockchip/evb_rk3328
 F:      include/configs/evb_rk3328.h
 F:      configs/evb-rk3328_defconfig
 
+NANOPI-R2S-RK3328
+M:      David Bauer <mail@david-bauer.net>
+S:      Maintained
+F:      configs/nanopi-r2s-rk3328_defconfig
+F:      arch/arm/dts/rk3328-nanopi-r2s-u-boot.dtsi
+F:      arch/arm/dts/rk3328-nanopi-r2s.dts
+
 ROC-RK3328-CC
 M:      Loic Devulder <ldevulder@suse.com>
 M:      Chen-Yu Tsai <wens@csie.org>
--- /dev/null
+++ b/configs/nanopi-r2s-rk3328_defconfig
@@ -0,0 +1,99 @@
+CONFIG_ARM=y
+CONFIG_ARCH_ROCKCHIP=y
+CONFIG_SYS_TEXT_BASE=0x00200000
+CONFIG_SPL_GPIO_SUPPORT=y
+CONFIG_ENV_OFFSET=0x3F8000
+CONFIG_ROCKCHIP_RK3328=y
+CONFIG_TPL_ROCKCHIP_COMMON_BOARD=y
+CONFIG_TPL_LIBCOMMON_SUPPORT=y
+CONFIG_TPL_LIBGENERIC_SUPPORT=y
+CONFIG_SPL_DRIVERS_MISC_SUPPORT=y
+CONFIG_SPL_STACK_R_ADDR=0x600000
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_DEBUG_UART_BASE=0xFF130000
+CONFIG_DEBUG_UART_CLOCK=24000000
+CONFIG_SMBIOS_PRODUCT_NAME="nanopi_r2s_rk3328"
+CONFIG_DEBUG_UART=y
+CONFIG_TPL_SYS_MALLOC_F_LEN=0x800
+# CONFIG_ANDROID_BOOT_IMAGE is not set
+CONFIG_FIT=y
+CONFIG_FIT_VERBOSE=y
+CONFIG_SPL_LOAD_FIT=y
+CONFIG_DEFAULT_FDT_FILE="rockchip/rk3328-nanopi-r2s.dtb"
+CONFIG_MISC_INIT_R=y
+# CONFIG_DISPLAY_CPUINFO is not set
+CONFIG_DISPLAY_BOARDINFO_LATE=y
+# CONFIG_SPL_RAW_IMAGE_SUPPORT is not set
+CONFIG_TPL_SYS_MALLOC_SIMPLE=y
+CONFIG_SPL_STACK_R=y
+CONFIG_SPL_I2C_SUPPORT=y
+CONFIG_SPL_POWER_SUPPORT=y
+CONFIG_SPL_ATF=y
+CONFIG_SPL_ATF_NO_PLATFORM_PARAM=y
+CONFIG_CMD_BOOTZ=y
+CONFIG_CMD_GPT=y
+CONFIG_CMD_MMC=y
+CONFIG_CMD_USB=y
+# CONFIG_CMD_SETEXPR is not set
+CONFIG_CMD_TIME=y
+CONFIG_SPL_OF_CONTROL=y
+CONFIG_TPL_OF_CONTROL=y
+CONFIG_DEFAULT_DEVICE_TREE="rk3328-nanopi-r2s"
+CONFIG_OF_SPL_REMOVE_PROPS="clock-names interrupt-parent assigned-clocks assigned-clock-rates assigned-clock-parents"
+CONFIG_TPL_OF_PLATDATA=y
+CONFIG_ENV_IS_IN_MMC=y
+CONFIG_SYS_RELOC_GD_ENV_ADDR=y
+CONFIG_NET_RANDOM_ETHADDR=y
+CONFIG_TPL_DM=y
+CONFIG_REGMAP=y
+CONFIG_SPL_REGMAP=y
+CONFIG_TPL_REGMAP=y
+CONFIG_SYSCON=y
+CONFIG_SPL_SYSCON=y
+CONFIG_TPL_SYSCON=y
+CONFIG_CLK=y
+CONFIG_SPL_CLK=y
+CONFIG_FASTBOOT_BUF_ADDR=0x800800
+CONFIG_FASTBOOT_CMD_OEM_FORMAT=y
+CONFIG_ROCKCHIP_GPIO=y
+CONFIG_SYS_I2C_ROCKCHIP=y
+CONFIG_MMC_DW=y
+CONFIG_MMC_DW_ROCKCHIP=y
+CONFIG_SF_DEFAULT_SPEED=20000000
+CONFIG_DM_ETH=y
+CONFIG_ETH_DESIGNWARE=y
+CONFIG_GMAC_ROCKCHIP=y
+CONFIG_PINCTRL=y
+CONFIG_SPL_PINCTRL=y
+CONFIG_DM_PMIC=y
+CONFIG_PMIC_RK8XX=y
+CONFIG_SPL_DM_REGULATOR=y
+CONFIG_REGULATOR_PWM=y
+CONFIG_DM_REGULATOR_FIXED=y
+CONFIG_SPL_DM_REGULATOR_FIXED=y
+CONFIG_REGULATOR_RK8XX=y
+CONFIG_PWM_ROCKCHIP=y
+CONFIG_RAM=y
+CONFIG_SPL_RAM=y
+CONFIG_TPL_RAM=y
+CONFIG_DM_RESET=y
+CONFIG_BAUDRATE=1500000
+CONFIG_DEBUG_UART_SHIFT=2
+CONFIG_SYSRESET=y
+# CONFIG_TPL_SYSRESET is not set
+CONFIG_USB=y
+CONFIG_USB_XHCI_HCD=y
+CONFIG_USB_XHCI_DWC3=y
+CONFIG_USB_EHCI_HCD=y
+CONFIG_USB_EHCI_GENERIC=y
+CONFIG_USB_OHCI_HCD=y
+CONFIG_USB_OHCI_GENERIC=y
+CONFIG_USB_DWC2=y
+CONFIG_USB_DWC3=y
+# CONFIG_USB_DWC3_GADGET is not set
+CONFIG_USB_GADGET=y
+CONFIG_USB_GADGET_DWC2_OTG=y
+CONFIG_SPL_TINY_MEMSET=y
+CONFIG_TPL_TINY_MEMSET=y
+CONFIG_ERRNO_STR=y
+CONFIG_SMBIOS_MANUFACTURER="pine64"
