// SPDX-License-Identifier: GPL-2.0
/dts-v1/;

#include "mt7621_netgear_sercomm_bzv.dtsi"

/ {
	compatible = "netgear,r6800", "mediatek,mt7621-soc";
	model = "Netgear R6800";

	aliases {
		led-boot = &led_power_white;
		led-failsafe = &led_power_orange;
		led-running = &led_power_white;
		led-upgrade = &led_power_orange;
	};

	leds {
		compatible = "gpio-leds";

		led_power_orange: power_orange {
			gpios = <&gpio_expander 0 GPIO_ACTIVE_LOW>;
			label = "r6800:orange:power";
		};

		led_power_white: power_white {
			gpios = <&gpio_expander 1 GPIO_ACTIVE_LOW>;
			label = "r6800:white:power";
		};

		wan_orange {
			gpios = <&gpio_expander 2 GPIO_ACTIVE_LOW>;
			label = "r6800:orange:wan";
		};

		wan_white {
			gpios = <&gpio_expander 3 GPIO_ACTIVE_LOW>;
			label = "r6800:white:wan";
		};

		wlan2g {
			gpios = <&gpio_expander 4 GPIO_ACTIVE_LOW>;
			label = "r6800:white:wlan2g";
			linux,default-trigger = "phy0radio";
		};

		wlan5g {
			gpios = <&gpio_expander 5 GPIO_ACTIVE_LOW>;
			label = "r6800:white:wlan5g";
			linux,default-trigger = "phy1radio";
		};

		usb2 {
			gpios = <&gpio_expander 6 GPIO_ACTIVE_LOW>;
			label = "r6800:white:usb2";
			linux,default-trigger = "usbport";
			trigger-sources = <&ehci_port2>;
		};

		usb3 {
			gpios = <&gpio_expander 7 GPIO_ACTIVE_LOW>;
			label = "r6800:white:usb3";
			linux,default-trigger = "usbport";
			trigger-sources = <&xhci_ehci_port1>;
		};

		lan1_orange {
			gpios = <&gpio_expander 8 GPIO_ACTIVE_LOW>;
			label = "r6800:orange:lan1";
		};

		lan1_white {
			gpios = <&gpio_expander 9 GPIO_ACTIVE_LOW>;
			label = "r6800:white:lan1";
		};

		lan2_orange {
			gpios = <&gpio_expander 10 GPIO_ACTIVE_LOW>;
			label = "r6800:orange:lan2";
		};

		lan2_white {
			gpios = <&gpio_expander 11 GPIO_ACTIVE_LOW>;
			label = "r6800:white:lan2";
		};

		lan3_orange {
			gpios = <&gpio_expander 12 GPIO_ACTIVE_LOW>;
			label = "r6800:orange:lan3";
		};

		lan3_white {
			gpios = <&gpio_expander 13 GPIO_ACTIVE_LOW>;
			label = "r6800:white:lan3";
		};

		lan4_orange {
			gpios = <&gpio_expander 14 GPIO_ACTIVE_LOW>;
			label = "r6800:orange:lan4";
		};

		lan4_white {
			gpios = <&gpio_expander 15 GPIO_ACTIVE_LOW>;
			label = "r6800:white:lan4";
		};

		wps {
			gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
			label = "r6800:white:wps";
		};

		wlan {
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
			label = "r6800:white:wlan";
		};
	};
};

&state_default {
	gpio {
		groups = "uart3", "uart2", "jtag", "wdt";
		function = "gpio";
	};
};
