From 6731d2c9039fbe1ecf21915eab3acee0a999508a Mon Sep 17 00:00:00 2001
From: David Bauer <mail@david-bauer.net>
Date: Fri, 10 Jul 2020 21:38:20 +0200
Subject: [PATCH] rockchip: use system LED for OpenWrt

Use the SYS LED on the casing for showing system status.

This patch is kept seperate from the NanoPi R2S support patch, as i plan
on submitting the device support upstream.

Signed-off-by: David Bauer <mail@david-bauer.net>
---
 arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2s.dts | 9 ++++++++-
 1 file changed, 8 insertions(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2s.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2s.dts
@@ -17,6 +17,13 @@
 		stdout-path = "serial2:1500000n8";
 	};
 
+	aliases {
+		led-boot = &led_sys;
+		led-failsafe = &led_sys;
+		led-running = &led_sys;
+		led-upgrade = &led_sys;
+	};
+
 	gmac_clkin: external-gmac-clock {
 		compatible = "fixed-clock";
 		clock-frequency = <125000000>;
@@ -67,7 +74,7 @@
 		pinctrl-names = "default";
 		pinctrl-0 = <&led_pins>;
 
-		sys {
+		led_sys: sys {
 			gpios = <&gpio0 RK_PA2 GPIO_ACTIVE_HIGH>;
 			label = "nanopi-r2s:red:sys";
 		};
