From 971a2bb14b459819db1bda8fcdf953e493242b42 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Tue, 19 May 2020 16:20:30 +0100
Subject: [PATCH] drm/vc4: Add FKMS as an acceptable node for dma
 ranges.

Under FKMS, the firmware (via FKMS) also requires the VideoCore cache
aliases for image planes, as defined by the dma-ranges under /soc.

Add rpi-firmware-kms to the list of acceptable nodes to look for
to copy dma config from.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/gpu/drm/vc4/vc4_drv.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/gpu/drm/vc4/vc4_drv.c
+++ b/drivers/gpu/drm/vc4/vc4_drv.c
@@ -251,6 +251,7 @@ static void vc4_match_add_drivers(struct
 
 const struct of_device_id vc4_dma_range_matches[] = {
 	{ .compatible = "brcm,bcm2835-hvs" },
+	{ .compatible = "raspberrypi,rpi-firmware-kms" },
 	{ .compatible = "brcm,bcm2835-v3d" },
 	{ .compatible = "brcm,cygnus-v3d" },
 	{ .compatible = "brcm,vc4-v3d" },
