From d8715f02b84c1a210b6fd84badc41eced6272424 Mon Sep 17 00:00:00 2001
From: Yangbo Lu <yangbo.lu@nxp.com>
Date: Mon, 30 Mar 2020 16:30:26 +0800
Subject: [PATCH] Revert "ASoC: fsl: add imx-pcm-dma v2 platform driver (part
 2)"

This reverts commit 5d816f1a5cac458a7fff9ecf896c85eb351a7352.
---
 sound/soc/fsl/fsl_sai.c | 4 +---
 1 file changed, 1 insertion(+), 3 deletions(-)

--- a/sound/soc/fsl/fsl_sai.c
+++ b/sound/soc/fsl/fsl_sai.c
@@ -1519,8 +1519,6 @@ static int fsl_sai_probe(struct platform
 				   MCLK_DIR(index));
 	}
 
-	sai->dma_params_rx.filter_data = "rx";
-	sai->dma_params_tx.filter_data = "tx";
 	sai->dma_params_rx.addr = res->start + FSL_SAI_RDR0;
 	sai->dma_params_tx.addr = res->start + FSL_SAI_TDR0;
 	sai->dma_params_rx.maxburst = FSL_SAI_MAXBURST_RX;
@@ -1540,7 +1538,7 @@ static int fsl_sai_probe(struct platform
 		goto err_pm_disable;
 
 	if (sai->soc->imx)
-		ret = imx_pcm_platform_register(&pdev->dev);
+		ret = imx_pcm_dma_init(pdev, IMX_SAI_DMABUF_SIZE);
 		if (ret)
 			goto err_pm_disable;
 	} else {
