From dc45d9e04572b5cd6d32f51cdf9f62b18022e6dd Mon Sep 17 00:00:00 2001
From: Russell King <rmk+kernel@armlinux.org.uk>
Date: Thu, 21 Nov 2019 17:32:59 +0000
Subject: [PATCH 644/660] net: sfp: derive interface mode from ethtool link
 modes

We don't need the EEPROM ID to derive the phy interface mode as we can
derive it merely from the ethtool link modes.  Remove the EEPROM ID
argument to sfp_select_interface().

Signed-off-by: Russell King <rmk+kernel@armlinux.org.uk>
---
 drivers/net/phy/marvell10g.c |  2 +-
 drivers/net/phy/phylink.c    |  2 +-
 drivers/net/phy/sfp-bus.c    | 11 ++++-------
 include/linux/sfp.h          |  2 --
 4 files changed, 6 insertions(+), 11 deletions(-)

--- a/drivers/net/phy/marvell10g.c
+++ b/drivers/net/phy/marvell10g.c
@@ -227,7 +227,7 @@ static int mv3310_sfp_insert(void *upstr
 	phy_interface_t iface;
 
 	sfp_parse_support(phydev->sfp_bus, id, support);
-	iface = sfp_select_interface(phydev->sfp_bus, id, support);
+	iface = sfp_select_interface(phydev->sfp_bus, support);
 
 	if (iface != PHY_INTERFACE_MODE_10GKR) {
 		dev_err(&phydev->mdio.dev, "incompatible SFP module inserted\n");
--- a/drivers/net/phy/phylink.c
+++ b/drivers/net/phy/phylink.c
@@ -1663,7 +1663,7 @@ static int phylink_sfp_module_insert(voi
 
 	linkmode_copy(support1, support);
 
-	iface = sfp_select_interface(pl->sfp_bus, id, config.advertising);
+	iface = sfp_select_interface(pl->sfp_bus, config.advertising);
 	if (iface == PHY_INTERFACE_MODE_NA) {
 		netdev_err(pl->netdev,
 			   "selection of interface failed, advertisement %*pb\n",
--- a/drivers/net/phy/sfp-bus.c
+++ b/drivers/net/phy/sfp-bus.c
@@ -319,16 +319,12 @@ EXPORT_SYMBOL_GPL(sfp_parse_support);
 /**
  * sfp_select_interface() - Select appropriate phy_interface_t mode
  * @bus: a pointer to the &struct sfp_bus structure for the sfp module
- * @id: a pointer to the module's &struct sfp_eeprom_id
  * @link_modes: ethtool link modes mask
  *
- * Derive the phy_interface_t mode for the information found in the
- * module's identifying EEPROM and the link modes mask. There is no
- * standard or defined way to derive this information, so we decide
- * based upon the link mode mask.
+ * Derive the phy_interface_t mode for the SFP module from the link
+ * modes mask.
  */
 phy_interface_t sfp_select_interface(struct sfp_bus *bus,
-				     const struct sfp_eeprom_id *id,
 				     unsigned long *link_modes)
 {
 	if (phylink_test(link_modes, 10000baseCR_Full) ||
@@ -341,7 +337,8 @@ phy_interface_t sfp_select_interface(str
 	if (phylink_test(link_modes, 2500baseX_Full))
 		return PHY_INTERFACE_MODE_2500BASEX;
 
-	if (id->base.e1000_base_t)
+	if (phylink_test(link_modes, 1000baseT_Half) ||
+	    phylink_test(link_modes, 1000baseT_Full))
 		return PHY_INTERFACE_MODE_SGMII;
 
 	if (phylink_test(link_modes, 1000baseX_Full))
--- a/include/linux/sfp.h
+++ b/include/linux/sfp.h
@@ -504,7 +504,6 @@ int sfp_parse_port(struct sfp_bus *bus,
 void sfp_parse_support(struct sfp_bus *bus, const struct sfp_eeprom_id *id,
 		       unsigned long *support);
 phy_interface_t sfp_select_interface(struct sfp_bus *bus,
-				     const struct sfp_eeprom_id *id,
 				     unsigned long *link_modes);
 
 int sfp_get_module_info(struct sfp_bus *bus, struct ethtool_modinfo *modinfo);
@@ -532,7 +531,6 @@ static inline void sfp_parse_support(str
 }
 
 static inline phy_interface_t sfp_select_interface(struct sfp_bus *bus,
-						   const struct sfp_eeprom_id *id,
 						   unsigned long *link_modes)
 {
 	return PHY_INTERFACE_MODE_NA;
