From a3488aa9bed37c56e405967d44e821c484b5d6b9 Mon Sep 17 00:00:00 2001
From: Ram Chandra Jangir <rjangir@codeaurora.org>
Date: Fri, 28 Sep 2018 15:19:50 +0530
Subject: [PATCH] ipq8064: pinctrl: Fixed missing RGMII pincontrol definitions

Signed-off-by: Ram Chandra Jangir <rjangir@codeaurora.org>
---
 drivers/pinctrl/qcom/pinctrl-ipq8064.c | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

--- a/drivers/pinctrl/qcom/pinctrl-ipq8064.c
+++ b/drivers/pinctrl/qcom/pinctrl-ipq8064.c
@@ -299,7 +299,7 @@ static const char * const gpio_groups[]
 };
 
 static const char * const mdio_groups[] = {
-	"gpio0", "gpio1", "gpio10", "gpio11",
+	"gpio0", "gpio1", "gpio2", "gpio10", "gpio11", "gpio66",
 };
 
 static const char * const mi2s_groups[] = {
@@ -403,8 +403,8 @@ static const char * const usb2_hsic_grou
 };
 
 static const char * const rgmii2_groups[] = {
-	"gpio27", "gpio28", "gpio29", "gpio30", "gpio31", "gpio32",
-	"gpio51", "gpio52", "gpio59", "gpio60", "gpio61", "gpio62",
+	"gpio2", "gpio27", "gpio28", "gpio29", "gpio30", "gpio31", "gpio32",
+	"gpio51", "gpio52", "gpio59", "gpio60", "gpio61", "gpio62", "gpio66",
 };
 
 static const char * const sata_groups[] = {
@@ -539,7 +539,7 @@ static const struct msm_function ipq8064
 static const struct msm_pingroup ipq8064_groups[] = {
 	PINGROUP(0, mdio, NA, NA, NA, NA, NA, NA, NA, NA, NA),
 	PINGROUP(1, mdio, NA, NA, NA, NA, NA, NA, NA, NA, NA),
-	PINGROUP(2, gsbi5_spi_cs3, NA, NA, NA, NA, NA, NA, NA, NA, NA),
+	PINGROUP(2, gsbi5_spi_cs3, rgmii2, mdio, NA, NA, NA, NA, NA, NA, NA),
 	PINGROUP(3, pcie1_rst, pcie1_prsnt, pdm, NA, NA, NA, NA, NA, NA, NA),
 	PINGROUP(4, pcie1_pwren_n, pcie1_pwren, NA, NA, NA, NA, NA, NA, NA, NA),
 	PINGROUP(5, pcie1_clk_req, pcie1_pwrflt, NA, NA, NA, NA, NA, NA, NA, NA),
@@ -603,7 +603,7 @@ static const struct msm_pingroup ipq8064
 	PINGROUP(63, pcie3_rst, NA, NA, NA, NA, NA, NA, NA, NA, NA),
 	PINGROUP(64, NA, NA, NA, NA, NA, NA, NA, NA, NA, NA),
 	PINGROUP(65, pcie3_clk_req, NA, NA, NA, NA, NA, NA, NA, NA, NA),
-	PINGROUP(66, NA, NA, NA, NA, NA, NA, NA, NA, NA, NA),
+	PINGROUP(66, rgmii2, mdio, NA, NA, NA, NA, NA, NA, NA, NA),
 	PINGROUP(67, usb2_hsic, NA, NA, NA, NA, NA, NA, NA, NA, NA),
 	PINGROUP(68, usb2_hsic, NA, NA, NA, NA, NA, NA, NA, NA, NA),
 	SDC_PINGROUP(sdc3_clk, 0x204a, 14, 6),
