From 559391fc20fae506adcb311b904cc544c76436c0 Mon Sep 17 00:00:00 2001
From: Russell King <rmk+kernel@armlinux.org.uk>
Date: Thu, 7 Nov 2019 18:52:07 +0000
Subject: [PATCH 634/660] net: sfp: allow modules with slow diagnostics to
 probe

When a module is inserted, we attempt to read read the ID from address
0x50.  Once we are able to read the ID, we immediately attempt to
initialise the hwmon support by reading from address 0x51.  If this
fails, then we fall into error state, and assume that the module is
not usable.

Modules such as the ALCATELLUCENT 3FE46541AA use a real EEPROM for
I2C address 0x50, which responds immediately.  However, address 0x51
is an emulated, which only becomes available once the on-board firmware
has booted.  This prompts us to fall into the error state.

Since the module may be usable without diagnostics, arrange for the
hwmon probe independent of the rest of the SFP itself, retrying every
5s for up to about 60s for the monitoring to become available, and
print an error message if it doesn't become available.

Signed-off-by: Russell King <rmk+kernel@armlinux.org.uk>
---
 drivers/net/phy/sfp.c | 96 +++++++++++++++++++++++++++++++++----------
 1 file changed, 74 insertions(+), 22 deletions(-)

--- a/drivers/net/phy/sfp.c
+++ b/drivers/net/phy/sfp.c
@@ -216,6 +216,8 @@ struct sfp {
 
 #if IS_ENABLED(CONFIG_HWMON)
 	struct sfp_diag diag;
+	struct delayed_work hwmon_probe;
+	unsigned int hwmon_tries;
 	struct device *hwmon_dev;
 	char *hwmon_name;
 #endif
@@ -1094,29 +1096,27 @@ static const struct hwmon_chip_info sfp_
 	.info = sfp_hwmon_info,
 };
 
-static int sfp_hwmon_insert(struct sfp *sfp)
+static void sfp_hwmon_probe(struct work_struct *work)
 {
+	struct sfp *sfp = container_of(work, struct sfp, hwmon_probe.work);
 	int err, i;
 
-	if (sfp->id.ext.sff8472_compliance == SFP_SFF8472_COMPLIANCE_NONE)
-		return 0;
-
-	if (!(sfp->id.ext.diagmon & SFP_DIAGMON_DDM))
-		return 0;
-
-	if (sfp->id.ext.diagmon & SFP_DIAGMON_ADDRMODE)
-		/* This driver in general does not support address
-		 * change.
-		 */
-		return 0;
-
 	err = sfp_read(sfp, true, 0, &sfp->diag, sizeof(sfp->diag));
-	if (err < 0)
-		return err;
+	if (err < 0) {
+		if (sfp->hwmon_tries--) {
+			mod_delayed_work(system_wq, &sfp->hwmon_probe,
+					 T_PROBE_RETRY_SLOW);
+		} else {
+			dev_warn(sfp->dev, "hwmon probe failed: %d\n", err);
+		}
+		return;
+	}
 
 	sfp->hwmon_name = kstrdup(dev_name(sfp->dev), GFP_KERNEL);
-	if (!sfp->hwmon_name)
-		return -ENODEV;
+	if (!sfp->hwmon_name) {
+		dev_err(sfp->dev, "out of memory for hwmon name\n");
+		return;
+	}
 
 	for (i = 0; sfp->hwmon_name[i]; i++)
 		if (hwmon_is_bad_char(sfp->hwmon_name[i]))
@@ -1126,18 +1126,52 @@ static int sfp_hwmon_insert(struct sfp *
 							 sfp->hwmon_name, sfp,
 							 &sfp_hwmon_chip_info,
 							 NULL);
+	if (IS_ERR(sfp->hwmon_dev))
+		dev_err(sfp->dev, "failed to register hwmon device: %ld\n",
+			PTR_ERR(sfp->hwmon_dev));
+}
+
+static int sfp_hwmon_insert(struct sfp *sfp)
+{
+	if (sfp->id.ext.sff8472_compliance == SFP_SFF8472_COMPLIANCE_NONE)
+		return 0;
+
+	if (!(sfp->id.ext.diagmon & SFP_DIAGMON_DDM))
+		return 0;
+
+	if (sfp->id.ext.diagmon & SFP_DIAGMON_ADDRMODE)
+		/* This driver in general does not support address
+		 * change.
+		 */
+		return 0;
+
+	mod_delayed_work(system_wq, &sfp->hwmon_probe, 1);
+	sfp->hwmon_tries = R_PROBE_RETRY_SLOW;
 
-	return PTR_ERR_OR_ZERO(sfp->hwmon_dev);
+	return 0;
 }
 
 static void sfp_hwmon_remove(struct sfp *sfp)
 {
+	cancel_delayed_work_sync(&sfp->hwmon_probe);
 	if (!IS_ERR_OR_NULL(sfp->hwmon_dev)) {
 		hwmon_device_unregister(sfp->hwmon_dev);
 		sfp->hwmon_dev = NULL;
 		kfree(sfp->hwmon_name);
 	}
 }
+
+static int sfp_hwmon_init(struct sfp *sfp)
+{
+	INIT_DELAYED_WORK(&sfp->hwmon_probe, sfp_hwmon_probe);
+
+	return 0;
+}
+
+static void sfp_hwmon_exit(struct sfp *sfp)
+{
+	cancel_delayed_work_sync(&sfp->hwmon_probe);
+}
 #else
 static int sfp_hwmon_insert(struct sfp *sfp)
 {
@@ -1147,6 +1181,15 @@ static int sfp_hwmon_insert(struct sfp *
 static void sfp_hwmon_remove(struct sfp *sfp)
 {
 }
+
+static int sfp_hwmon_init(struct sfp *sfp)
+{
+	return 0;
+}
+
+static void sfp_hwmon_exit(struct sfp *sfp)
+{
+}
 #endif
 
 /* Helpers */
@@ -1483,10 +1526,6 @@ static int sfp_sm_mod_probe(struct sfp *
 	if (ret < 0)
 		return ret;
 
-	ret = sfp_hwmon_insert(sfp);
-	if (ret < 0)
-		return ret;
-
 	return 0;
 }
 
@@ -1635,6 +1674,15 @@ static void sfp_sm_module(struct sfp *sf
 	case SFP_MOD_ERROR:
 		break;
 	}
+
+#if IS_ENABLED(CONFIG_HWMON)
+	if (sfp->sm_mod_state >= SFP_MOD_WAITDEV &&
+	    IS_ERR_OR_NULL(sfp->hwmon_dev)) {
+		err = sfp_hwmon_insert(sfp);
+		if (err)
+			dev_warn(sfp->dev, "hwmon probe failed: %d\n", err);
+	}
+#endif
 }
 
 static void sfp_sm_main(struct sfp *sfp, unsigned int event)
@@ -1936,6 +1984,8 @@ static struct sfp *sfp_alloc(struct devi
 	INIT_DELAYED_WORK(&sfp->poll, sfp_poll);
 	INIT_DELAYED_WORK(&sfp->timeout, sfp_timeout);
 
+	sfp_hwmon_init(sfp);
+
 	return sfp;
 }
 
@@ -1943,6 +1993,8 @@ static void sfp_cleanup(void *data)
 {
 	struct sfp *sfp = data;
 
+	sfp_hwmon_exit(sfp);
+
 	cancel_delayed_work_sync(&sfp->poll);
 	cancel_delayed_work_sync(&sfp->timeout);
 	if (sfp->i2c_mii) {
