From 9a379dd76a0369c09f1b613bdd869b6b0354a0f3 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Wed, 31 Oct 2018 14:57:21 +0000
Subject: [PATCH] media: tc358743: Add support for 972Mbit/s link freq.

Adds register setups for running the CSI lanes at 972Mbit/s,
which allows 1080P50 UYVY down 2 lanes.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 drivers/media/i2c/tc358743.c | 47 +++++++++++++++++++++++++-----------
 1 file changed, 33 insertions(+), 14 deletions(-)

--- a/drivers/media/i2c/tc358743.c
+++ b/drivers/media/i2c/tc358743.c
@@ -1976,6 +1976,7 @@ static int tc358743_probe_of(struct tc35
 	/*
 	 * The CSI bps per lane must be between 62.5 Mbps and 1 Gbps.
 	 * The default is 594 Mbps for 4-lane 1080p60 or 2-lane 720p60.
+	 * 972 Mbps allows 1080P50 UYVY over 2-lane.
 	 */
 	bps_pr_lane = 2 * endpoint.link_frequencies[0];
 	if (bps_pr_lane < 62500000U || bps_pr_lane > 1000000000U) {
@@ -1988,23 +1989,41 @@ static int tc358743_probe_of(struct tc35
 			       state->pdata.refclk_hz * state->pdata.pll_prd;
 
 	/*
-	 * FIXME: These timings are from REF_02 for 594 Mbps per lane (297 MHz
-	 * link frequency). In principle it should be possible to calculate
+	 * FIXME: These timings are from REF_02 for 594 or 972 Mbps per lane
+	 * (297 MHz or 486 MHz link frequency).
+	 * In principle it should be possible to calculate
 	 * them based on link frequency and resolution.
 	 */
-	if (bps_pr_lane != 594000000U)
+	switch (bps_pr_lane) {
+	default:
 		dev_warn(dev, "untested bps per lane: %u bps\n", bps_pr_lane);
-	state->pdata.lineinitcnt = 0xe80;
-	state->pdata.lptxtimecnt = 0x003;
-	/* tclk-preparecnt: 3, tclk-zerocnt: 20 */
-	state->pdata.tclk_headercnt = 0x1403;
-	state->pdata.tclk_trailcnt = 0x00;
-	/* ths-preparecnt: 3, ths-zerocnt: 1 */
-	state->pdata.ths_headercnt = 0x0103;
-	state->pdata.twakeup = 0x4882;
-	state->pdata.tclk_postcnt = 0x008;
-	state->pdata.ths_trailcnt = 0x2;
-	state->pdata.hstxvregcnt = 0;
+	case 594000000U:
+		state->pdata.lineinitcnt = 0xe80;
+		state->pdata.lptxtimecnt = 0x003;
+		/* tclk-preparecnt: 3, tclk-zerocnt: 20 */
+		state->pdata.tclk_headercnt = 0x1403;
+		state->pdata.tclk_trailcnt = 0x00;
+		/* ths-preparecnt: 3, ths-zerocnt: 1 */
+		state->pdata.ths_headercnt = 0x0103;
+		state->pdata.twakeup = 0x4882;
+		state->pdata.tclk_postcnt = 0x008;
+		state->pdata.ths_trailcnt = 0x2;
+		state->pdata.hstxvregcnt = 0;
+		break;
+	case 972000000U:
+		state->pdata.lineinitcnt = 0x1b58;
+		state->pdata.lptxtimecnt = 0x007;
+		/* tclk-preparecnt: 6, tclk-zerocnt: 40 */
+		state->pdata.tclk_headercnt = 0x2806;
+		state->pdata.tclk_trailcnt = 0x00;
+		/* ths-preparecnt: 6, ths-zerocnt: 8 */
+		state->pdata.ths_headercnt = 0x0806;
+		state->pdata.twakeup = 0x4268;
+		state->pdata.tclk_postcnt = 0x008;
+		state->pdata.ths_trailcnt = 0x5;
+		state->pdata.hstxvregcnt = 0;
+		break;
+	}
 
 	state->reset_gpio = devm_gpiod_get_optional(dev, "reset",
 						    GPIOD_OUT_LOW);
