// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include "mt7620a_netgear_ex3x00_ex61xx.dtsi"

/ {
	compatible = "netgear,ex6120", "ralink,mt7620a-soc";
	model = "Netgear EX6120";

	aliases {
		led-boot = &led_power_amber;
		led-failsafe = &led_power_amber;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power_green {
			label = "ex6120:green:power";
			gpios = <&gpio2 23 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		led_power_amber: power_amber {
			label = "ex6120:amber:power";
			gpios = <&gpio2 28 GPIO_ACTIVE_LOW>;
		};

		router_green {
			label = "ex6120:green:router";
			gpios = <&gpio2 25 GPIO_ACTIVE_LOW>;
		};

		router_red {
			label = "ex6120:red:router";
			gpios = <&gpio2 24 GPIO_ACTIVE_LOW>;
		};

		device_green {
			label = "ex6120:green:device";
			gpios = <&gpio2 20 GPIO_ACTIVE_LOW>;
		};

		device_red {
			label = "ex6120:red:device";
			gpios = <&gpio2 21 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "ex6120:green:wps";
			gpios = <&gpio2 27 GPIO_ACTIVE_LOW>;
		};
	};
};
