/dts-v1/;

#include "bcm6358.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "T-Com Speedport W 303V";
	compatible = "t-com,speedport-w-303v", "brcm,bcm6358";

	aliases {
		led-boot = &led_power_adsl_green;
		led-failsafe = &led_power_adsl_green;
		led-running = &led_power_adsl_green;
		led-upgrade = &led_power_adsl_green;
	};

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&pinctrl 11 0>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		ses {
			label = "ses";
			gpios = <&pinctrl 37 1>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		ses_green {
			label = "spw303v:green:ses";
			gpios = <&pinctrl 0 1>;
		};
		power_adsl_red {
			label = "spw303v:red:power+adsl";
			gpios = <&pinctrl 2 1>;
		};
		ppp_green {
			label = "spw303v:green:ppp";
			gpios = <&pinctrl 5 1>;
		};
		led_power_adsl_green: power_adsl_green {
			label = "spw303v:green:power+adsl";
			gpios = <&pinctrl 22 1>;
			default-state = "on";
		};
		voip_green {
			label = "spw303v:green:voip";
			gpios = <&pinctrl 27 1>;
		};
		pots_green {
			label = "spw303v:green:pots";
			gpios = <&pinctrl 31 1>;
		};
	};
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		cfe@0 {
			label = "CFE";
			reg = <0x000000 0x010000>;
			read-only;
		};

		linux@10000 {
			label = "linux";
			reg = <0x010000 0x7e0000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		nvram@7f0000 {
			label = "nvram";
			reg = <0x7f0000 0x010000>;
		};
	};
};

&uart0 {
	status = "okay";
};
