From d4806e4f103895387dc679fe53e1f4a5d41391bf Mon Sep 17 00:00:00 2001
From: Peter Chen <peter.chen@nxp.com>
Date: Thu, 18 Jan 2018 11:03:24 +0800
Subject: [PATCH] MLK-17380-3 usb: move EH SINGLE_STEP_SET_FEATURE implement to
 core

Since other USB 2.0 host may need it, like USB2 for XHCI. We move
this design to HCD core.

Acked-by: Jun Li <jun.li@nxp.com>
Signed-off-by: Peter Chen <peter.chen@nxp.com>
(cherry picked from commit 035a27e1a3088261f40f77534aaccfe5825c2f96)
---
 drivers/usb/core/hcd.c      | 134 ++++++++++++++++++++++++++++++++++++++++++
 drivers/usb/host/ehci-hcd.c |   4 ++
 drivers/usb/host/ehci-hub.c | 139 --------------------------------------------
 drivers/usb/host/ehci-q.c   |   2 +-
 include/linux/usb/hcd.h     |  13 ++++-
 5 files changed, 151 insertions(+), 141 deletions(-)

--- a/drivers/usb/core/hcd.c
+++ b/drivers/usb/core/hcd.c
@@ -2104,6 +2104,140 @@ int usb_hcd_get_frame_number (struct usb
 }
 
 /*-------------------------------------------------------------------------*/
+#ifdef CONFIG_USB_HCD_TEST_MODE
+
+static void usb_ehset_completion(struct urb *urb)
+{
+	struct completion  *done = urb->context;
+
+	complete(done);
+}
+/*
+ * Allocate and initialize a control URB. This request will be used by the
+ * EHSET SINGLE_STEP_SET_FEATURE test in which the DATA and STATUS stages
+ * of the GetDescriptor request are sent 15 seconds after the SETUP stage.
+ * Return NULL if failed.
+ */
+static struct urb *request_single_step_set_feature_urb(
+	struct usb_device	*udev,
+	void			*dr,
+	void			*buf,
+	struct completion	*done
+) {
+	struct urb *urb;
+	struct usb_hcd *hcd = bus_to_hcd(udev->bus);
+	struct usb_host_endpoint *ep;
+
+	urb = usb_alloc_urb(0, GFP_KERNEL);
+	if (!urb)
+		return NULL;
+
+	urb->pipe = usb_rcvctrlpipe(udev, 0);
+	ep = (usb_pipein(urb->pipe) ? udev->ep_in : udev->ep_out)
+				[usb_pipeendpoint(urb->pipe)];
+	if (!ep) {
+		usb_free_urb(urb);
+		return NULL;
+	}
+
+	urb->ep = ep;
+	urb->dev = udev;
+	urb->setup_packet = (void *)dr;
+	urb->transfer_buffer = buf;
+	urb->transfer_buffer_length = USB_DT_DEVICE_SIZE;
+	urb->complete = usb_ehset_completion;
+	urb->status = -EINPROGRESS;
+	urb->actual_length = 0;
+	urb->transfer_flags = URB_DIR_IN;
+	usb_get_urb(urb);
+	atomic_inc(&urb->use_count);
+	atomic_inc(&urb->dev->urbnum);
+	urb->setup_dma = dma_map_single(
+			hcd->self.sysdev,
+			urb->setup_packet,
+			sizeof(struct usb_ctrlrequest),
+			DMA_TO_DEVICE);
+	urb->transfer_dma = dma_map_single(
+			hcd->self.sysdev,
+			urb->transfer_buffer,
+			urb->transfer_buffer_length,
+			DMA_FROM_DEVICE);
+	urb->context = done;
+	return urb;
+}
+
+int ehset_single_step_set_feature(struct usb_hcd *hcd, int port)
+{
+	int retval = -ENOMEM;
+	struct usb_ctrlrequest *dr;
+	struct urb *urb;
+	struct usb_device *udev;
+	struct usb_device_descriptor *buf;
+	DECLARE_COMPLETION_ONSTACK(done);
+
+	/* Obtain udev of the rhub's child port */
+	udev = usb_hub_find_child(hcd->self.root_hub, port);
+	if (!udev) {
+		dev_err(hcd->self.controller, "No device attached to the RootHub\n");
+		return -ENODEV;
+	}
+	buf = kmalloc(USB_DT_DEVICE_SIZE, GFP_KERNEL);
+	if (!buf)
+		return -ENOMEM;
+
+	dr = kmalloc(sizeof(struct usb_ctrlrequest), GFP_KERNEL);
+	if (!dr) {
+		kfree(buf);
+		return -ENOMEM;
+	}
+
+	/* Fill Setup packet for GetDescriptor */
+	dr->bRequestType = USB_DIR_IN;
+	dr->bRequest = USB_REQ_GET_DESCRIPTOR;
+	dr->wValue = cpu_to_le16(USB_DT_DEVICE << 8);
+	dr->wIndex = 0;
+	dr->wLength = cpu_to_le16(USB_DT_DEVICE_SIZE);
+	urb = request_single_step_set_feature_urb(udev, dr, buf, &done);
+	if (!urb)
+		goto cleanup;
+
+	/* Submit just the SETUP stage */
+	retval = hcd->driver->submit_single_step_set_feature(hcd, urb, 1);
+	if (retval)
+		goto out1;
+	if (!wait_for_completion_timeout(&done, msecs_to_jiffies(2000))) {
+		usb_kill_urb(urb);
+		retval = -ETIMEDOUT;
+		dev_err(hcd->self.controller,
+			"%s SETUP stage timed out on ep0\n", __func__);
+		goto out1;
+	}
+	msleep(15 * 1000);
+
+	/* Complete remaining DATA and STATUS stages using the same URB */
+	urb->status = -EINPROGRESS;
+	usb_get_urb(urb);
+	atomic_inc(&urb->use_count);
+	atomic_inc(&urb->dev->urbnum);
+	retval = hcd->driver->submit_single_step_set_feature(hcd, urb, 0);
+	if (!retval && !wait_for_completion_timeout(&done,
+						msecs_to_jiffies(2000))) {
+		usb_kill_urb(urb);
+		retval = -ETIMEDOUT;
+		dev_err(hcd->self.controller,
+			"%s IN stage timed out on ep0\n", __func__);
+	}
+out1:
+	usb_free_urb(urb);
+cleanup:
+	kfree(dr);
+	kfree(buf);
+	return retval;
+}
+EXPORT_SYMBOL_GPL(ehset_single_step_set_feature);
+#endif /* CONFIG_USB_HCD_TEST_MODE */
+
+/*-------------------------------------------------------------------------*/
 
 #ifdef	CONFIG_PM
 
--- a/drivers/usb/host/ehci-hcd.c
+++ b/drivers/usb/host/ehci-hcd.c
@@ -1232,6 +1232,10 @@ static const struct hc_driver ehci_hc_dr
 	 * device support
 	 */
 	.free_dev =		ehci_remove_device,
+#ifdef CONFIG_USB_HCD_TEST_MODE
+	/* EH SINGLE_STEP_SET_FEATURE test support */
+	.submit_single_step_set_feature	= ehci_submit_single_step_set_feature,
+#endif
 };
 
 void ehci_init_driver(struct hc_driver *drv,
--- a/drivers/usb/host/ehci-hub.c
+++ b/drivers/usb/host/ehci-hub.c
@@ -725,145 +725,6 @@ ehci_hub_descriptor (
 }
 
 /*-------------------------------------------------------------------------*/
-#ifdef CONFIG_USB_HCD_TEST_MODE
-
-#define EHSET_TEST_SINGLE_STEP_SET_FEATURE 0x06
-
-static void usb_ehset_completion(struct urb *urb)
-{
-	struct completion  *done = urb->context;
-
-	complete(done);
-}
-static int submit_single_step_set_feature(
-	struct usb_hcd	*hcd,
-	struct urb	*urb,
-	int		is_setup
-);
-
-/*
- * Allocate and initialize a control URB. This request will be used by the
- * EHSET SINGLE_STEP_SET_FEATURE test in which the DATA and STATUS stages
- * of the GetDescriptor request are sent 15 seconds after the SETUP stage.
- * Return NULL if failed.
- */
-static struct urb *request_single_step_set_feature_urb(
-	struct usb_device	*udev,
-	void			*dr,
-	void			*buf,
-	struct completion	*done
-) {
-	struct urb *urb;
-	struct usb_hcd *hcd = bus_to_hcd(udev->bus);
-	struct usb_host_endpoint *ep;
-
-	urb = usb_alloc_urb(0, GFP_KERNEL);
-	if (!urb)
-		return NULL;
-
-	urb->pipe = usb_rcvctrlpipe(udev, 0);
-	ep = (usb_pipein(urb->pipe) ? udev->ep_in : udev->ep_out)
-				[usb_pipeendpoint(urb->pipe)];
-	if (!ep) {
-		usb_free_urb(urb);
-		return NULL;
-	}
-
-	urb->ep = ep;
-	urb->dev = udev;
-	urb->setup_packet = (void *)dr;
-	urb->transfer_buffer = buf;
-	urb->transfer_buffer_length = USB_DT_DEVICE_SIZE;
-	urb->complete = usb_ehset_completion;
-	urb->status = -EINPROGRESS;
-	urb->actual_length = 0;
-	urb->transfer_flags = URB_DIR_IN;
-	usb_get_urb(urb);
-	atomic_inc(&urb->use_count);
-	atomic_inc(&urb->dev->urbnum);
-	urb->setup_dma = dma_map_single(
-			hcd->self.sysdev,
-			urb->setup_packet,
-			sizeof(struct usb_ctrlrequest),
-			DMA_TO_DEVICE);
-	urb->transfer_dma = dma_map_single(
-			hcd->self.sysdev,
-			urb->transfer_buffer,
-			urb->transfer_buffer_length,
-			DMA_FROM_DEVICE);
-	urb->context = done;
-	return urb;
-}
-
-static int ehset_single_step_set_feature(struct usb_hcd *hcd, int port)
-{
-	int retval = -ENOMEM;
-	struct usb_ctrlrequest *dr;
-	struct urb *urb;
-	struct usb_device *udev;
-	struct ehci_hcd *ehci = hcd_to_ehci(hcd);
-	struct usb_device_descriptor *buf;
-	DECLARE_COMPLETION_ONSTACK(done);
-
-	/* Obtain udev of the rhub's child port */
-	udev = usb_hub_find_child(hcd->self.root_hub, port);
-	if (!udev) {
-		ehci_err(ehci, "No device attached to the RootHub\n");
-		return -ENODEV;
-	}
-	buf = kmalloc(USB_DT_DEVICE_SIZE, GFP_KERNEL);
-	if (!buf)
-		return -ENOMEM;
-
-	dr = kmalloc(sizeof(struct usb_ctrlrequest), GFP_KERNEL);
-	if (!dr) {
-		kfree(buf);
-		return -ENOMEM;
-	}
-
-	/* Fill Setup packet for GetDescriptor */
-	dr->bRequestType = USB_DIR_IN;
-	dr->bRequest = USB_REQ_GET_DESCRIPTOR;
-	dr->wValue = cpu_to_le16(USB_DT_DEVICE << 8);
-	dr->wIndex = 0;
-	dr->wLength = cpu_to_le16(USB_DT_DEVICE_SIZE);
-	urb = request_single_step_set_feature_urb(udev, dr, buf, &done);
-	if (!urb)
-		goto cleanup;
-
-	/* Submit just the SETUP stage */
-	retval = submit_single_step_set_feature(hcd, urb, 1);
-	if (retval)
-		goto out1;
-	if (!wait_for_completion_timeout(&done, msecs_to_jiffies(2000))) {
-		usb_kill_urb(urb);
-		retval = -ETIMEDOUT;
-		ehci_err(ehci, "%s SETUP stage timed out on ep0\n", __func__);
-		goto out1;
-	}
-	msleep(15 * 1000);
-
-	/* Complete remaining DATA and STATUS stages using the same URB */
-	urb->status = -EINPROGRESS;
-	usb_get_urb(urb);
-	atomic_inc(&urb->use_count);
-	atomic_inc(&urb->dev->urbnum);
-	retval = submit_single_step_set_feature(hcd, urb, 0);
-	if (!retval && !wait_for_completion_timeout(&done,
-						msecs_to_jiffies(2000))) {
-		usb_kill_urb(urb);
-		retval = -ETIMEDOUT;
-		ehci_err(ehci, "%s IN stage timed out on ep0\n", __func__);
-	}
-out1:
-	usb_free_urb(urb);
-cleanup:
-	kfree(dr);
-	kfree(buf);
-	return retval;
-}
-#endif /* CONFIG_USB_HCD_TEST_MODE */
-/*-------------------------------------------------------------------------*/
 
 int ehci_hub_control(
 	struct usb_hcd	*hcd,
--- a/drivers/usb/host/ehci-q.c
+++ b/drivers/usb/host/ehci-q.c
@@ -1165,7 +1165,7 @@ submit_async (
  * performed; TRUE - SETUP and FALSE - IN+STATUS
  * Returns 0 if success
  */
-static int submit_single_step_set_feature(
+static int ehci_submit_single_step_set_feature(
 	struct usb_hcd  *hcd,
 	struct urb      *urb,
 	int             is_setup
--- a/include/linux/usb/hcd.h
+++ b/include/linux/usb/hcd.h
@@ -409,7 +409,10 @@ struct hc_driver {
 	int	(*find_raw_port_number)(struct usb_hcd *, int);
 	/* Call for power on/off the port if necessary */
 	int	(*port_power)(struct usb_hcd *hcd, int portnum, bool enable);
-
+	/* Call for SINGLE_STEP_SET_FEATURE Test for USB2 EH certification */
+#define EHSET_TEST_SINGLE_STEP_SET_FEATURE 0x06
+	int	(*submit_single_step_set_feature)(struct usb_hcd *,
+			struct urb *, int);
 };
 
 static inline int hcd_giveback_urb_in_bh(struct usb_hcd *hcd)
@@ -474,6 +477,14 @@ int usb_hcd_setup_local_mem(struct usb_h
 
 struct platform_device;
 extern void usb_hcd_platform_shutdown(struct platform_device *dev);
+#ifdef CONFIG_USB_HCD_TEST_MODE
+extern int ehset_single_step_set_feature(struct usb_hcd *hcd, int port);
+#else
+static inline int ehset_single_step_set_feature(struct usb_hcd *hcd, int port)
+{
+	return 0;
+}
+#endif /* CONFIG_USB_HCD_TEST_MODE */
 
 #ifdef CONFIG_USB_PCI
 struct pci_dev;
