From f4128f3224df2309262ef8d1275d928717ebefd0 Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Tue, 6 Mar 2018 09:21:46 +0100
Subject: [PATCH 22/27] MIPS: ath79: drop pci.c

This patch drops pci.c fromt he ath79 folder and moves the the pcibios
callbacks to a new fixup file.

Signed-off-by: John Crispin <john@phrozen.org>
---
 arch/mips/ath79/Makefile    |   1 -
 arch/mips/ath79/pci.c       | 285 --------------------------------------------
 arch/mips/pci/Makefile      |   1 +
 arch/mips/pci/fixup-ath79.c |  21 ++++
 4 files changed, 22 insertions(+), 286 deletions(-)
 delete mode 100644 arch/mips/ath79/pci.c
 create mode 100644 arch/mips/pci/fixup-ath79.c

--- a/arch/mips/ath79/Makefile
+++ b/arch/mips/ath79/Makefile
@@ -11,7 +11,6 @@
 obj-y	:= prom.o setup.o irq.o common.o clock.o
 
 obj-$(CONFIG_EARLY_PRINTK)		+= early_printk.o
-obj-$(CONFIG_PCI)			+= pci.o
 
 #
 # Devices
--- a/arch/mips/ath79/pci.c
+++ /dev/null
@@ -1,285 +0,0 @@
-/*
- *  Atheros AR71XX/AR724X specific PCI setup code
- *
- *  Copyright (C) 2011 René Bolldorf <xsecute@googlemail.com>
- *  Copyright (C) 2008-2011 Gabor Juhos <juhosg@openwrt.org>
- *  Copyright (C) 2008 Imre Kaloz <kaloz@openwrt.org>
- *
- *  Parts of this file are based on Atheros' 2.6.15 BSP
- *
- *  This program is free software; you can redistribute it and/or modify it
- *  under the terms of the GNU General Public License version 2 as published
- *  by the Free Software Foundation.
- */
-
-#include <linux/init.h>
-#include <linux/pci.h>
-#include <linux/resource.h>
-#include <linux/platform_device.h>
-#include <asm/mach-ath79/ar71xx_regs.h>
-#include <asm/mach-ath79/ath79.h>
-#include <asm/mach-ath79/irq.h>
-#include "pci.h"
-
-static int (*ath79_pci_plat_dev_init)(struct pci_dev *dev);
-static const struct ath79_pci_irq *ath79_pci_irq_map;
-static unsigned ath79_pci_nr_irqs;
-
-static const struct ath79_pci_irq ar71xx_pci_irq_map[] = {
-	{
-		.slot	= 17,
-		.pin	= 1,
-		.irq	= ATH79_PCI_IRQ(0),
-	}, {
-		.slot	= 18,
-		.pin	= 1,
-		.irq	= ATH79_PCI_IRQ(1),
-	}, {
-		.slot	= 19,
-		.pin	= 1,
-		.irq	= ATH79_PCI_IRQ(2),
-	}
-};
-
-static const struct ath79_pci_irq ar724x_pci_irq_map[] = {
-	{
-		.slot	= 0,
-		.pin	= 1,
-		.irq	= ATH79_PCI_IRQ(0),
-	}
-};
-
-static const struct ath79_pci_irq qca955x_pci_irq_map[] = {
-	{
-		.bus	= 0,
-		.slot	= 0,
-		.pin	= 1,
-		.irq	= ATH79_PCI_IRQ(0),
-	},
-	{
-		.bus	= 1,
-		.slot	= 0,
-		.pin	= 1,
-		.irq	= ATH79_PCI_IRQ(1),
-	},
-};
-
-int pcibios_map_irq(const struct pci_dev *dev, uint8_t slot, uint8_t pin)
-{
-	int irq = -1;
-	int i;
-
-	if (ath79_pci_nr_irqs == 0 ||
-	    ath79_pci_irq_map == NULL) {
-		if (soc_is_ar71xx()) {
-			ath79_pci_irq_map = ar71xx_pci_irq_map;
-			ath79_pci_nr_irqs = ARRAY_SIZE(ar71xx_pci_irq_map);
-		} else if (soc_is_ar724x() ||
-			   soc_is_ar9342() ||
-			   soc_is_ar9344()) {
-			ath79_pci_irq_map = ar724x_pci_irq_map;
-			ath79_pci_nr_irqs = ARRAY_SIZE(ar724x_pci_irq_map);
-		} else if (soc_is_qca955x()) {
-			ath79_pci_irq_map = qca955x_pci_irq_map;
-			ath79_pci_nr_irqs = ARRAY_SIZE(qca955x_pci_irq_map);
-		} else if (soc_is_qca956x()) {
-			ath79_pci_irq_map = qca956x_pci_irq_map;
-			ath79_pci_nr_irqs = ARRAY_SIZE(qca956x_pci_irq_map);
-		} else {
-			pr_crit("pci %s: invalid irq map\n",
-				pci_name((struct pci_dev *) dev));
-			return irq;
-		}
-	}
-
-	for (i = 0; i < ath79_pci_nr_irqs; i++) {
-		const struct ath79_pci_irq *entry;
-
-		entry = &ath79_pci_irq_map[i];
-		if (entry->bus == dev->bus->number &&
-		    entry->slot == slot &&
-		    entry->pin == pin) {
-			irq = entry->irq;
-			break;
-		}
-	}
-
-	if (irq < 0)
-		pr_crit("pci %s: no irq found for pin %u\n",
-			pci_name((struct pci_dev *) dev), pin);
-	else
-		pr_info("pci %s: using irq %d for pin %u\n",
-			pci_name((struct pci_dev *) dev), irq, pin);
-
-	return irq;
-}
-
-int pcibios_plat_dev_init(struct pci_dev *dev)
-{
-	if (ath79_pci_plat_dev_init)
-		return ath79_pci_plat_dev_init(dev);
-
-	return 0;
-}
-
-void __init ath79_pci_set_irq_map(unsigned nr_irqs,
-				  const struct ath79_pci_irq *map)
-{
-	ath79_pci_nr_irqs = nr_irqs;
-	ath79_pci_irq_map = map;
-}
-
-void __init ath79_pci_set_plat_dev_init(int (*func)(struct pci_dev *dev))
-{
-	ath79_pci_plat_dev_init = func;
-}
-
-static struct platform_device *
-ath79_register_pci_ar71xx(void)
-{
-	struct platform_device *pdev;
-	struct resource res[4];
-
-	memset(res, 0, sizeof(res));
-
-	res[0].name = "cfg_base";
-	res[0].flags = IORESOURCE_MEM;
-	res[0].start = AR71XX_PCI_CFG_BASE;
-	res[0].end = AR71XX_PCI_CFG_BASE + AR71XX_PCI_CFG_SIZE - 1;
-
-	res[1].flags = IORESOURCE_IRQ;
-	res[1].start = ATH79_CPU_IRQ(2);
-	res[1].end = ATH79_CPU_IRQ(2);
-
-	res[2].name = "io_base";
-	res[2].flags = IORESOURCE_IO;
-	res[2].start = 0;
-	res[2].end = 0;
-
-	res[3].name = "mem_base";
-	res[3].flags = IORESOURCE_MEM;
-	res[3].start = AR71XX_PCI_MEM_BASE;
-	res[3].end = AR71XX_PCI_MEM_BASE + AR71XX_PCI_MEM_SIZE - 1;
-
-	pdev = platform_device_register_simple("ar71xx-pci", -1,
-					       res, ARRAY_SIZE(res));
-	return pdev;
-}
-
-static struct platform_device *
-ath79_register_pci_ar724x(int id,
-			  unsigned long cfg_base,
-			  unsigned long ctrl_base,
-			  unsigned long crp_base,
-			  unsigned long mem_base,
-			  unsigned long mem_size,
-			  unsigned long io_base,
-			  int irq)
-{
-	struct platform_device *pdev;
-	struct resource res[6];
-
-	memset(res, 0, sizeof(res));
-
-	res[0].name = "cfg_base";
-	res[0].flags = IORESOURCE_MEM;
-	res[0].start = cfg_base;
-	res[0].end = cfg_base + AR724X_PCI_CFG_SIZE - 1;
-
-	res[1].name = "ctrl_base";
-	res[1].flags = IORESOURCE_MEM;
-	res[1].start = ctrl_base;
-	res[1].end = ctrl_base + AR724X_PCI_CTRL_SIZE - 1;
-
-	res[2].flags = IORESOURCE_IRQ;
-	res[2].start = irq;
-	res[2].end = irq;
-
-	res[3].name = "mem_base";
-	res[3].flags = IORESOURCE_MEM;
-	res[3].start = mem_base;
-	res[3].end = mem_base + mem_size - 1;
-
-	res[4].name = "io_base";
-	res[4].flags = IORESOURCE_IO;
-	res[4].start = io_base;
-	res[4].end = io_base;
-
-	res[5].name = "crp_base";
-	res[5].flags = IORESOURCE_MEM;
-	res[5].start = crp_base;
-	res[5].end = crp_base + AR724X_PCI_CRP_SIZE - 1;
-
-	pdev = platform_device_register_simple("ar724x-pci", id,
-					       res, ARRAY_SIZE(res));
-	return pdev;
-}
-
-int __init ath79_register_pci(void)
-{
-	struct platform_device *pdev = NULL;
-
-	if (soc_is_ar71xx()) {
-		pdev = ath79_register_pci_ar71xx();
-	} else if (soc_is_ar724x()) {
-		pdev = ath79_register_pci_ar724x(-1,
-						 AR724X_PCI_CFG_BASE,
-						 AR724X_PCI_CTRL_BASE,
-						 AR724X_PCI_CRP_BASE,
-						 AR724X_PCI_MEM_BASE,
-						 AR724X_PCI_MEM_SIZE,
-						 0,
-						 ATH79_CPU_IRQ(2));
-	} else if (soc_is_ar9342() ||
-		   soc_is_ar9344()) {
-		u32 bootstrap;
-
-		bootstrap = ath79_reset_rr(AR934X_RESET_REG_BOOTSTRAP);
-		if ((bootstrap & AR934X_BOOTSTRAP_PCIE_RC) == 0)
-			return -ENODEV;
-
-		pdev = ath79_register_pci_ar724x(-1,
-						 AR724X_PCI_CFG_BASE,
-						 AR724X_PCI_CTRL_BASE,
-						 AR724X_PCI_CRP_BASE,
-						 AR724X_PCI_MEM_BASE,
-						 AR724X_PCI_MEM_SIZE,
-						 0,
-						 ATH79_IP2_IRQ(0));
-	} else if (soc_is_qca9558()) {
-		pdev = ath79_register_pci_ar724x(0,
-						 QCA955X_PCI_CFG_BASE0,
-						 QCA955X_PCI_CTRL_BASE0,
-						 QCA955X_PCI_CRP_BASE0,
-						 QCA955X_PCI_MEM_BASE0,
-						 QCA955X_PCI_MEM_SIZE,
-						 0,
-						 ATH79_IP2_IRQ(0));
-
-		pdev = ath79_register_pci_ar724x(1,
-						 QCA955X_PCI_CFG_BASE1,
-						 QCA955X_PCI_CTRL_BASE1,
-						 QCA955X_PCI_CRP_BASE1,
-						 QCA955X_PCI_MEM_BASE1,
-						 QCA955X_PCI_MEM_SIZE,
-						 1,
-						 ATH79_IP3_IRQ(2));
-	} else if (soc_is_qca956x()) {
-		pdev = ath79_register_pci_ar724x(0,
-						 QCA956X_PCI_CFG_BASE1,
-						 QCA956X_PCI_CTRL_BASE1,
-						 QCA956X_PCI_CRP_BASE1,
-						 QCA956X_PCI_MEM_BASE1,
-						 QCA956X_PCI_MEM_SIZE,
-						 1,
-						 ATH79_IP3_IRQ(2));
-	} else {
-		/* No PCI support */
-		return -ENODEV;
-	}
-
-	if (!pdev)
-		pr_err("unable to register PCI controller device\n");
-
-	return pdev ? 0 : -ENODEV;
-}
--- a/arch/mips/pci/Makefile
+++ b/arch/mips/pci/Makefile
@@ -29,6 +29,7 @@ obj-$(CONFIG_MIPS_PCI_VIRTIO)	+= pci-vir
 #
 # These are still pretty much in the old state, watch, go blind.
 #
+obj-$(CONFIG_ATH79)		+= fixup-ath79.o
 obj-$(CONFIG_LASAT)		+= pci-lasat.o
 obj-$(CONFIG_MIPS_COBALT)	+= fixup-cobalt.o
 obj-$(CONFIG_LEMOTE_FULOONG2E)	+= fixup-fuloong2e.o ops-loongson2.o
--- /dev/null
+++ b/arch/mips/pci/fixup-ath79.c
@@ -0,0 +1,21 @@
+/*
+ *  Copyright (C) 2018 John Crispin <john@phrozen.org>
+ *
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ */
+
+#include <linux/pci.h>
+//#include <linux/of_irq.h>
+#include <linux/of_pci.h>
+
+int pcibios_plat_dev_init(struct pci_dev *dev)
+{
+	return PCIBIOS_SUCCESSFUL;
+}
+
+int pcibios_map_irq(const struct pci_dev *dev, u8 slot, u8 pin)
+{
+	return of_irq_parse_and_map_pci(dev, slot, pin);
+}
