#!/bin/sh

. /lib/functions/system.sh
. /lib/functions/uci-defaults.sh
. /lib/functions/k2t.sh

ath79_setup_interfaces()
{
	local board="$1"

	case "$board" in
	"etactica,eg200")
		ucidef_set_interface_lan "eth0" "dhcp"
		;;
	"avm,fritz300e"|\
	"tplink,re450-v2"|\
	"tplink,tl-mr10u"|\
	"tplink,tl-wr703n"|\
	"ubnt,unifiac-lite"|\
	"ubnt,unifiac-mesh"|\
	"ubnt,unifi")
		ucidef_set_interface_lan "eth0"
		;;

	"embeddedwireless,dorin")
		ucidef_add_switch "switch0" \
			"0@eth0" "1:wan" "2:lan:3" "3:lan:2"
		;;

	"glinet,ar150")
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		;;

	"glinet,ar300m")
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		;;

	"netgear,wnr612-v2"|\
	"on,n150r")
		ucidef_set_interfaces_lan_wan "eth1.1" "eth0"
		ucidef_add_switch "switch0" \
		"0@eth1" "1:lan" "2:lan" "3:lan:3" "4:lan:4"
		;;

	"tplink,tl-archer-c7-v2")
		ucidef_set_interfaces_lan_wan "eth1.1" "eth0.2"
		ucidef_add_switch "switch0" \
			"0@eth1" "2:lan" "3:lan" "4:lan" "5:lan" "6@eth0" "1:wan"
		;;

	"tplink,tl-mr3020-v1")
		ucidef_set_interface_lan "eth0.1"
		ucidef_add_switch "switch0" "0@eth0" "1:lan"
		;;
	"tplink,tl-mr3220-v1"|\
	"tplink,tl-mr3420-v1"|\
	"tplink,tl-wr841-v7")
		ucidef_set_interface_wan "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1"
		;;
	"tplink,tl-wdr3600"|\
	"tplink,tl-wdr4300")
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:1" "3:lan:2" "4:lan:3" "5:lan:4" "1:wan"
		;;

	"tplink,tl-wr740n-v2")
		ucidef_set_interfaces_lan_wan "eth1.1" "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan" "2:lan" "3:lan" "4:lan"
		;;

	"tplink,tl-wr741nd-v4"|\
	"tplink,tl-wr740nd-v4")
		ucidef_set_interfaces_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1"
		;;

	"tplink,tl-wr1043nd-v1")
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "5@eth0"
		;;
	"tplink,tl-wr1043nd-v4")
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "5:wan"
		;;
	"tplink,tl-wr1043nd-v2"|\
	"tplink,tl-wr1043nd-v3")
		ucidef_set_interfaces_lan_wan "eth1.1" "eth0.2"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "5:wan" "6@eth0"
		;;
	"tplink,tl-wr2543-v1")
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "9@eth0"
		;;
	"netgear,wndr3800")
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		ucidef_add_switch "switch0" \
			"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "5u@eth0"

		ucidef_add_switch_attr "switch0" "blinkrate" 2
		ucidef_add_switch_port_attr "switch0" 1 led 6
		ucidef_add_switch_port_attr "switch0" 2 led 9
		ucidef_add_switch_port_attr "switch0" 5 led 2
		;;
	"buffalo,wzr-hp-g450h")
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:lan" "4:lan" "5:lan" "1:wan"
		;;
	"phicomm,k2t")
		ucidef_add_switch "switch0" \
			"0@eth0" "3:lan:1" "5:lan:2" "4:wan"
		;;
	"ubnt,unifiac-pro")
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:wan"
		;;
	*)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		;;
	esac
}

ath79_setup_macs()
{
	local board="$1"

	case "$board" in
	avm,fritz300e)
		lan_mac=$(fritz_tffs -n maca -i $(find_mtd_part "tffs (1)"))
		;;
	phicomm,k2t)
		lan_mac=$(k2t_get_mac "lan_mac")
		wan_mac=$(k2t_get_mac "wan_mac")
		;;
	"tplink,tl-wr1043nd-v4")
		base_mac=$(mtd_get_mac_binary product-info 8)
		wan_mac=$(macaddr_add "$base_mac" 1)
		;;
	esac

	[ -n "$lan_mac" ] && ucidef_set_interface_macaddr "lan" $lan_mac
	[ -n "$wan_mac" ] && ucidef_set_interface_macaddr "wan" $wan_mac
}

board_config_update
board=$(board_name)
ath79_setup_interfaces $board
ath79_setup_macs $board
board_config_flush

exit 0
