From 0669ee7a69a004ce34fed41e50aa575f8e04427b Mon Sep 17 00:00:00 2001
From: Simon Kelley <simon@thekelleys.org.uk>
Date: Fri, 4 May 2018 16:46:24 +0100
Subject: [PATCH 02/17] Fix DHCP broken-ness when --no-ping AND
 --dhcp-sequential-ip are set.

Signed-off-by: Kevin Darbyshire-Bryant <ldir@darbyshire-bryant.me.uk>
---
 CHANGELOG  | 3 ++-
 src/dhcp.c | 2 +-
 2 files changed, 3 insertions(+), 2 deletions(-)

--- a/CHANGELOG
+++ b/CHANGELOG
@@ -14,7 +14,8 @@ version 2.80
         when the upstream namesevers do not support DNSSEC, and in this
         case no DNSSEC validation at all is occuring.
 
-
+        Fix DHCP broken-ness when --no-ping AND --dhcp-sequential-ip
+	are set. Thanks to Daniel Miess for help with this.
 
 
 version 2.79
--- a/src/dhcp.c
+++ b/src/dhcp.c
@@ -678,7 +678,7 @@ struct ping_result *do_icmp_ping(time_t
   if ((count >= max) || option_bool(OPT_NO_PING) || loopback)
     {
       /* overloaded, or configured not to check, loopback interface, return "not in use" */
-      dummy.hash = 0;
+      dummy.hash = hash;
       return &dummy;
     }
   else if (icmp_ping(addr))
