#!/bin/sh

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)
boardname="${board##*,}"

case "$board" in
"avm,fritz300e")
	ucidef_set_led_netdev "lan" "LAN" "$boardname:green:lan" "eth0"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "$boardname:green:rssi0" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "$boardname:green:rssi1" "wlan0" "20" "100"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "$boardname:green:rssi2" "wlan0" "40" "100"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "$boardname:green:rssi3" "wlan0" "60" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "$boardname:green:rssi4" "wlan0" "80" "100"
	;;
"etactica,eg200")
	ucidef_set_led_netdev "lan" "LAN" "$boardname:red:eth0" "eth0"
	ucidef_set_led_oneshot "modbus" "Modbus" "$boardname:red:modbus" "100" "33"
	ucidef_set_led_default "etactica" "etactica" "$boardname:red:etactica" "ignore"
	;;
"netgear,wnr612-v2"|\
"on,n150r")
	ucidef_set_led_netdev "wan" "WAN" "netgear:green:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "netgear:green:lan1" "switch0" "0x02" "0x0f"
	ucidef_set_led_switch "lan2" "LAN2" "netgear:green:lan2" "switch0" "0x04" "0x0f"
	;;
"tplink,re450-v2")
	ucidef_set_led_netdev "lan_data" "LAN Data" "tp-link:green:lan_data" "eth0" "tx rx"
	ucidef_set_led_netdev "lan_link" "LAN Link" "tp-link:green:lan_link" "eth0" "link"
	;;
"tplink,tl-mr3020-v1")
	ucidef_set_led_switch "lan" "LAN" "tp-link:green:lan" "switch0" "0x02"
	;;
"tplink,tl-wr1043nd-v4")
	ucidef_set_led_switch "wan" "WAN" "tp-link:green:wan" "switch0" "0x20"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x04"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	;;
"tplink,tl-wr740n-v2")
	ucidef_set_led_netdev "wan" "WAN" "$boardname:green:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "$boardname:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "$boardname:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "$boardname:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "$boardname:green:lan4" "switch0" "0x10"
	;;
"tplink,tl-wr741nd-v4"|\
"tplink,tl-wr740nd-v4")
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	;;
esac

board_config_flush

exit 0
