From 54204ef3edbb1aa2390cabba61fe185a12cc39f0 Mon Sep 17 00:00:00 2001
From: Felix Fietkau <nbd@nbd.name>
Date: Tue, 6 Mar 2018 08:35:44 +0100
Subject: [PATCH 11/27] MIPS: ath79: fix register address in
 ath79_ddr_wb_flush()

ath79_ddr_wb_flush_base has the type void __iomem *, so register offsets
need to be a multiple of 4.

Cc: Alban Bedel <albeu@free.fr>
Fixes: 24b0e3e84fbf ("MIPS: ath79: Improve the DDR controller interface")
Signed-off-by: Felix Fietkau <nbd@nbd.name>
---
 arch/mips/ath79/common.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/mips/ath79/common.c
+++ b/arch/mips/ath79/common.c
@@ -58,7 +58,7 @@ EXPORT_SYMBOL_GPL(ath79_ddr_ctrl_init);
 
 void ath79_ddr_wb_flush(u32 reg)
 {
-	void __iomem *flush_reg = ath79_ddr_wb_flush_base + reg;
+	void __iomem *flush_reg = ath79_ddr_wb_flush_base + (reg * 4);
 
 	/* Flush the DDR write buffer. */
 	__raw_writel(0x1, flush_reg);
