From 883dc66755313e133a787eba4dfde313fe33525b Mon Sep 17 00:00:00 2001
From: Russell King <rmk+kernel@armlinux.org.uk>
Date: Fri, 14 Apr 2017 16:41:55 +0100
Subject: sfp: use netdev sfp_bus for start/stop

Signed-off-by: Russell King <rmk+kernel@armlinux.org.uk>
---
 drivers/net/phy/phylink.c | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

--- a/drivers/net/phy/phylink.c
+++ b/drivers/net/phy/phylink.c
@@ -755,8 +755,8 @@ void phylink_start(struct phylink *pl)
 	clear_bit(PHYLINK_DISABLE_STOPPED, &pl->phylink_disable_state);
 	phylink_run_resolve(pl);
 
-	if (pl->sfp_bus)
-		sfp_upstream_start(pl->sfp_bus);
+	if (pl->netdev->sfp_bus)
+		sfp_upstream_start(pl->netdev->sfp_bus);
 	if (pl->phydev)
 		phy_start(pl->phydev);
 }
@@ -768,8 +768,8 @@ void phylink_stop(struct phylink *pl)
 
 	if (pl->phydev)
 		phy_stop(pl->phydev);
-	if (pl->sfp_bus)
-		sfp_upstream_stop(pl->sfp_bus);
+	if (pl->netdev->sfp_bus)
+		sfp_upstream_stop(pl->netdev->sfp_bus);
 
 	set_bit(PHYLINK_DISABLE_STOPPED, &pl->phylink_disable_state);
 	queue_work(system_power_efficient_wq, &pl->resolve);
