diff -urN linux-2.6.17/drivers/net/Kconfig linux-2.6.17.new/drivers/net/Kconfig
--- linux-2.6.17/drivers/net/Kconfig	2006-06-18 03:49:35.000000000 +0200
+++ linux-2.6.17.new/drivers/net/Kconfig	2006-09-25 13:14:27.000000000 +0200
@@ -1358,6 +1358,19 @@
 	  <file:Documentation/networking/net-modules.txt>.  The module will be
 	  called apricot.
 
+config R6040
+	tristate "RDC Fast-Ethernet support (EXPERIMENTAL)"
+	depends on NET_PCI && EXPERIMENTAL
+	select MII
+	help
+	  If you have a network (Ethernet) controller of this type, say Y and
+	  read the Ethernet-HOWTO, available from
+          <http://www.tldp.org/docs.html#howto>.
+
+          To compile this driver as a module, choose M here and read
+          <file:Documentation/networking/net-modules.txt>.  The module will be
+          called r6040.
+
 config B44
 	tristate "Broadcom 4400 ethernet support (EXPERIMENTAL)"
 	depends on NET_PCI && PCI && EXPERIMENTAL
diff -urN linux-2.6.17/drivers/net/Makefile linux-2.6.17.new/drivers/net/Makefile
--- linux-2.6.17/drivers/net/Makefile	2006-06-18 03:49:35.000000000 +0200
+++ linux-2.6.17.new/drivers/net/Makefile	2006-09-25 13:14:45.000000000 +0200
@@ -106,6 +106,7 @@
 obj-$(CONFIG_NE3210) += ne3210.o 8390.o
 obj-$(CONFIG_NET_SB1250_MAC) += sb1250-mac.o
 obj-$(CONFIG_B44) += b44.o
+obj-$(CONFIG_R6040) += r6040.o
 obj-$(CONFIG_FORCEDETH) += forcedeth.o
 obj-$(CONFIG_NE_H8300) += ne-h8300.o 8390.o
 
