[ "$ACTION" == "add" ] || exit 0

PHYNBR=${DEVPATH##*/phy}

[ -n $PHYNBR ] || exit 0

. /lib/functions.sh
. /lib/functions/system.sh

board=$(board_name)

case "$board" in
	linksys,ea7300-v1|\
	linksys,ea7500-v2)
		hw_mac_addr=$(mtd_get_mac_ascii devinfo hw_mac_addr)
		[ "$PHYNBR" = "0" ] && macaddr_add $hw_mac_addr 1 > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && macaddr_add $hw_mac_addr 2 > /sys${DEVPATH}/macaddress
		;;
esac
