From eb5a26bcaddb35fd42a978ad37831e58b1118853 Mon Sep 17 00:00:00 2001
From: Pawel Dembicki <paweldembicki@gmail.com>
Date: Tue, 17 Apr 2018 19:53:59 +0200
Subject: [PATCH] net: qmi_wwan: add Wistron Neweb D19Q1

This modem is embedded on dlink dwr-960 router.
The oem configuration states:

T: Bus=01 Lev=01 Prnt=01 Port=00 Cnt=01 Dev#= 2 Spd=480 MxCh= 0
D: Ver= 2.10 Cls=00(>ifc ) Sub=00 Prot=00 MxPS=64 #Cfgs= 1
P: Vendor=1435 ProdID=d191 Rev=ff.ff
S: Manufacturer=Android
S: Product=Android
S: SerialNumber=0123456789ABCDEF
C:* #Ifs= 6 Cfg#= 1 Atr=80 MxPwr=500mA
I:* If#= 0 Alt= 0 #EPs= 2 Cls=ff(vend.) Sub=ff Prot=ff Driver=(none)
E: Ad=81(I) Atr=02(Bulk) MxPS= 512 Ivl=0ms
E: Ad=01(O) Atr=02(Bulk) MxPS= 512 Ivl=0ms
I:* If#= 1 Alt= 0 #EPs= 2 Cls=ff(vend.) Sub=42 Prot=01 Driver=(none)
E: Ad=02(O) Atr=02(Bulk) MxPS= 512 Ivl=0ms
E: Ad=82(I) Atr=02(Bulk) MxPS= 512 Ivl=0ms
I:* If#= 2 Alt= 0 #EPs= 3 Cls=ff(vend.) Sub=00 Prot=00 Driver=(none)
E: Ad=84(I) Atr=03(Int.) MxPS= 10 Ivl=32ms
E: Ad=83(I) Atr=02(Bulk) MxPS= 512 Ivl=0ms
E: Ad=03(O) Atr=02(Bulk) MxPS= 512 Ivl=0ms
I:* If#= 3 Alt= 0 #EPs= 3 Cls=ff(vend.) Sub=00 Prot=00 Driver=(none)
E: Ad=86(I) Atr=03(Int.) MxPS= 10 Ivl=32ms
E: Ad=85(I) Atr=02(Bulk) MxPS= 512 Ivl=0ms
E: Ad=04(O) Atr=02(Bulk) MxPS= 512 Ivl=0ms
I:* If#= 4 Alt= 0 #EPs= 3 Cls=ff(vend.) Sub=ff Prot=ff Driver=qmi_wwan
E: Ad=88(I) Atr=03(Int.) MxPS= 8 Ivl=32ms
E: Ad=87(I) Atr=02(Bulk) MxPS= 512 Ivl=0ms
E: Ad=05(O) Atr=02(Bulk) MxPS= 512 Ivl=0ms
I:* If#= 5 Alt= 0 #EPs= 2 Cls=08(stor.) Sub=06 Prot=50 Driver=(none)
E: Ad=89(I) Atr=02(Bulk) MxPS= 512 Ivl=0ms
E: Ad=06(O) Atr=02(Bulk) MxPS= 512 Ivl=125us

Tested on openwrt distribution

Signed-off-by: Pawel Dembicki <paweldembicki@gmail.com>
---
 drivers/net/usb/qmi_wwan.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/net/usb/qmi_wwan.c
+++ b/drivers/net/usb/qmi_wwan.c
@@ -1138,6 +1138,7 @@ static const struct usb_device_id produc
 	{QMI_FIXED_INTF(0x1435, 0xd181, 3)},	/* Wistron NeWeb D18Q1 */
 	{QMI_FIXED_INTF(0x1435, 0xd181, 4)},	/* Wistron NeWeb D18Q1 */
 	{QMI_FIXED_INTF(0x1435, 0xd181, 5)},	/* Wistron NeWeb D18Q1 */
+	{QMI_FIXED_INTF(0x1435, 0xd191, 4)},	/* Wistron NeWeb D19Q1 */
 	{QMI_QUIRK_SET_DTR(0x1508, 0x1001, 4)},	/* Fibocom NL668 series */
 	{QMI_FIXED_INTF(0x1690, 0x7588, 4)},    /* ASKEY WWHC050 */
 	{QMI_FIXED_INTF(0x16d8, 0x6003, 0)},	/* CMOTech 6003 */
